(footprint "VQFN-64-1EP_9x9mm_P0.5mm_EP4x4mm" (version 20210424) (generator pcbnew) (layer "F.Cu")
  (tedit 60AFB0BB)
  (descr "VQFN, 64 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf#page=718), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "VQFN NoLead")
  (property "Sheetfile" "ESC12S30.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "U3" (at 0 -5.8) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cfed130b-f41a-4aa5-8750-5ddbd91385b1)
  )
  (fp_text value "ST_STSPIN32G4" (at 0 5.8) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b6e132bf-ec2c-4086-ac95-a1ebe636370f)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5b47a6f5-00f2-4893-b05d-d9ab1a0e1a0d)
  )
  (fp_line (start 4.61 4.61) (end 4.61 4.135) (layer "F.SilkS") (width 0.12) (tstamp 0f8552d7-9294-4d9e-b7b1-098847e36c7c))
  (fp_line (start 4.135 -4.61) (end 4.61 -4.61) (layer "F.SilkS") (width 0.12) (tstamp 1ca813ff-e66d-4658-a644-857ba11528f0))
  (fp_line (start -4.135 4.61) (end -4.61 4.61) (layer "F.SilkS") (width 0.12) (tstamp 66d9aa64-1178-4ebd-8690-27134cbddc16))
  (fp_line (start -4.61 4.61) (end -4.61 4.135) (layer "F.SilkS") (width 0.12) (tstamp 9bb8cb50-a694-4c54-9f1a-89647916b782))
  (fp_line (start 4.135 4.61) (end 4.61 4.61) (layer "F.SilkS") (width 0.12) (tstamp bf7085ec-bf76-4206-a0da-ddfbd21e8bf7))
  (fp_line (start 4.61 -4.61) (end 4.61 -4.135) (layer "F.SilkS") (width 0.12) (tstamp c74c1d80-92a3-4105-bd62-f2989eb43aa8))
  (fp_line (start -4.135 -4.61) (end -4.61 -4.61) (layer "F.SilkS") (width 0.12) (tstamp f93fe28d-0ab2-4615-8a82-dd4647e02b25))
  (fp_line (start 5.1 -5.1) (end -5.1 -5.1) (layer "F.CrtYd") (width 0.05) (tstamp 258e8f16-966b-4553-be79-edbe3d993e52))
  (fp_line (start 5.1 5.1) (end 5.1 -5.1) (layer "F.CrtYd") (width 0.05) (tstamp c7a8e713-effe-4af3-bdfd-30bdd5565af6))
  (fp_line (start -5.1 -5.1) (end -5.1 5.1) (layer "F.CrtYd") (width 0.05) (tstamp f5b559c1-638c-48ae-bfa2-1daa3a72c138))
  (fp_line (start -5.1 5.1) (end 5.1 5.1) (layer "F.CrtYd") (width 0.05) (tstamp f7fbcdf4-fd74-4ca2-a941-26ca857fa431))
  (fp_line (start -3.5 -4.5) (end 4.5 -4.5) (layer "F.Fab") (width 0.1) (tstamp 347ff25c-f875-4b90-8233-32746dbf85f6))
  (fp_line (start 4.5 4.5) (end -4.5 4.5) (layer "F.Fab") (width 0.1) (tstamp 4d446ef5-b835-4dc1-a9e5-60c1835af703))
  (fp_line (start -4.5 4.5) (end -4.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp aacc9a3e-c515-4fa8-b45e-4e1563ca74f4))
  (fp_line (start 4.5 -4.5) (end 4.5 4.5) (layer "F.Fab") (width 0.1) (tstamp caf02145-0f38-45ee-983b-b7cf86c5c9bc))
  (fp_line (start -4.5 -3.5) (end -3.5 -4.5) (layer "F.Fab") (width 0.1) (tstamp e9c95f05-8e0d-4799-9125-3ef34275c85e))
  (pad "" smd roundrect (at 1.2 -1.2) (size 1.65 1.65) (layers "F.Paste") (roundrect_rratio 0.172) (tstamp 559f299d-84b0-4cfb-b661-8e745680a59e))
  (pad "" smd roundrect (at -1.2 1.2) (size 1.65 1.65) (layers "F.Paste") (roundrect_rratio 0.172) (tstamp caeb12ab-9485-4d2f-96ae-3b59dee396ba))
  (pad "" smd roundrect (at 1.2 1.2) (size 1.65 1.65) (layers "F.Paste") (roundrect_rratio 0.172) (tstamp cb6e3e32-1eed-4834-8bd6-a56d8ea5264b))
  (pad "" smd roundrect (at -1.2 -1.2) (size 1.65 1.65) (layers "F.Paste") (roundrect_rratio 0.172) (tstamp fa68e040-9dae-4c99-b68d-758ef9f185ee))
  (pad "1" smd roundrect (at -4.4375 -3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3214fa64-a56b-4a6b-a909-6a060ecfc69c))
  (pad "2" smd roundrect (at -4.4375 -3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dafbccd8-3dc7-4d5f-aa14-c408c28d5e4e))
  (pad "3" smd roundrect (at -4.4375 -2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 23b2220e-733e-4bb1-9706-a2b3474ad3cc))
  (pad "4" smd roundrect (at -4.4375 -2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e3445baf-bfe9-4b22-8641-a89ee47f8429))
  (pad "5" smd roundrect (at -4.4375 -1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c490b2c7-fb2a-448e-9bf2-414c9319bf09))
  (pad "6" smd roundrect (at -4.4375 -1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 42810809-4e16-476f-ade9-08852fe0033b))
  (pad "7" smd roundrect (at -4.4375 -0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1cece31a-45dc-43bf-8975-5c9c1d35f545))
  (pad "8" smd roundrect (at -4.4375 -0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 675370ff-cdbd-4c88-8874-148c15bd1e16))
  (pad "9" smd roundrect (at -4.4375 0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 38a07387-3cf4-4d4a-b3d6-8b99400c9ada))
  (pad "10" smd roundrect (at -4.4375 0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ede95cba-ff39-4162-a6f2-3be55c341c16))
  (pad "11" smd roundrect (at -4.4375 1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8cab0815-7ed8-41b0-946b-cfcc0f4028f3))
  (pad "12" smd roundrect (at -4.4375 1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 70463c9e-a4f5-40e3-8a95-57be678909bd))
  (pad "13" smd roundrect (at -4.4375 2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ae45dca1-1055-4ff4-8d79-56720940ba73))
  (pad "14" smd roundrect (at -4.4375 2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bcc2d6a2-d3c8-4ada-830d-fc1041f2baa9))
  (pad "15" smd roundrect (at -4.4375 3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 584d0817-c5c1-4ebb-a123-f6bcb5414925))
  (pad "16" smd roundrect (at -4.4375 3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d7b79b99-73d6-4bce-9a7f-c3b8905bc119))
  (pad "17" smd roundrect (at -3.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 947b2556-c645-4bca-b5de-270d23dd0744))
  (pad "18" smd roundrect (at -3.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7863ad09-7074-4cd6-b6d8-356bb857e513))
  (pad "19" smd roundrect (at -2.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp df6f8596-65a1-48f3-8923-3fe2fb324f83))
  (pad "20" smd roundrect (at -2.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d300ad82-1889-4798-be8a-a392feb7249e))
  (pad "21" smd roundrect (at -1.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 562384ae-03eb-41c2-8b51-11d493027f39))
  (pad "22" smd roundrect (at -1.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1ef9f59b-3922-4f9e-8fe2-24ccd579829b))
  (pad "23" smd roundrect (at -0.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e6c99dc5-a9dc-41a4-95ef-178798512ea9))
  (pad "24" smd roundrect (at -0.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e369b7e7-91ee-4d62-944d-a67dcf97557f))
  (pad "25" smd roundrect (at 0.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5baef7d4-f1b5-49c9-a458-f904d5ac1c6e))
  (pad "26" smd roundrect (at 0.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1b553617-a559-4f3c-a460-8f10561623d7))
  (pad "27" smd roundrect (at 1.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f6726ca0-dce6-4f99-935c-58144012942c))
  (pad "28" smd roundrect (at 1.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c10432de-412f-46e8-a761-0ed8c9ec4bd7))
  (pad "29" smd roundrect (at 2.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 36832294-f9e0-461a-be4e-75043acd8fc9))
  (pad "30" smd roundrect (at 2.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f471a625-6684-46be-845b-2219f41a0da4))
  (pad "31" smd roundrect (at 3.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cebd6d2b-7ab1-4c16-9bbd-eebe26395e3b))
  (pad "32" smd roundrect (at 3.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6739f6e2-0bd6-4fff-8227-3e981e6b8659))
  (pad "33" smd roundrect (at 4.4375 3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 664cd8be-6158-40a0-be6d-9976c4d2948f))
  (pad "34" smd roundrect (at 4.4375 3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d17cb239-5cfa-486e-8c70-b32e9877b7ac))
  (pad "35" smd roundrect (at 4.4375 2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a2a9d66f-a0bc-4550-9bb6-318cf53b1412))
  (pad "36" smd roundrect (at 4.4375 2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b77519e6-61f7-4823-8bfb-2600b5d189eb))
  (pad "37" smd roundrect (at 4.4375 1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 50525069-a18b-4203-90c8-ca49b26bdbee))
  (pad "38" smd roundrect (at 4.4375 1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d600664f-a008-4b24-9fdd-6e8400cd9f24))
  (pad "39" smd roundrect (at 4.4375 0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 63da7d3a-490a-4c2a-ac15-4fed8d853cf8))
  (pad "40" smd roundrect (at 4.4375 0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c11db806-a01d-4807-afb2-f2cd7dd43d5c))
  (pad "41" smd roundrect (at 4.4375 -0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 93a523b9-6058-479d-a198-4c67572fa8c3))
  (pad "42" smd roundrect (at 4.4375 -0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 91efa007-b280-496c-9c13-55a073d7f01f))
  (pad "43" smd roundrect (at 4.4375 -1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a9932eed-83a9-4092-b5c1-4ea837b275df))
  (pad "44" smd roundrect (at 4.4375 -1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2a471983-b123-4d77-ba6c-7f4d436461ba))
  (pad "45" smd roundrect (at 4.4375 -2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 00796c4b-e14f-4e03-a7fc-bc1fad785905))
  (pad "46" smd roundrect (at 4.4375 -2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 970b5b93-d0a5-47fc-9e1f-9bb1be674781))
  (pad "47" smd roundrect (at 4.4375 -3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e17aa938-9519-487e-84b3-3edcd6b4fe3d))
  (pad "48" smd roundrect (at 4.4375 -3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f7a5b0ba-e41e-4045-af2b-0c65b66ab558))
  (pad "49" smd roundrect (at 3.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 7267d4ed-ffb0-40f4-9430-6cd4bb5fada5))
  (pad "50" smd roundrect (at 3.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4fd6e2f0-9d27-4610-b2e3-dbdebb374b29))
  (pad "51" smd roundrect (at 2.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5013320f-02eb-46f7-aba4-59d5ee50b2f4))
  (pad "52" smd roundrect (at 2.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 63a3dcb4-695a-4a72-8c06-5ab576adb1c7))
  (pad "53" smd roundrect (at 1.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0dd5e94a-72c7-4860-ae71-4b29e8fdcf7e))
  (pad "54" smd roundrect (at 1.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9081d8e2-4d73-4361-8cfc-17cdbc27352e))
  (pad "55" smd roundrect (at 0.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8228f177-653b-4d74-a284-5a899d93fb3e))
  (pad "56" smd roundrect (at 0.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 460385ac-48c8-4d86-a0ac-34b0fd04fc49))
  (pad "57" smd roundrect (at -0.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 90ab3ac5-ada9-4003-bea0-9c64abbd0433))
  (pad "58" smd roundrect (at -0.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 18239c1d-d041-460e-a3f1-6d3da368ca42))
  (pad "59" smd roundrect (at -1.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp eab33c0e-ab2d-4f31-96bd-c96f78e973ba))
  (pad "60" smd roundrect (at -1.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9febe69c-b6c0-434d-b121-c4f79e83538b))
  (pad "61" smd roundrect (at -2.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 472b7938-877b-46b1-9524-55dbed67e069))
  (pad "62" smd roundrect (at -2.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 95e98da0-8142-462e-a18c-8c233d2c22b7))
  (pad "63" smd roundrect (at -3.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f8c61b2e-bbc9-4125-ad55-df979820c13c))
  (pad "64" smd roundrect (at -3.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 53cdd632-56a8-4965-86e5-d05e79d1c8aa))
  (pad "65" smd rect (at 0 0) (size 4 4) (layers "F.Cu" "F.Mask") (tstamp af5bf701-9084-4d04-b9f3-cad090ab91b7))
  (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm.wrl" hide
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
