(footprint "SMD Nut M2 x 3.5 SMTSO2035" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C2916322")
  (property "MFG" "Sinhoo")
  (property "MPN" "SMTSO2035CTJ")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "H9" (at 0 -7.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9c8abda2-44f8-4e9e-93d8-cf8ca73c398a)
  )
  (fp_text value "MOUNT_HOLE" (at 0 -6 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fb57a98b-baf5-4d4a-bac1-b8e77db2d3e4)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.5 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 53125a34-16d6-46ee-9d02-651522baa49c)
  )
  (fp_arc (start -2.533845 0.788749) (mid -2.65374 -0.012456) (end -2.526329 -0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp ebdd6db1-94d1-4c2d-b286-fed809707954))
  (fp_arc (start -1.95 -1.8) (mid -1.316084 -2.304435) (end -0.559519 -2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 06413059-2a42-4852-a30a-b685988b1999))
  (fp_arc (start -0.583845 2.588749) (mid -1.337657 2.291979) (end -1.96681 1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 652d0416-9fd5-41cf-9384-df2de2bfd4fe))
  (fp_arc (start 0.583845 -2.588749) (mid 1.337657 -2.291979) (end 1.96681 -1.781615)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp d4b2f87f-b90e-436d-8588-26bf4073b6e6))
  (fp_arc (start 1.95 1.8) (mid 1.316084 2.304435) (end 0.559519 2.594115)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp f1691ee9-2a97-4764-87be-2108a3b8240f))
  (fp_arc (start 2.533845 -0.788749) (mid 2.65374 0.012456) (end 2.526329 0.8125)
    (stroke (width 0.9) (type default)) (layer "F.Paste") (tstamp 76e4f9b0-550f-4f9e-bc4b-80fcd6fd067a))
  (pad "1" thru_hole circle (at 0 0) (size 4.03 4.03) (drill 3.73) (layers "*.Cu" "B.Mask")
    (zone_connect 2) (tstamp cd7dc539-8eee-4b54-85e4-86361e3a82a4))
  (pad "1" smd circle (at 0 0) (size 6.2 6.2) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp 220045da-4410-4c07-bad8-48fe4bdea1b4))
  (model ":KICAD7_3DMODEL_DIR:Hardware.3dshapes/Nut [SMTSO] [M2 x 3.5].step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
