(footprint "OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "XDFN4 footprint (as found on the https://www.onsemi.com/pub/Collateral/NCP115-D.PDF)")
  (tags "OnSemi XDFN4")
  (property "LCSC" "C603489")
  (property "MFG" "OnSemi")
  (property "MPN" "NCP114AMX220TCG")
  (property "Sheetfile" "Samsung_S5KGN2_Module.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "300mA Low-Dropout Linear Regulators, 1.2V output voltage, LDO with low noise and enable pin, XDFN-4")
  (property "ki_keywords" "Single Output LDO")
  (attr smd)
  (fp_text reference "U5" (at 0 1.45 180) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp c9cffd6d-df50-4653-87d4-e9d1b93d0532)
  )
  (fp_text value "NCP114AMX220TCG" (at 0 -0.65 180) (layer "F.Fab")
      (effects (font (size 0.1 0.1) (thickness 0.025)))
    (tstamp ff72a256-0e13-4851-b0f5-66ba8d9cee22)
  )
  (fp_text user "${REFERENCE}" (at 0.7 0 90) (layer "F.Fab")
      (effects (font (size 0.1 0.1) (thickness 0.025)))
    (tstamp 4970e2f1-477a-45a7-8a19-b8f1083a54bb)
  )
  (fp_arc (start -0.775 -0.6) (mid -0.753033 -0.653033) (end -0.7 -0.675)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp de122df0-9d2a-451a-bd4c-2906356bfc8f))
  (fp_arc (start -0.7 0.675) (mid -0.753033 0.653033) (end -0.775 0.6)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e0a2518a-17a7-40f1-93eb-6ed12febf438))
  (fp_arc (start 0.7 -0.675) (mid 0.753033 -0.653033) (end 0.775 -0.6)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 85f4d2b8-4045-4446-b72e-b194e6ede705))
  (fp_arc (start 0.775 0.6) (mid 0.753033 0.653033) (end 0.7 0.675)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 362a0b81-f678-4224-a1d5-41280f02b5ff))
  (fp_poly
    (pts
      (xy -0.35 -0.6)
      (xy -0.2 -0.8)
      (xy -0.5 -0.8)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 180a1fd8-4192-4255-98d4-157594fc2a68))
  (fp_poly
    (pts
      (xy -0.45 0.6)
      (xy -0.7 0.6)
      (xy -0.7 -0.6)
      (xy -0.55 -0.6)
      (xy -0.55 -0.75)
      (xy -0.7 -0.75)
      (xy -0.85 -0.6)
      (xy -0.85 0.6)
      (xy -0.7 0.75)
      (xy -0.45 0.75)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1aabab5a-d7c2-4eb7-8f01-24b8e90b1d57))
  (fp_poly
    (pts
      (xy 0.45 -0.6)
      (xy 0.7 -0.6)
      (xy 0.7 0.6)
      (xy 0.45 0.6)
      (xy 0.45 0.75)
      (xy 0.7 0.75)
      (xy 0.85 0.6)
      (xy 0.85 -0.6)
      (xy 0.7 -0.75)
      (xy 0.45 -0.75)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2276b50b-7aab-48e9-94da-34f9fbfd5e8c))
  (fp_line (start -0.75 0.5) (end -0.75 -0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp eeeb0328-de15-46f2-a38b-eddf04d17384))
  (fp_line (start -0.5 -0.75) (end 0.5 -0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4879cf81-4997-4c65-af2b-f06af3e089ab))
  (fp_line (start 0.5 0.75) (end -0.5 0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 58d3e617-0a1d-4aba-9f3a-0c79d519fc6c))
  (fp_line (start 0.75 -0.5) (end 0.75 0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f941654-c701-4f1d-8aee-6dd057e98498))
  (fp_arc (start -0.75 -0.5) (mid -0.676777 -0.676777) (end -0.5 -0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp da1b2074-e792-431d-aa90-d01de178bbd8))
  (fp_arc (start -0.5 0.75) (mid -0.676777 0.676777) (end -0.75 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2f577e51-3cdb-4948-a690-40e19a25eefb))
  (fp_arc (start 0.5 -0.75) (mid 0.676777 -0.676777) (end 0.75 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0809c748-4068-4894-8e6b-678b025a2cd3))
  (fp_arc (start 0.75 0.5) (mid 0.676777 0.676777) (end 0.5 0.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dff27645-5686-44cc-a9b6-b48b05ed60b1))
  (fp_line (start -0.5 -0.5) (end 0.5 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77d44d0e-db13-4dce-b47b-da5475526c78))
  (fp_line (start -0.5 0.5) (end -0.5 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d285c13e-3d94-49de-b133-790326b3d844))
  (fp_line (start 0.5 -0.5) (end 0.5 0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 196085a2-dd6d-4a57-a624-268ab23d0c5a))
  (fp_line (start 0.5 0.5) (end -0.5 0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d3d5dac-8c7b-4af6-a3ef-651cf06ea036))
  (pad "" smd roundrect (at -0.43 -0.35) (size 0.34 0.21) (layers "F.Paste") (roundrect_rratio 0.15)
    (chamfer_ratio 0.5) (chamfer bottom_right)
    (zone_connect 0) (thermal_bridge_angle 45) (tstamp 6783c490-c82e-41f9-b16d-c1748adc176f))
  (pad "" smd roundrect (at -0.43 0.35 180) (size 0.34 0.21) (layers "F.Paste") (roundrect_rratio 0.15)
    (chamfer_ratio 0.5) (chamfer bottom_left)
    (zone_connect 0) (thermal_bridge_angle 45) (tstamp 5f79b7fe-1453-4c9a-87a0-4ab52b10d5cc))
  (pad "" smd roundrect (at 0 0 135) (size 0.45 0.45) (layers "F.Paste") (roundrect_rratio 0.2222222222) (tstamp 296ff8c2-7618-4493-9090-0fc8a3becef1))
  (pad "" smd roundrect (at 0.43 -0.35) (size 0.34 0.21) (layers "F.Paste") (roundrect_rratio 0.15)
    (chamfer_ratio 0.5) (chamfer bottom_left)
    (zone_connect 0) (thermal_bridge_angle 45) (tstamp f68d61be-f86d-4d89-bb24-6317067101f0))
  (pad "" smd roundrect (at 0.43 0.35 180) (size 0.34 0.21) (layers "F.Paste") (roundrect_rratio 0.15)
    (chamfer_ratio 0.5) (chamfer bottom_right)
    (zone_connect 0) (thermal_bridge_angle 45) (tstamp a96ed715-2a79-4847-8f3e-98e8eb5f959d))
  (pad "1" smd custom (at -0.485 -0.325 270) (size 0.26 0.23) (layers "F.Cu" "F.Mask")
    (zone_connect 0) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.13 -0.115)
          (xy -0.13 -0.115)
          (xy -0.13 -0.275)
          (xy -0.02 -0.275)
        )
        (width 0) (fill yes))
    ) (tstamp 552e9029-a9ad-40f8-b218-c6599f62a11a))
  (pad "2" smd custom (at -0.485 0.325 270) (size 0.26 0.23) (layers "F.Cu" "F.Mask")
    (zone_connect 0) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.13 -0.115)
          (xy -0.13 -0.115)
          (xy 0.02 -0.275)
          (xy 0.13 -0.275)
        )
        (width 0) (fill yes))
    ) (tstamp 571ae088-038f-4e29-af1c-c06b900918c7))
  (pad "3" smd custom (at 0.485 0.325 90) (size 0.26 0.23) (layers "F.Cu" "F.Mask")
    (zone_connect 0) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.13 -0.115)
          (xy -0.13 -0.115)
          (xy -0.13 -0.275)
          (xy -0.02 -0.275)
        )
        (width 0) (fill yes))
    ) (tstamp 11da4ff8-6e6e-48bb-8a24-97acc4bea530))
  (pad "4" smd custom (at 0.485 -0.325 90) (size 0.26 0.23) (layers "F.Cu" "F.Mask")
    (zone_connect 0) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.13 -0.115)
          (xy -0.13 -0.115)
          (xy 0.02 -0.275)
          (xy 0.13 -0.275)
        )
        (width 0) (fill yes))
    ) (tstamp dc912ad6-f2d9-4e93-9d72-738d39e36b3d))
  (pad "5" smd rect (at 0 0 135) (size 0.52 0.52) (layers "F.Cu" "F.Mask") (tstamp 946342b5-ca15-41f0-af01-0a5ad1adf714))
  (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/OnSemi_XDFN4-1EP_1.0x1.0mm_EP0.52x0.52mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
