(module TQFN1010-57 (layer F.Cu) (tedit 5B39023E)
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.001)
  (attr smd)
  (fp_text reference REF** (at -6 0 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value TQFN1010-57 (at 0 -6.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -5 -5) (end 5 -5) (layer F.Fab) (width 0.05))
  (fp_line (start 5 -5) (end 5 5) (layer F.Fab) (width 0.05))
  (fp_line (start 5 5) (end -5 5) (layer F.Fab) (width 0.05))
  (fp_line (start -5 5) (end -5 -5) (layer F.Fab) (width 0.05))
  (fp_line (start -5.4 -4.6) (end -5.4 -5.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.4 -5.4) (end -4.6 -5.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.6 -5.4) (end 5.4 -5.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.4 -5.4) (end 5.4 -4.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.4 4.6) (end 5.4 5.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.4 5.4) (end 4.6 5.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.6 5.4) (end -5.4 5.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.4 5.4) (end -5.4 4.6) (layer F.SilkS) (width 0.15))
  (fp_circle (center -5.7 -5.3) (end -5.7 -5.4) (layer F.SilkS) (width 0.15))
  (pad 1 smd roundrect (at -5 -4.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 2 smd roundrect (at -5 -3.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 3 smd roundrect (at -5 -3.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 4 smd roundrect (at -5 -2.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 5 smd roundrect (at -5 -2.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 6 smd roundrect (at -5 -1.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 7 smd roundrect (at -5 -1.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 8 smd roundrect (at -5 -0.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 9 smd roundrect (at -5 -0.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 10 smd roundrect (at -5 0.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 11 smd roundrect (at -5 0.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 12 smd roundrect (at -5 1.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 13 smd roundrect (at -5 1.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 14 smd roundrect (at -5 2.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 15 smd roundrect (at -5 2.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 16 smd roundrect (at -5 3.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 17 smd roundrect (at -5 3.75) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 18 smd roundrect (at -5 4.25) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 19 smd roundrect (at -4.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 20 smd roundrect (at -3.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 21 smd roundrect (at -3.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 22 smd roundrect (at -2.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 23 smd roundrect (at -2.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 24 smd roundrect (at -1.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 25 smd roundrect (at -1.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 26 smd roundrect (at -0.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 27 smd roundrect (at -0.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 28 smd roundrect (at 0.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 29 smd roundrect (at 0.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 30 smd roundrect (at 1.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 31 smd roundrect (at 1.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 32 smd roundrect (at 2.25 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 33 smd roundrect (at 2.75 5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 34 smd roundrect (at 5 3.5) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 35 smd roundrect (at 5 3) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 36 smd roundrect (at 5 2.5) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 37 smd roundrect (at 5 0.5) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 38 smd roundrect (at 5 0) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 39 smd roundrect (at 5 -0.5) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 40 smd roundrect (at 5 -2.5) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 41 smd roundrect (at 5 -3) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 42 smd roundrect (at 5 -3.5) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 43 smd roundrect (at 2.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 44 smd roundrect (at 2.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 45 smd roundrect (at 1.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 46 smd roundrect (at 1.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 47 smd roundrect (at 0.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 48 smd roundrect (at 0.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 49 smd roundrect (at -0.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 50 smd roundrect (at -0.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 51 smd roundrect (at -1.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 52 smd roundrect (at -1.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 53 smd roundrect (at -2.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 54 smd roundrect (at -2.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 55 smd roundrect (at -3.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 56 smd roundrect (at -3.75 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 57 smd roundrect (at -4.25 -5 90) (size 0.9 0.25) (layers F.Cu F.Mask) (roundrect_rratio 0.2))
  (pad 1 smd roundrect (at -5 -4.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 2 smd roundrect (at -5 -3.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 3 smd roundrect (at -5 -3.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 4 smd roundrect (at -5 -2.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 5 smd roundrect (at -5 -2.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 6 smd roundrect (at -5 -1.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 7 smd roundrect (at -5 -1.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 8 smd roundrect (at -5 -0.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 9 smd roundrect (at -5 -0.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 10 smd roundrect (at -5 0.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 11 smd roundrect (at -5 0.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 12 smd roundrect (at -5 1.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 13 smd roundrect (at -5 1.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 14 smd roundrect (at -5 2.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 15 smd roundrect (at -5 2.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 16 smd roundrect (at -5 3.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 17 smd roundrect (at -5 3.75 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 18 smd roundrect (at -5 4.25 180) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 19 smd roundrect (at -4.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 20 smd roundrect (at -3.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 21 smd roundrect (at -3.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 22 smd roundrect (at -2.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 23 smd roundrect (at -2.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 24 smd roundrect (at -1.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 25 smd roundrect (at -1.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 26 smd roundrect (at -0.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 27 smd roundrect (at -0.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 28 smd roundrect (at 0.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 29 smd roundrect (at 0.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 30 smd roundrect (at 1.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 31 smd roundrect (at 1.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 32 smd roundrect (at 2.25 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 33 smd roundrect (at 2.75 5 270) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 34 smd roundrect (at 5 3.5) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 35 smd roundrect (at 5 3) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 36 smd roundrect (at 5 2.5) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 37 smd roundrect (at 5 0.5) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 38 smd roundrect (at 5 0) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 39 smd roundrect (at 5 -0.5) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 40 smd roundrect (at 5 -2.5) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 41 smd roundrect (at 5 -3) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 42 smd roundrect (at 5 -3.5) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 43 smd roundrect (at 2.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 44 smd roundrect (at 2.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 45 smd roundrect (at 1.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 46 smd roundrect (at 1.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 47 smd roundrect (at 0.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 48 smd roundrect (at 0.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 49 smd roundrect (at -0.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 50 smd roundrect (at -0.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 51 smd roundrect (at -1.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 52 smd roundrect (at -1.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 53 smd roundrect (at -2.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 54 smd roundrect (at -2.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 55 smd roundrect (at -3.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 56 smd roundrect (at -3.75 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 57 smd roundrect (at -4.25 -5 90) (size 0.5 0.25) (layers F.Paste) (roundrect_rratio 0.2))
  (pad 58 smd roundrect (at 0 0) (size 5.1 3.1) (layers F.Cu F.Mask) (roundrect_rratio 0.03))
  (pad 58 thru_hole circle (at -2 -1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at -1 -1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 0 -1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 1 -1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 2 -1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at -2 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at -1 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 1 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 2 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at -2 1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at -1 1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 0 1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 1 1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 thru_hole circle (at 2 1) (size 0.7 0.7) (drill 0.3302) (layers *.Cu))
  (pad 58 smd roundrect (at -1.5 -0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at -0.5 -0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at 0.5 -0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at 1.5 -0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at -1.5 0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at -0.5 0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at 0.5 0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad 58 smd roundrect (at 1.5 0.85) (size 0.65 1.4) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
)
