(footprint "3P_4.5x4_4.5_pitch" (version 20220621) (generator pcbnew)
  (layer "F.Cu")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "M1" (at 0 -7.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b7cd0a39-251e-4edd-b5e6-135aad211c99)
  )
  (fp_text value "STEPPER" (at 2.5 0 270) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05)))
    (tstamp cf3bcf98-e4b7-4c63-a88b-783d00ff8a26)
  )
  (pad "1" connect roundrect (at 0 -4.5) (size 4.5 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp cb501d50-0779-44eb-994e-ef16eeab444a))
  (pad "2" connect roundrect (at 0 0) (size 4.5 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp b4c9e831-59fc-4a1d-9be5-e458b30dd381))
  (pad "3" connect roundrect (at 0 4.5) (size 4.5 4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.167) (tstamp e63ed007-3dbb-4535-b437-ce1ffc33b2e0))
)
