(module USB_Cable_Pads_4P (layer F.Cu) (tedit 54974959)
  (solder_mask_margin 0.05)
  (attr virtual)
  (fp_text reference USB_Cable_Pads_4P (at 0 -3.1) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 3) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 connect oval (at -2.75 0) (size 2.25 5) (layers F.Cu F.Mask))
  (pad 4 connect oval (at 2.75 0.1) (size 2.25 5) (layers F.Cu F.Mask))
  (pad 2 connect oval (at -0.75 0) (size 1.25 5) (layers F.Cu F.Mask))
  (pad 3 connect oval (at 0.75 0) (size 1.25 5) (layers F.Cu F.Mask))
)
