(footprint "TO-220-2_Horizontal_TabUp_SMD" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "TO-220-2, Horizontal, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF")
  (tags "TO-220-2 Horizontal RM 5.08mm")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "C2929078")
  (property "MFG" "Viking")
  (property "MPN" "TR35JDD0100")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "Servo_Controller.kicad_sch")
  (property "Sheetname" "")
  (property "Sim.Device" "SPICE")
  (property "Sim.Params" "")
  (property "Sim.Pins" "1=1 2=2")
  (property "Tolerance" "")
  (property "Voltage" "")
  (attr through_hole)
  (fp_text reference "R29" (at 0 -0.5 270) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 802243f1-8bc4-45f8-8d32-34f304f1719b)
  )
  (fp_text value "10R 35W" (at 0 0.95 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b3228f0e-6ce7-4c9b-b373-5d33847ea64a)
  )
  (fp_text user "${REFERENCE}" (at 0.05 2.9 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8c2eb73f-ecfb-4447-af90-41f3c89223ff)
  )
  (fp_line (start -5.25 -0.3) (end -5.25 15.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9ba0d4ae-8f63-437a-bef0-c11948aea92d))
  (fp_line (start -5.25 15.9) (end 5.25 15.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9c6317d9-6037-4af2-bcf9-f806eb740879))
  (fp_line (start -3.7 -3.65) (end -3.7 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c89e9f9f-ecc1-4a87-8f32-b8f2f91f86f9))
  (fp_line (start -3.7 -0.3) (end -5.25 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5c19b677-09eb-4cf6-8fc9-ba99539be22c))
  (fp_line (start -2.9 -4.45) (end -2.15 -4.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ea79e590-801b-4be1-a44d-2242dd4ace68))
  (fp_line (start -1.35 -3.65) (end -1.35 -0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3677c5c7-2526-4c98-b78c-1f9620dc601d))
  (fp_line (start -1.35 -0.25) (end 1.35 -0.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c908d1d8-564f-45a6-bbb5-2c41ea47c1b5))
  (fp_line (start 1.35 -0.25) (end 1.35 -3.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 05dca9f0-7275-4dfe-8c40-86b51349aed8))
  (fp_line (start 2.9 -4.45) (end 2.15 -4.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c404219b-59d2-4958-9929-61fdf9288a71))
  (fp_line (start 3.7 -3.65) (end 3.7 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ce94eeed-e87b-4a97-a4ee-c555e444a727))
  (fp_line (start 3.7 -0.3) (end 5.25 -0.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8f12358f-3f13-4409-8fc5-6256bbdd37ef))
  (fp_line (start 5.25 15.9) (end 5.25 -0.3)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 78dd564c-7c3f-4704-a857-befa0c6741a4))
  (fp_arc (start -3.7 -3.65) (mid -3.465685 -4.215685) (end -2.9 -4.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 468ffdbd-76e7-4723-9f88-23a510188d01))
  (fp_arc (start -2.15 -4.45) (mid -1.584315 -4.215685) (end -1.35 -3.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9c675767-7641-42f3-9cac-4c7915866af6))
  (fp_arc (start 1.35 -3.65) (mid 1.584315 -4.215685) (end 2.15 -4.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1b0d73c7-1724-4de1-b2a9-2b32891b0074))
  (fp_arc (start 2.9 -4.45) (mid 3.465685 -4.215685) (end 3.7 -3.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3057b738-177e-4b68-9c3e-d304d4403fca))
  (fp_line (start -5 0) (end -5 9.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12036f05-c00b-41a5-9a17-1f8a12aa196b))
  (fp_line (start -5 9.25) (end -5 15.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 298b2696-3426-4983-9277-aadbe469f223))
  (fp_line (start -5 9.25) (end 5 9.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 547486a5-a9b9-43bc-bd58-5a9aaf38dbdd))
  (fp_line (start -5 15.65) (end 5 15.65)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f20b3ada-8578-49af-9785-6c0ed524ea75))
  (fp_line (start 5 0) (end -5 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 426eb2d5-83f1-4cc4-accd-816f9401dbb0))
  (fp_line (start 5 9.25) (end -5 9.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 801bc01e-e4fa-46be-8326-63c5b3bac6db))
  (fp_line (start 5 9.25) (end 5 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 439c4136-67eb-4315-a2f2-01d9e8d03839))
  (fp_line (start 5 15.65) (end 5 9.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dae529e5-6793-408a-a626-11b9c96326d9))
  (fp_circle (center 0 12.85) (end 1.85 12.85)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2550999a-6505-4532-ab69-afd0bd814b0d))
  (pad "1" smd roundrect (at -2.54 -2.3) (size 2 4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right) (tstamp 734eabab-f25d-4739-9fa4-18d4724ff9bc))
  (pad "2" smd roundrect (at 2.54 -2.3) (size 2 4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right) (tstamp 1266df0c-46e9-41f9-a119-8fb286a98c13))
  (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-2_Horizontal_TabUp.wrl"
    (offset (xyz -2.54 3.81 -1.08))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
