(module Fuse_radial_lead_Bel_0697H (layer F.Cu) (tedit 5980B9E3)
  (fp_text reference F2 (at 0 -2.75) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 10A (at 0 1.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1 0) (end -1.5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0) (end 1.5 0) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0.5 0) (end 0 0) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_arc (start -0.5 0) (end 0 0) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.175 -2) (end -4.175 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.175 2) (end 4.175 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.175 2) (end 4.175 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.175 -2) (end -4.175 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.175 2) (end -4.175 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 4.175 2) (end -4.175 2) (layer F.Fab) (width 0.1))
  (fp_line (start 4.175 -2) (end 4.175 2) (layer F.Fab) (width 0.1))
  (fp_line (start -4.175 -2) (end 4.175 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -4.425 -2.25) (end -4.425 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.425 2.25) (end 4.425 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.425 2.25) (end 4.425 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.425 -2.25) (end -4.425 -2.25) (layer F.CrtYd) (width 0.05))
  (pad 2 connect roundrect (at 2.54 0) (size 1.2 2) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 1 connect roundrect (at -2.54 0) (size 1.2 2) (layers B.Cu B.Mask)(roundrect_rratio 0.25))
  (pad 2 thru_hole circle (at 2.54 0) (size 1 1) (drill 0.7) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.54 0) (size 1 1) (drill 0.7) (layers *.Cu *.Mask))
  (model "{KISYS3DMOD}/Fuse.3dshapes/Bel_0697Hxxxx.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
