(footprint "RJ45_Pulse_JXD6-0001NL_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "RJ45 ethernet transformer with magnetics (https://productfinder.pulseeng.com/doc_type/WEB301/doc_num/JXD6-0001NL/doc_part/JXD6-0001NL.pdf)")
  (tags "ethernet 8p8c transformer magjack")
  (attr smd)
  (fp_text reference "REF**" (at 0 -9.5 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 05c1233b-38a7-4b8f-a3b3-7099633f7c11)
  )
  (fp_text value "RJ45_Pulse_JXD6-0001NL_Horizontal" (at 0 9.5 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bee3a37e-3eec-4003-b9c4-b59e9a9baf1c)
  )
  (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 666de975-7bb0-4548-abc3-4538476c472b)
  )
  (fp_line (start -11.645 -8.52) (end 2.775 -8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 149832b2-91d1-4389-897b-a322de7dfca0))
  (fp_line (start -11.645 -6.55) (end -13.625 -6.55)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 406e230b-d1db-4a2d-9b20-29d838a62ef3))
  (fp_line (start -11.645 -6.55) (end -11.645 -8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ffb1793-5d48-4154-b312-3fc5446de66d))
  (fp_line (start -11.645 6.55) (end -11.645 8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 815320a4-fd4e-4408-95ab-36c13eb9266b))
  (fp_line (start -11.645 8.52) (end 2.775 8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 44362286-4e8f-4d15-81ad-d06b692754f6))
  (fp_line (start 7.775 -8.52) (end 11.645 -8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 506540ef-ea6d-4ff7-9da2-fbdfb9d967f5))
  (fp_line (start 7.775 8.52) (end 11.645 8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ed95bf3-1f25-4d60-b644-5f1cac503bab))
  (fp_line (start 11.645 -8.52) (end 11.645 8.52)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 913c3568-6359-4db0-8a6a-a0a34bec638f))
  (fp_line (start -14.13 -8.9) (end -14.13 8.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 73ee7eaf-e70c-48c7-a28d-4a305b4e51ce))
  (fp_line (start 12.03 -8.9) (end -14.13 -8.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a6cd8711-c163-4087-9edd-3a57804cf65c))
  (fp_line (start 12.03 -8.9) (end 12.03 8.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c74a171a-3c9a-4dd6-aa0f-f6113c80c8ef))
  (fp_line (start 12.03 8.9) (end -14.13 8.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 951633d7-1194-4599-a94b-e35d34563be9))
  (fp_line (start -11.525 -7.4) (end -11.525 8.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7961466-da05-4f38-83b0-6b1db86e2c12))
  (fp_line (start -11.525 -7.4) (end -10.525 -8.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 219db8cb-09a5-4626-a0d9-521810150107))
  (fp_line (start 11.525 -8.4) (end -10.525 -8.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65f34242-7d9f-42f0-8dac-2ba5195821cf))
  (fp_line (start 11.525 8.4) (end -11.525 8.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d51f2ad-eb5b-4c2e-8d03-7e31281c79a8))
  (fp_line (start 11.525 8.4) (end 11.525 -8.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d00a021d-2b5b-46a3-8c2d-6785258babe4))
  (pad "" np_thru_hole circle (at 0.775 -5.715) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask") (tstamp 02b239f8-518c-49d1-bd49-baaeec359007))
  (pad "" np_thru_hole circle (at 0.775 5.715) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask") (tstamp ac5b6b6e-25ae-4a23-ad09-1ef599982625))
  (pad "1" smd roundrect (at -11.875 -5.715) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9e881987-bf69-42f3-aa52-767e05de7672))
  (pad "2" smd roundrect (at -11.875 -4.445) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 104d467c-901f-47f3-a487-89eccffdfeb9))
  (pad "3" smd roundrect (at -11.875 -3.175) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e0ec4dbd-1248-4b94-bff5-a8f09380e682))
  (pad "4" smd roundrect (at -11.875 -1.905) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 54adc38a-5bb1-417a-98c4-ce066e7219ca))
  (pad "5" smd roundrect (at -11.875 -0.635) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6d520272-4551-40d3-a060-ca2854ed8440))
  (pad "6" smd roundrect (at -11.875 0.635) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6d3cdc9e-1268-4224-a07d-51d1bcdce144))
  (pad "7" smd roundrect (at -11.875 1.905) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ce3a9788-2edc-48b0-b3e6-a5221ed19a8d))
  (pad "8" smd roundrect (at -11.875 3.175) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f7d85f06-3ecd-4835-99d5-f366809f518d))
  (pad "9" smd roundrect (at -11.875 4.445) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a93c99ae-6629-4997-bb16-aaf416b2a87a))
  (pad "10" smd roundrect (at -11.875 5.715) (size 3.5 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4ee8aec0-e999-4936-8563-b41620487a7e))
  (pad "SH" smd roundrect (at 5.275 -6.77) (size 4.6 3.26) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d5551536-8702-45cb-b9e5-6d65f55ebb2d))
  (pad "SH" smd roundrect (at 5.275 6.77) (size 4.6 3.26) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3f87217f-0bbe-44ee-857a-742f0c7d6a9f))
  (model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Pulse_JXD6-0001NL_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_RJ.3dshapes/JXD6-0001NL.STEP"
    (offset (xyz 11.27 -0.25 -3.3))
    (scale (xyz 1 1 1))
    (rotate (xyz -180 0 90))
  )
)
