(footprint "Forlinx FET3588-C" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "exclude_from_bom" "")
  (attr exclude_from_bom)
  (fp_text reference "A1" (at 0 -24 180 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a8434c03-e224-41f8-a8fe-f950ab0b1bff)
  )
  (fp_text value "Forlinx FET3588-C" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8721c4eb-0cc1-481a-a4e7-72cd8acaaa1e)
  )
  (fp_text user "P4" (at 26 -22.5 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify right bottom))
    (tstamp 1869dc3c-13d2-4a38-98c2-dae659ae63f8)
  )
  (fp_text user "P1" (at -26 22 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 5370ce91-8537-4d3e-8f40-062406a69716)
  )
  (fp_text user "P2" (at -26 -22 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp d1843b84-8109-401b-8b09-d02b305bedbc)
  )
  (fp_text user "Board needs >= 1.5mm stack height to clear" (at 0 19.25 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
    (tstamp e3c2da2b-ca05-4c46-99eb-533900be2bba)
  )
  (fp_text user "P3" (at 26 22.5 unlocked) (layer "Dwgs.User")
      (effects (font (size 1 1) (thickness 0.15)) (justify right bottom))
    (tstamp e7335a41-1fe7-47f0-b9f6-dea23b7f8947)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cca6c9f5-3776-472f-9ef0-0cbd981c91b5)
  )
  (fp_line (start -26 -22) (end -8 -22)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 95845cd7-79d8-4959-9825-8c6b4d625292))
  (fp_line (start -26 -20.5) (end -25 -20.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp d50d4b02-4a5b-40c3-9363-0df695a902e8))
  (fp_line (start -26 22) (end -8 22)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 7511ea67-3cf2-46c5-b669-6cff30a4b076))
  (fp_line (start -26 24) (end -25 24)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 3714ad6c-af1c-40f4-aa55-bdb391cb262d))
  (fp_line (start -25.5 -21.5) (end -26 -20.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp d2a6ead6-8461-437c-9baf-850c42bf703f))
  (fp_line (start -25.5 23) (end -26 24)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 55a399b5-a3bc-4daf-9207-6feafc070fbd))
  (fp_line (start -25 -20.5) (end -25.5 -21.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp ca974918-f7d0-4b1b-90ed-e33ba47cfdbc))
  (fp_line (start -25 24) (end -25.5 23)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp aa633c7d-db6a-4272-84af-b952131d482d))
  (fp_line (start -17 -25.5) (end -17 -19.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 29c23ccc-0080-40ed-a355-b7ada2587eae))
  (fp_line (start -17 18.5) (end -17 24.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 1444f814-1495-46ae-b13a-fc3bbdb95328))
  (fp_line (start 8 -22.5) (end 26 -22.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 44fc14f9-a87a-4b28-966f-4d330ee036f0))
  (fp_line (start 8 -21) (end 9 -21)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 613c07ef-a4a8-4bb0-ac4f-7f327c1b2bd3))
  (fp_line (start 8 22.5) (end 26 22.5)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp f38b4f42-6462-4b9c-93f7-012bef30df9e))
  (fp_line (start 8 24) (end 9 24)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 06cd88f6-a2a2-42c8-8fd5-75132ee88969))
  (fp_line (start 8.5 -22) (end 8 -21)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 8ebb93df-579c-446b-9703-7eebd163892d))
  (fp_line (start 8.5 23) (end 8 24)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 0fa4db34-e4a9-43a7-8430-af4093005ef1))
  (fp_line (start 9 -21) (end 8.5 -22)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 7e4a5196-5ab3-4921-881b-ca795aba9de0))
  (fp_line (start 9 24) (end 8.5 23)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 85deef4b-0ff1-4e7c-be6b-018cfc670930))
  (fp_line (start 17 -26) (end 17 -20)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 2f7e7604-9848-4e32-a680-624ffa71d641))
  (fp_line (start 17 19) (end 17 25)
    (stroke (width 0.12) (type dash)) (layer "Dwgs.User") (tstamp 7b4d4f59-b5b5-4f31-9e43-e4ba6a3b0949))
  (fp_line (start -34 23) (end -34 -23)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7a4d55f0-6ddb-4d0c-b3c2-85367ea626ff))
  (fp_line (start -32 -25) (end 32 -25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp e39fb3a0-1ef3-426b-8335-11b5255ad403))
  (fp_line (start 32 25) (end -32 25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 071e0a61-83c2-46ad-bb46-e831dada31b4))
  (fp_line (start 34 -23) (end 34 23)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp dda015ec-0f44-4225-985d-cc83c75974ba))
  (fp_arc (start -34 -23) (mid -33.414214 -24.414214) (end -32 -25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp eeaae8a2-d9cc-4c23-b7bd-1dbd86cff382))
  (fp_arc (start -32 25) (mid -33.414214 24.414214) (end -34 23)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 5a1bf92d-d2a5-4ff0-a692-7843a951b533))
  (fp_arc (start 32 -25) (mid 33.414214 -24.414214) (end 34 -23)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c1a05650-32e0-451c-8221-11a045547a78))
  (fp_arc (start 34 23) (mid 33.414214 24.414214) (end 32 25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp baa6469d-3f5a-4ff8-9068-d7bf01160f31))
  (fp_circle (center -32.000001 -23.000001) (end -31 -23)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 82746f64-614a-4ebd-b11d-3031f5f4670f))
  (fp_circle (center -32.000001 23.000001) (end -31 23)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 4185f9d5-475a-415f-a1a1-11ae8369b4c9))
  (fp_circle (center 32 -23) (end 33 -23)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 12a18dcc-5896-4911-b0cf-26fabb0ed3be))
  (fp_circle (center 32 23) (end 33 23)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp e1aaa56d-8300-4f9a-82dd-8a6396c0d98a))
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp ac3c4e5a-45a2-4949-9a99-01962b0a216b) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -34 -20)
        (xy -5 -20)
        (xy -5 -25)
        (xy 5 -25)
        (xy 5 -20.5)
        (xy 34 -20.5)
        (xy 34 20.5)
        (xy 5 20.5)
        (xy 5 25)
        (xy -5 25)
        (xy -5 20)
        (xy -34 20)
      )
    )
  )
  (model "${KICAD7_3DMODEL_DIR}/Module.3dshapes/Forlinx FET3588-C.STEP" hide
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -180))
  )
  (model "${KICAD7_3DMODEL_DIR}/Module.3dshapes/Forlinx FET3588-C with heatsink.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -180))
  )
)
