(module Diode_Bridge_30x4.6 (layer F.Cu) (tedit 58F856DB)
  (fp_text reference REF** (at 0 8.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Diode_Bridge_30x4.6 (at 0 -1.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -15 0) (end 15 0) (layer F.Fab) (width 0.05))
  (fp_line (start 15 0) (end 15 4.6) (layer F.Fab) (width 0.05))
  (fp_line (start 15 4.6) (end -15 4.6) (layer F.Fab) (width 0.05))
  (fp_line (start -15 4.6) (end -15 0) (layer F.Fab) (width 0.05))
  (fp_line (start -15 3.6) (end 15 3.6) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 3.6) (end -1.6 0) (layer F.Fab) (width 0.05))
  (fp_line (start -1.6 0) (end -1.6 0) (layer F.Fab) (width 0.05))
  (fp_line (start 1.6 3.6) (end 1.6 0) (layer F.Fab) (width 0.05))
  (fp_line (start 1.6 0) (end 1.6 0) (layer F.Fab) (width 0.05))
  (fp_line (start -15.5 -0.5) (end -15.5 0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -15.5 0.5) (end -15.5 0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -15.5 -0.5) (end -14.5 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -14.5 -0.5) (end -14.5 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -15.5 5.1) (end -15.5 4.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -15.5 4.1) (end -15.5 4.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -15.5 5.1) (end -14.5 5.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -14.5 5.1) (end -14.5 5.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 15.5 5.1) (end 14.5 5.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 14.5 5.1) (end 14.5 5.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 15.5 5.1) (end 15.5 4.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 15.5 4.1) (end 15.5 4.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 15.5 -0.5) (end 15.5 0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 15.5 0.5) (end 15.5 0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 15.5 -0.5) (end 14.5 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 14.5 -0.5) (end 14.5 -0.5) (layer F.SilkS) (width 0.125))
  (pad 1 thru_hole circle (at -12.5 3.05) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -2.5 3.05) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5 3.05) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 12.5 3.05) (size 1.6 1.6) (drill 1.3) (layers *.Cu *.Mask))
)
