(footprint "1006_B_KA" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0402 1005 Capacitor")
  (property "Dielectric" "X5R")
  (property "Footprint_Density" "C")
  (property "Footprint_Library" "Capacitor_SMD")
  (property "JLCPCB Part" "C1525")
  (property "LCSC" "C162179")
  (property "MFG" "Murata Electronics")
  (property "MPN" "GRM155R62A104ME14D")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "1005")
  (property "Sheetfile" "Servo_Controller.kicad_sch")
  (property "Sheetname" "")
  (property "Sim.Device" "SPICE")
  (property "Sim.Params" "type=\"C\" model=\"100n\" lib=\"\"")
  (property "Sim.Pins" "1=1 2=2")
  (property "Tolerance" "10%")
  (property "Voltage" "100V")
  (solder_mask_margin 0.03)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "D12" (at 0.85 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.4 0.4) (thickness 0.1)) (justify left))
    (tstamp f8e7c50d-4657-4fc2-9a31-97496243aa8d)
  )
  (fp_text value "12V" (at 0.85 0.375 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp 834b4ed7-4d61-4c86-a683-e3654632c5e4)
  )
  (fp_arc (start -0.9 -0.175) (mid -0.819454 -0.369454) (end -0.625 -0.45)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 1f66043e-1a27-4e30-975a-0e9000fca700))
  (fp_arc (start -0.625 0.45) (mid -0.819454 0.369454) (end -0.9 0.175)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 0fb0960d-27e0-4cc4-b901-f0683bfcea22))
  (fp_poly
    (pts
      (xy -0.825 -0.175)
      (xy -0.825 0.175)
      (xy -0.975 0.175)
      (xy -0.975 -0.175)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 61a585a0-9e99-4b30-bf86-c5cea96aaaf6))
  (fp_poly
    (pts
      (xy 0.225 -0.375)
      (xy -0.625 -0.375)
      (xy -0.625 -0.525)
      (xy 0.225 -0.525)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 57719c3f-f1e2-4e3b-a6f6-8e0f2a2e70b4))
  (fp_poly
    (pts
      (xy 0.225 0.525)
      (xy -0.625 0.525)
      (xy -0.625 0.375)
      (xy 0.225 0.375)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 3dd6a80b-6f59-4be4-bc3e-8b354aa89d70))
  (fp_line (start -0.9 -0.175) (end -0.9 0.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 969d64c4-df13-496d-8434-16702210d259))
  (fp_line (start -0.625 0.45) (end 0.625 0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3e2ca2b9-509f-4575-833f-186231b48f13))
  (fp_line (start 0.625 -0.45) (end -0.625 -0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b06a48b6-2d65-467e-9643-6880d916bf04))
  (fp_line (start 0.9 0.175) (end 0.9 -0.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9c43a527-bb33-4905-a2bc-c436bd17c1e8))
  (fp_arc (start -0.9 -0.175) (mid -0.819454 -0.369454) (end -0.625 -0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ecce51e3-dbc2-479a-a46b-1359a1295ca2))
  (fp_arc (start -0.625 0.45) (mid -0.819454 0.369454) (end -0.9 0.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 808c45fc-eb18-4dfc-98ef-7abda2240239))
  (fp_arc (start 0.625 -0.45) (mid 0.819454 -0.369454) (end 0.9 -0.175)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7d78b40a-5427-4b6a-b74c-685e17963a8a))
  (fp_arc (start 0.9 0.175) (mid 0.819454 0.369454) (end 0.625 0.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 79937770-0c62-4309-818a-049b1ee5d93b))
  (fp_rect (start -0.5 -0.3) (end 0.5 0.3)
    (stroke (width 0.01) (type solid)) (fill none) (layer "F.Fab") (tstamp d8593e18-0b4c-4c54-a107-6ea8cd76b701))
  (pad "" smd oval (at -0.5 0) (size 0.4 0.5) (layers "F.Paste") (tstamp 5facdda8-34e5-42d5-b278-10e5946aa3c6))
  (pad "" smd oval (at 0.5 0) (size 0.4 0.5) (layers "F.Paste") (tstamp 6b76b0e3-7225-42a8-b514-1e59de160c00))
  (pad "A" smd roundrect (at 0.5 0) (size 0.5 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer top_left bottom_left) (tstamp eda3421e-bd66-4f0b-be77-add58201a8f6))
  (pad "K" smd roundrect (at -0.5 0) (size 0.5 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp e2177e58-d4c8-45f0-8cb6-968cd47d3fa1))
  (model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
