(footprint "TSSOP-20_4.4x6.5mm_P0.65mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "SSOP 0.65")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "C2874739")
  (property "MFG" "UNI-SEMI")
  (property "MPN" "U5316")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "../../library/blocks/UNI-SEMI U5315 Gate Driver.kicad_sch")
  (property "Sheetname" "Gate Driver")
  (property "Sim.Device" "SPICE")
  (property "Sim.Params" "")
  (property "Sim.Pins" "1=1 2=2 3=3 4=4 5=5 6=6 7=7 8=8 9=9 10=10 11=11 12=12 13=13 14=14 15=15 16=16 17=17 18=18 19=19 20=20")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (attr smd)
  (fp_text reference "U13" (at 0 -4.3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c728eb72-18dc-4606-8c5b-90838a3b51c7)
  )
  (fp_text value "UNI-SEMI U5315" (at 0 4.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4aa5d575-bbcd-4b17-982b-54af54ec10b8)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 9378c1b8-8b35-4753-99d4-c36f08e5a819)
  )
  (fp_line (start -3.75 -3.45) (end 2.225 -3.45)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp d35a9129-fdfa-4e1c-818b-235df87fb598))
  (fp_line (start -2.225 3.45) (end 2.225 3.45)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp fe631c87-5dca-4999-b403-ec45024f4138))
  (fp_line (start -3.825 3.05) (end -3.825 -3.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp de16983c-14b5-4c02-a516-21a34b4328bb))
  (fp_line (start -3.575 -3.3) (end -2.445145 -3.299029)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c56f814f-e7f6-4018-bc1e-fbc888ab3cf4))
  (fp_line (start -3.575 3.3) (end -2.445145 3.299029)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8abbfada-b014-439c-aa87-1b4715caa7ba))
  (fp_line (start -2.2 -3.5) (end 2.2 -3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5194efaa-64b1-4769-88de-ff9f478eab3f))
  (fp_line (start 2.2 3.5) (end -2.2 3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 46be2976-73f7-4a68-9f5e-0ee01bbb5983))
  (fp_line (start 3.575 -3.3) (end 2.445145 -3.299029)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8000bba7-833a-418f-96ab-1fdaa2cc49fa))
  (fp_line (start 3.575 3.3) (end 2.445145 3.299029)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ff5c65b9-83d1-47f8-8cca-67bcfbf033c8))
  (fp_line (start 3.825 -3.05) (end 3.825 3.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 57e84da3-1417-4145-93a9-a82fe4bece8c))
  (fp_arc (start -3.825 -3.05) (mid -3.751777 -3.226777) (end -3.575 -3.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 833d8de2-a1e8-4309-b239-1bee38d083d0))
  (fp_arc (start -3.575 3.3) (mid -3.751777 3.226777) (end -3.825 3.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 809ae9de-fef8-4bfe-9895-01393c5cc2fa))
  (fp_arc (start -2.445145 -3.299029) (mid -2.358497 -3.443335) (end -2.2 -3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e814fe8c-7b51-4d30-bdea-418c7ceff033))
  (fp_arc (start -2.2 3.5) (mid -2.358497 3.443336) (end -2.445145 3.299029)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6b70bf8b-602d-4a98-929f-8af6d2e254ae))
  (fp_arc (start 2.2 -3.5) (mid 2.358497 -3.443336) (end 2.445145 -3.299029)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b938104a-01fe-4042-8d07-f8a1c3529d2b))
  (fp_arc (start 2.445145 3.299029) (mid 2.358497 3.443335) (end 2.2 3.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4436f79f-fe2c-4952-9b3d-9e2779208fad))
  (fp_arc (start 3.575 -3.3) (mid 3.751777 -3.226777) (end 3.825 -3.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3fadc4f9-ce52-4a39-b132-5f3886476bba))
  (fp_arc (start 3.825 3.05) (mid 3.751777 3.226777) (end 3.575 3.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8151d143-4dac-4cc8-ae7b-bb58437855c6))
  (fp_line (start -2.2 -2.25) (end -1.2 -3.25)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp a0edac77-9b8b-43e7-8e28-4034aee6288d))
  (fp_line (start -2.2 3.25) (end -2.2 -2.25)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ad9e032a-5b22-4aaf-9d72-7a6f89b583bc))
  (fp_line (start -1.2 -3.25) (end 2.2 -3.25)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 89b1f77f-5ca5-46d3-b884-89329e559ad5))
  (fp_line (start 2.2 -3.25) (end 2.2 3.25)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp e7f2aa68-81f0-4180-b868-5cf0aeb42fc6))
  (fp_line (start 2.2 3.25) (end -2.2 3.25)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 1c9a8be7-2a6b-4447-a549-14aabdbd7eb9))
  (pad "1" smd roundrect (at -2.95 -2.925) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 59190568-8ed1-492f-b87a-4168889cbbcf))
  (pad "2" smd roundrect (at -2.95 -2.275) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4d8a231f-277a-4761-a9c3-83c10dcb679b))
  (pad "3" smd roundrect (at -2.95 -1.625) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1d32d294-9261-4eac-811d-4a05d6314c14))
  (pad "4" smd roundrect (at -2.95 -0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8e19da56-0e07-458f-a5ee-0e36d1e781b8))
  (pad "5" smd roundrect (at -2.95 -0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 582ab7db-bfc5-4900-8615-783809a34cec))
  (pad "6" smd roundrect (at -2.95 0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 00a07697-9718-4b42-8a07-b119aa6ef78c))
  (pad "7" smd roundrect (at -2.95 0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9e60a362-155c-4570-9942-7439e46360b7))
  (pad "8" smd roundrect (at -2.95 1.625) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4ed89731-e502-4383-a27f-4b1f5114439e))
  (pad "9" smd roundrect (at -2.95 2.275) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bed86fd2-0d3c-4163-82f1-b88a6f671327))
  (pad "10" smd roundrect (at -2.95 2.925) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0781bef8-5a67-45dc-b3a5-c5bd44d463b3))
  (pad "11" smd roundrect (at 2.95 2.925) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp aeb118e7-dcf9-4239-8c86-a0b00ea6c15d))
  (pad "12" smd roundrect (at 2.95 2.275) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9a36dce4-9353-4442-b40c-017c15b11d26))
  (pad "13" smd roundrect (at 2.95 1.625) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4ecc9ee8-1e6a-4905-b2f4-0a8ca401dba4))
  (pad "14" smd roundrect (at 2.95 0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 27431dcc-6db1-4087-a0ac-79fee34e2b02))
  (pad "15" smd roundrect (at 2.95 0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp adcae0f0-ec70-42a5-bc86-ac21cd2fee1c))
  (pad "16" smd roundrect (at 2.95 -0.325) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cd5b7987-2c30-4247-a7ec-48d4b5a605a6))
  (pad "17" smd roundrect (at 2.95 -0.975) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0e3973c3-687b-4704-a658-c9e30ad80dbd))
  (pad "18" smd roundrect (at 2.95 -1.625) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c6440f62-2523-4942-ba4f-180e9ee4d5b0))
  (pad "19" smd roundrect (at 2.95 -2.275) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fa651b00-65e4-4fa9-9a98-1335e7757528))
  (pad "20" smd roundrect (at 2.95 -2.925) (size 1.45 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 783f46fa-c561-4bf9-a215-e4e85a2b08ba))
  (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
