(footprint "Texas_VQFN-HR_RPA0010A_3x3_10P" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.35 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 04787ca4-ff83-4402-b236-c501d0524c19)
  )
  (fp_text value "Texas_VQFN-HR_RPA0010A_3x3_10P" (at 0 -3 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp a367414c-2822-45fd-a910-ceb35074250e)
  )
  (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 60d1271d-cf2f-4638-a78e-ef0f72ee1030)
  )
  (fp_arc (start -1.675 -1.6) (mid -1.653033 -1.653033) (end -1.6 -1.675)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 960c2507-c456-4034-bb35-4354ae547ac1))
  (fp_arc (start -1.6 1.675) (mid -1.653033 1.653033) (end -1.675 1.6)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 16cf6cf2-499d-4502-a6dd-86c4f605aa26))
  (fp_arc (start 1.6 -1.675) (mid 1.653033 -1.653033) (end 1.675 -1.6)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp bb14dfcf-2457-4ccc-9b57-083ee7753318))
  (fp_arc (start 1.675 1.6) (mid 1.653033 1.653033) (end 1.6 1.675)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 45f49454-b70c-4d3f-9379-3eb3f2165214))
  (fp_poly
    (pts
      (xy -1.8 -0.75)
      (xy -2.05 -0.9)
      (xy -2.05 -0.6)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b44c98f9-1971-454f-81ca-3a5a0e455046))
  (fp_poly
    (pts
      (xy -1.6 -1.6)
      (xy -1.2 -1.6)
      (xy -1.2 -1.75)
      (xy -1.6 -1.75)
      (xy -1.75 -1.6)
      (xy -1.75 -1)
      (xy -1.6 -1)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e54d119f-2e25-4aca-975e-337477fe716e))
  (fp_poly
    (pts
      (xy -1.6 1.6)
      (xy -1.2 1.6)
      (xy -1.2 1.75)
      (xy -1.6 1.75)
      (xy -1.75 1.6)
      (xy -1.75 1)
      (xy -1.6 1)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e3698b3e-2d36-4b9f-af84-117f0ebcacf5))
  (fp_poly
    (pts
      (xy 1.6 -1.6)
      (xy 1.25 -1.6)
      (xy 1.25 -1.75)
      (xy 1.6 -1.75)
      (xy 1.75 -1.6)
      (xy 1.75 -1)
      (xy 1.6 -1)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8272f7f1-31b7-434d-bf22-67683828ca53))
  (fp_poly
    (pts
      (xy 1.6 1.6)
      (xy 1.2 1.6)
      (xy 1.2 1.75)
      (xy 1.6 1.75)
      (xy 1.75 1.6)
      (xy 1.75 1)
      (xy 1.6 1)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5f5cddcf-e1eb-42c2-b4a1-948cf2f311d2))
  (fp_line (start -1.95 1.5) (end -1.95 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 654713e0-b938-4cfa-b6d4-01d9defde00c))
  (fp_line (start -1.5 -1.95) (end 1.5 -1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0efb9e5e-309e-4396-a6b2-1b25fce12b0d))
  (fp_line (start 1.5 1.95) (end -1.5 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1395d78c-6a45-46ad-8530-f5c7aa6a6251))
  (fp_line (start 1.95 -1.5) (end 1.95 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dbed07d9-b0b1-44b1-8e7e-c6845d4a80f8))
  (fp_arc (start -1.95 -1.5) (mid -1.818198 -1.818198) (end -1.5 -1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ec0bca9a-af23-4dd2-ac35-7588d178840c))
  (fp_arc (start -1.5 1.95) (mid -1.818198 1.818198) (end -1.95 1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d6eda03c-cddf-49e6-ab82-74e8aaaf6a4a))
  (fp_arc (start 1.5 -1.95) (mid 1.818198 -1.818198) (end 1.95 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 75fc0c7f-d85c-498f-9637-2a4bc3a3f608))
  (fp_arc (start 1.95 1.5) (mid 1.818198 1.818198) (end 1.5 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6443e7cd-684d-4584-85d1-22c44ae79c39))
  (fp_rect (start -1.5 -1.5) (end 1.5 1.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 110b247f-e083-4da4-9fe7-a067dedc05eb))
  (pad "" smd roundrect (at -0.21 -1.25) (size 0.4 0.9) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp b691ae22-90e6-4245-af9a-688defa92942))
  (pad "" smd roundrect (at -0.21 -0.05) (size 0.4 0.9) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp 36724d0f-1488-4cde-89e9-14b76545987a))
  (pad "" smd roundrect (at 0.37 0.35) (size 0.25 0.7) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp dfe1d607-e349-493f-96cd-42b03b23f94b))
  (pad "" smd roundrect (at 0.37 1.35) (size 0.25 0.7) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp a57a2501-f807-432d-9e7b-667efe895bd7))
  (pad "" smd roundrect (at 0.95 -1.35) (size 0.4 0.7) (layers "F.Paste") (roundrect_rratio 0.25)
    (thermal_bridge_angle 45) (tstamp acd19d6b-4b72-4ecc-8e6a-0f6f724b9fcd))
  (pad "1" smd roundrect (at -1.4 -0.75) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 8963c39f-f250-46d6-9c7c-994007d65653))
  (pad "2" smd roundrect (at -1.4 -0.25) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 9180112d-97ea-44bd-8c7c-9b518061ca59))
  (pad "3" smd roundrect (at -1.4 0.25) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 78a20d95-0ac8-465a-9967-c5dc1c1191c6))
  (pad "4" smd roundrect (at -1.4 0.75) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 195c78d0-94c3-489e-b0bc-3d207b320eca))
  (pad "5" smd roundrect (at -0.93 1.4 90) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 51e25eb4-9938-430d-838b-a1008cba4717))
  (pad "6" smd roundrect (at 0.37 0.85 90) (size 1.7 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 64d7b20c-3a07-4bcb-af08-492937805196))
  (pad "7" smd roundrect (at 0.87 1.4 90) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 931cf000-8343-4211-8460-cf40532c4bbb))
  (pad "8" smd roundrect (at 0.95 -0.65 90) (size 2.1 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 1293526d-009a-4c2f-b1ba-c8449f29ba9b))
  (pad "8" smd roundrect (at 1.23 -0.75) (size 0.94 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 64b6e390-24d3-43cd-83af-d8cd37186dd7))
  (pad "8" smd roundrect (at 1.23 -0.25) (size 0.94 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 4d0b18f5-2037-4e9d-bf02-3167316e510f))
  (pad "8" smd roundrect (at 1.23 0.25) (size 0.94 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 6a3ad8ad-5f91-42e7-af98-65659d156191))
  (pad "9" smd roundrect (at -0.21 -0.65 90) (size 2.1 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 1b56abf3-aa2d-419a-862f-5285a8b54378))
  (pad "10" smd roundrect (at -0.93 -1.4 90) (size 0.6 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
    (thermal_bridge_angle 45) (tstamp 638548c7-5fde-41be-9180-4dbfde5992c9))
  (model ":KICAD7_3DMODEL_DIR:Package_DFN_QFN.3dshapes/rpa0010a.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
