(module DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm_C (layer F.Cu) (tedit 5BA542D3)
  (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
  (tags "DFN 0.5")
  (attr smd)
  (fp_text reference U2 (at 0 -2.05) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Microchip_ATECC608A (at 0 2.05) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.105)))
  )
  (fp_line (start -1.5 -1) (end 1.5 -1) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 -1) (end 1.5 1) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 1) (end -1.5 1) (layer F.Fab) (width 0.05))
  (fp_line (start -1.5 -1) (end -1.5 1) (layer F.Fab) (width 0.05))
  (fp_line (start -1.75 -1.25) (end -1.75 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 -1.25) (end 1.75 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -1.25) (end 1.75 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 1.25) (end 1.75 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.075 1.125) (end 1.075 1.125) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.675 -1.125) (end 1.075 -1.125) (layer F.SilkS) (width 0.15))
  (pad 1 smd roundrect (at -1.4125 -0.75) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 0 0) (size 1.3 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.077))
  (pad "" smd roundrect (at -0.325 -0.375) (size 0.5 0.6) (layers F.Paste) (roundrect_rratio 0.15))
  (pad "" smd roundrect (at -0.325 0.375) (size 0.5 0.6) (layers F.Paste) (roundrect_rratio 0.15))
  (pad "" smd roundrect (at 0.325 -0.375) (size 0.5 0.6) (layers F.Paste) (roundrect_rratio 0.15))
  (pad "" smd roundrect (at 0.325 0.375) (size 0.5 0.6) (layers F.Paste) (roundrect_rratio 0.15))
  (pad 2 smd roundrect (at -1.4125 -0.25) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.4125 0.25) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -1.4125 0.75) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 1.4125 0.75) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1.4125 0.25) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 1.4125 -0.25) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 1.4125 -0.75) (size 0.675 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
