(module MEAS_MS8607-02BA01 (layer F.Cu) (tedit 5BDDBB5B)
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.075)
  (attr smd)
  (fp_text reference U2 (at 0 -3.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value MEAS_MS8607-02BA01 (at 0 3.3 180) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -1.7 2.7) (end -1.7 2.4) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.7 2.7) (end 1.7 2.4) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 -2.7) (end -1.7 -2.4) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.7 -2.7) (end 1.7 -2.4) (layer F.SilkS) (width 0.125))
  (fp_text user "NO TRACKS HERE" (at -0.3 -0.2 90) (layer Cmts.User)
    (effects (font (size 0.25 0.25) (thickness 0.05)))
  )
  (fp_line (start -1.5 -1.875) (end -1.5 1.875) (layer Dwgs.User) (width 0.05))
  (fp_line (start -1.5 1.875) (end 1.5 1.875) (layer Dwgs.User) (width 0.05))
  (fp_line (start 1.5 1.875) (end 1.5 -1.875) (layer Dwgs.User) (width 0.05))
  (fp_line (start 1.5 -1.875) (end -1.5 -1.875) (layer Dwgs.User) (width 0.05))
  (fp_circle (center -0.65 1.65) (end -0.65 1.9) (layer F.Fab) (width 0.05))
  (fp_circle (center 0.65 -1.65) (end 0.65 -1.9) (layer F.Fab) (width 0.05))
  (fp_circle (center -2.1 -2.5) (end -2.2 -2.5) (layer F.SilkS) (width 0.2))
  (fp_line (start 1.7 2.7) (end 1.2 2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 2.7) (end -1.2 2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.7 -2.7) (end 1.2 -2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.7 -2.7) (end -1.2 -2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.75 -2.75) (end 1.75 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 2.75) (end -1.75 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 2.75) (end -1.75 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -2.75) (end 1.75 -2.75) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -1.1 -1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.1 -0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.1 0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.1 1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.1 1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.1 0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.1 -0.625) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.1 -1.875) (size 1.1 0.6) (layers F.Cu F.Paste F.Mask))
  (model Sensor_Pressure.3dshapes/MEAS_MS5611-01BA03.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
