(footprint "Google_Coral_Accelerator_Module" (version 20210126) (generator pcbnew) (layer "F.Cu")
  (tedit 603363DB)
  (attr smd)
  (fp_text reference "REF**" (at 0 -5.65 unlocked) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp a17dfb31-3f50-42c2-adce-9d1cefdb26f9)
  )
  (fp_text value "Google_Coral_Accelerator_Module" (at 0 -3.65 unlocked) (layer "F.Fab")
    (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 11dcdf6e-cdee-43b6-a596-d9946d750702)
  )
  (fp_text user "${REF}" (at 0 -3.25 unlocked) (layer "F.Fab")
    (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 03fd6a4d-7334-4048-8711-460d58f0b64e)
  )
  (fp_arc (start -7.650001 -5.15) (end -7.65 -5.225) (angle -90) (layer "F.SilkS") (width 0.15) (tstamp 0d772260-4f32-4cc2-bd19-549f79991c39))
  (fp_arc (start 7.650001 5.15) (end 7.65 5.225) (angle -90) (layer "F.SilkS") (width 0.15) (tstamp 212a3e37-6042-47f4-8f67-2e60a3ab561e))
  (fp_arc (start 7.65 -5.150001) (end 7.725 -5.15) (angle -90) (layer "F.SilkS") (width 0.15) (tstamp ab462511-48e5-4c55-a871-5c71f259a574))
  (fp_arc (start -7.65 5.150001) (end -7.725 5.15) (angle -90) (layer "F.SilkS") (width 0.15) (tstamp d8115940-f7e8-4333-bc32-2db4029e1657))
  (fp_poly (pts (xy 7.65 5.15)
    (xy 7.65 4)
    (xy 7.8 4)
    (xy 7.8 5.15)
    (xy 7.65 5.3)
    (xy 6.5 5.3)
    (xy 6.5 5.15)) (layer "F.SilkS") (width 0) (fill solid) (tstamp 10ff43fa-096d-4d2f-88f7-9c8249598313))
  (fp_poly (pts (xy -7.65 -5.15)
    (xy -7.65 -4)
    (xy -7.8 -4)
    (xy -7.8 -5.15)
    (xy -7.65 -5.3)
    (xy -6.5 -5.3)
    (xy -6.5 -5.15)) (layer "F.SilkS") (width 0) (fill solid) (tstamp 63dd7e29-a745-411b-bee2-380496314792))
  (fp_poly (pts (xy -7.65 5.15)
    (xy -6.5 5.15)
    (xy -6.5 5.3)
    (xy -7.65 5.3)
    (xy -7.8 5.15)
    (xy -7.8 4)
    (xy -7.65 4)) (layer "F.SilkS") (width 0) (fill solid) (tstamp a605c515-e54f-4b5f-88c5-f649c1484d6f))
  (fp_poly (pts (xy -7.85 -4.5)
    (xy -8.05 -4.35)
    (xy -8.05 -4.65)) (layer "F.SilkS") (width 0) (fill solid) (tstamp d23f1b87-209f-4fd2-9b28-3dba1f4b6da9))
  (fp_poly (pts (xy 7.65 -5.15)
    (xy 6.5 -5.15)
    (xy 6.5 -5.3)
    (xy 7.65 -5.3)
    (xy 7.8 -5.15)
    (xy 7.8 -4)
    (xy 7.65 -4)) (layer "F.SilkS") (width 0) (fill solid) (tstamp f9986c4e-3f8c-4bb5-8ccc-579bea033260))
  (fp_line (start 7.5 -5.15) (end -7.5 -5.15) (layer "F.CrtYd") (width 0.05) (tstamp 1af15e21-1d86-4643-99d5-acd547d0d153))
  (fp_line (start 7.65 5) (end 7.65 -5) (layer "F.CrtYd") (width 0.05) (tstamp 1b289017-fdd7-4f6e-9601-cd0e059395b9))
  (fp_line (start -7.65 -5) (end -7.65 5) (layer "F.CrtYd") (width 0.05) (tstamp 867c2c83-7e35-4c86-b4af-f525d4037fb9))
  (fp_line (start -7.5 5.15) (end 7.5 5.15) (layer "F.CrtYd") (width 0.05) (tstamp f6b6b63c-f627-418c-8162-d4ac037f9fec))
  (fp_arc (start -7.5 -5) (end -7.5 -5.15) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 0a996ce4-5a22-46ab-9ffd-2458470251ac))
  (fp_arc (start 7.5 5) (end 7.5 5.15) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 964d01a0-53c3-45d6-98da-432cda770838))
  (fp_arc (start 7.5 -5) (end 7.65 -5) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 9d2d6e76-2201-4058-ab4e-e1a6f1277326))
  (fp_arc (start -7.5 5) (end -7.65 5) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp a447b870-10be-4869-9aff-6c9c3f902dcb))
  (fp_rect (start -7.5 -5) (end 7.5 5) (layer "F.Fab") (width 0.1) (fill none) (tstamp 4b4ed8a5-ef33-40f3-ac4e-9fdd6750fdcb))
  (pad "1" smd roundrect (at -6.9 -4.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 802dba41-b64c-4914-af1e-5fa9e2621b14))
  (pad "2" smd roundrect (at -6.9 -4) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 26cdab7f-bb3b-44d3-9ceb-3b2422bce41f))
  (pad "3" smd roundrect (at -6.9 -3.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 242e1623-3846-4f14-b85a-c9e2b4d2b4f3))
  (pad "4" smd roundrect (at -6.9 -3) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp fc899aba-0188-44c3-be9a-d334b44d9a78))
  (pad "5" smd roundrect (at -6.9 -2.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 05c461c5-2d77-4da5-ae9e-70518b8919e0))
  (pad "6" smd roundrect (at -6.9 -2) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 97408027-5613-459d-9096-4f22b4a22760))
  (pad "7" smd roundrect (at -6.9 -1.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 4ed687ad-6fe0-4ed4-8cb3-55b0a8596af7))
  (pad "8" smd roundrect (at -6.9 -1) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 49c3989a-ad1b-431f-a1d3-1830405b3f86))
  (pad "9" smd roundrect (at -6.9 -0.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 180d9430-e2d5-4187-ad63-204123715fc4))
  (pad "10" smd roundrect (at -6.9 0) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 14797d8e-4967-4587-b265-26278a7be1c9))
  (pad "11" smd roundrect (at -6.9 0.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 16a93e7c-218d-4e6b-ab6c-2b9b2cc06896))
  (pad "12" smd roundrect (at -6.9 1) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 04347b78-d856-46d3-861e-4e481ec015af))
  (pad "13" smd roundrect (at -6.9 1.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 912e4f20-5d4d-4d8c-80e3-6962ec802d1a))
  (pad "14" smd roundrect (at -6.9 2) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 176f4b06-10bc-4316-a606-ffa6eaf814d1))
  (pad "15" smd roundrect (at -6.9 2.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 4b92f8df-4f50-4689-9606-0da22f65c6fc))
  (pad "16" smd roundrect (at -6.9 3) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 5d552611-b794-4e0b-bb6d-80558619bb45))
  (pad "17" smd roundrect (at -6.9 3.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 07f82963-9236-4a10-99de-90403bf10eb1))
  (pad "18" smd roundrect (at -6.9 4) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 70cf2b5f-bf9b-45ee-82ca-7cdddbd2a5c4))
  (pad "19" smd roundrect (at -6.9 4.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 8e2645ad-db97-41be-b5b5-18c142e01c7c))
  (pad "20" smd roundrect (at -6 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 946af2de-ca7e-453d-adb5-41937aa6cb02))
  (pad "21" smd roundrect (at -5.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp f90feea6-8809-48ff-a8b3-f3384fee9bb1))
  (pad "22" smd roundrect (at -5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp d40cb85a-c27d-4a5c-94a1-df596ede9383))
  (pad "23" smd roundrect (at -4.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp a62bebad-6737-43ce-ac8b-c1be8e93c1a8))
  (pad "24" smd roundrect (at -4 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp afe81753-d49a-4ba7-8a35-a0c8a1e6be7c))
  (pad "25" smd roundrect (at -3.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp c2a5a82f-1178-44c6-ab3a-053c4428f6e6))
  (pad "26" smd roundrect (at -3 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp e136cdac-8965-4b50-8368-3897f0654f15))
  (pad "27" smd roundrect (at -2.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 5f6b9621-7cf4-4afa-9f8a-aabafd65a56b))
  (pad "28" smd roundrect (at -2 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 35ca4931-e11d-4187-b6a0-516c50890fbe))
  (pad "29" smd roundrect (at -1.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 5f1c9780-a391-4ea2-b386-a9c5b13ee4d2))
  (pad "30" smd roundrect (at -1 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 3f334105-3b5b-452b-a3ef-416dc1835de0))
  (pad "31" smd roundrect (at -0.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 1b7e9e79-d6fc-4ebe-b88e-d4b0919f1247))
  (pad "32" smd roundrect (at 0 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 883ab778-0ccd-4cf0-8b83-934ddb90503a))
  (pad "33" smd roundrect (at 0.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 0aa7c7d5-5c0e-4b82-95b2-bfeea049ebc5))
  (pad "34" smd roundrect (at 1 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 71e45627-0699-485a-a3b8-2b7146690a66))
  (pad "35" smd roundrect (at 1.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp b6a9d13f-b466-44b4-8665-4af098be0b9d))
  (pad "36" smd roundrect (at 2 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp be705707-0a95-4b13-b112-edcaaacdb385))
  (pad "37" smd roundrect (at 2.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp ec20da86-6235-4078-9e57-38df20ff3708))
  (pad "38" smd roundrect (at 3 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 593fbaf1-bdff-4e5e-b07e-5cec9aa823d1))
  (pad "39" smd roundrect (at 3.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 2afd1d69-25de-4c2f-9539-1f132549b7ed))
  (pad "40" smd roundrect (at 4 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp e144d4d0-7ead-4601-9cb4-2d337e6debb3))
  (pad "41" smd roundrect (at 4.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 6ea79a04-bdb5-4ee1-8bbe-74202a5d04ea))
  (pad "42" smd roundrect (at 5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp c133734c-ed68-425b-97b1-dfe6be0f7a9f))
  (pad "43" smd roundrect (at 5.5 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp b65c8b66-6ee7-4bce-99cc-70e21148a30b))
  (pad "44" smd roundrect (at 6 4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp f53534aa-b2bf-4747-812f-3f7ccd47fc05))
  (pad "45" smd roundrect (at 6.9 4.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp faaf6f17-503c-4b7c-b5b0-490acd78e9af))
  (pad "46" smd roundrect (at 6.9 4) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 254bb1fd-aeac-4645-8f4c-3445674f7749))
  (pad "47" smd roundrect (at 6.9 3.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 7190f9a3-4ec0-427a-aaff-dc6354f1bf82))
  (pad "48" smd roundrect (at 6.9 3) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp bc36986c-f0eb-4fd9-8784-bec6e94fbb3a))
  (pad "49" smd roundrect (at 6.9 2.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp c07e327a-685b-47ca-a557-8c42644cf34b))
  (pad "50" smd roundrect (at 6.9 2) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 1b0f7aa9-7792-47a2-b25e-5dd636d9f290))
  (pad "51" smd roundrect (at 6.9 1.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 093e93e3-1651-47c9-8165-839883727842))
  (pad "52" smd roundrect (at 6.9 1) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 7caf4904-fa0e-4c08-b4a3-3301669c0026))
  (pad "53" smd roundrect (at 6.9 0.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp f1a10b45-8fa6-4a2f-b94f-e635c6ec3cab))
  (pad "54" smd roundrect (at 6.9 0) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 8a6a18e4-3033-4e91-a1d9-551de071f0af))
  (pad "55" smd roundrect (at 6.9 -0.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 1927ecba-5b25-4fc1-9b77-15bbb733f1b8))
  (pad "56" smd roundrect (at 6.9 -1) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 878aee11-fcec-4106-b104-eba093bdaa57))
  (pad "57" smd roundrect (at 6.9 -1.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp ce7c7c74-9a1a-46fe-91dc-c30e4cb6e460))
  (pad "58" smd roundrect (at 6.9 -2) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 9930f158-0b9f-4b21-8365-8022e5f473cb))
  (pad "59" smd roundrect (at 6.9 -2.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 3edf39aa-e29d-453f-9a70-4d5710631f4a))
  (pad "60" smd roundrect (at 6.9 -3) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 1b085fc5-0330-4d5d-bf64-d2d22224eb5f))
  (pad "61" smd roundrect (at 6.9 -3.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp ea845d5d-f017-45c1-96a6-f9ef80a77c21))
  (pad "62" smd roundrect (at 6.9 -4) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp a519a16e-b333-4ae8-a1fa-53891d155ff1))
  (pad "63" smd roundrect (at 6.9 -4.5) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 89427b74-1bcc-4a2c-9e52-a40d21756a4c))
  (pad "64" smd roundrect (at 6 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 6f0e0ae3-1a07-4d8c-878a-c6b8f8b459d9))
  (pad "65" smd roundrect (at 5.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 368ca922-46fb-427c-87c9-32d57b18f8b7))
  (pad "66" smd roundrect (at 5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp e9d1c3ab-cbfa-48b8-80fa-7bc6f35af937))
  (pad "67" smd roundrect (at 4.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp d2af71e1-c0d2-4287-a7e4-9a2edd4e4ffb))
  (pad "68" smd roundrect (at 4 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp ca0c97b2-7c8a-47e7-b731-719159929910))
  (pad "69" smd roundrect (at 3.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 792f1cb2-2214-40b5-bca9-b8b864990018))
  (pad "70" smd roundrect (at 3 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp c61e7a1a-153a-4e2e-88f4-0bc4733d4de6))
  (pad "71" smd roundrect (at 2.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp bcec7723-f055-4939-a01a-83242853aaf9))
  (pad "72" smd roundrect (at 2 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp b8946658-df36-4a82-9779-661b67805895))
  (pad "73" smd roundrect (at 1.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp b3124d85-8f0e-461c-a724-020f4d43c40a))
  (pad "74" smd roundrect (at 1 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 6be00345-1073-42ca-ad16-c8f20cd68476))
  (pad "75" smd roundrect (at 0.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 9341017a-442a-4339-9dac-a2ff1cf3f5de))
  (pad "76" smd roundrect (at 0 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 8d717347-7d02-4c07-9aa9-ae55a5657101))
  (pad "77" smd roundrect (at -0.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 119e131a-279d-4012-ac5e-ba0fc874d2a4))
  (pad "78" smd roundrect (at -1 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 8bdf6a75-36cd-4b60-bd9d-03f5cddf7d45))
  (pad "79" smd roundrect (at -1.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 43f74b01-4512-46c5-be36-84d755c33573))
  (pad "80" smd roundrect (at -2 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 037bad3f-2d05-4816-8cf2-b983ed2d40d4))
  (pad "81" smd roundrect (at -2.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 83d07881-3ccd-45c5-96a6-5591cd9f5048))
  (pad "82" smd roundrect (at -3 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp a6fad7f4-6f44-4f7c-be70-f0b2e24242fe))
  (pad "83" smd roundrect (at -3.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp e21502cb-eb07-44a1-a73e-878ea6893678))
  (pad "84" smd roundrect (at -4 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 6001f19e-a22f-47fd-a4bf-888362764449))
  (pad "85" smd roundrect (at -4.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp b13f923c-9269-480c-a721-df9418b9aef8))
  (pad "86" smd roundrect (at -5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 70cdd314-974b-43a4-a8dc-65d63e9a8c6e))
  (pad "87" smd roundrect (at -5.5 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp de16c97a-f057-41e5-8c5b-4aec0358bea5))
  (pad "88" smd roundrect (at -6 -4.4 90) (size 0.6 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 886e413c-d15e-42bf-b254-ed5c2cb3f4dd))
  (pad "89" smd roundrect (at -2.4 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 0aa1b77c-0216-4490-a054-8a2bf073d1a4))
  (pad "89" smd roundrect (at 2.4 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 0c0a2ef4-46ad-4ad4-9a14-94a9fd9f5e41))
  (pad "89" smd roundrect (at 2.4 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 1f50f771-2e2e-4672-8a49-5786abd25884))
  (pad "89" smd roundrect (at -5.6 -2.4) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062)
    (chamfer_ratio 0.5) (chamfer top_left) (tstamp 2ae3d4e2-b535-40ef-853c-d123e50522d4))
  (pad "89" smd roundrect (at 5.6 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 2f0a88b3-7343-43ee-a09e-833a73d2af5a))
  (pad "89" smd roundrect (at 0.8 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 3103b8c2-07e9-4633-bd8b-10c39fe14644))
  (pad "89" smd roundrect (at -4 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 3b1ee30d-4028-451c-869f-1133bad0276d))
  (pad "89" smd roundrect (at -0.8 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 3ba6477f-d528-4c34-81fe-6082cc191762))
  (pad "89" smd roundrect (at -2.4 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 4765e1c5-c6fd-4657-b9b4-f24c63f1ce29))
  (pad "89" smd roundrect (at -0.8 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 484ad5c1-6048-4d80-86b3-4a4f51a66543))
  (pad "89" smd roundrect (at -2.4 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 4868049d-c4ec-40fd-8a10-cf2084509cb5))
  (pad "89" smd roundrect (at -4 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 528e5f54-fddd-4697-ad76-fab7df5a9c34))
  (pad "89" smd roundrect (at 2.4 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 5397ef5c-041d-4df7-b2bf-48c597870515))
  (pad "89" smd roundrect (at 2.4 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 5912b9a6-67fc-4103-ad59-54face1708aa))
  (pad "89" smd roundrect (at -0.8 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 6822cf93-f77b-41e8-8866-739832ee41cf))
  (pad "89" smd roundrect (at 4 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 6a543576-f41a-46ba-a09d-33b5873d2758))
  (pad "89" smd roundrect (at -5.6 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 6ae934da-5233-4143-8b3e-6344d54e25ad))
  (pad "89" smd roundrect (at 5.6 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 6b66c2a7-9d57-4fe6-9d4d-f7b20d4910f5))
  (pad "89" smd roundrect (at -4 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 73c6fb19-a36e-4609-9a47-a4088771edfa))
  (pad "89" smd roundrect (at -0.8 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 7fc913a3-1f0c-40ea-afe2-9e74cb3e646c))
  (pad "89" smd roundrect (at 0.8 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 8530b09c-115d-4066-b7e5-9ca1fe7cfd84))
  (pad "89" smd roundrect (at -4 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 8e20b33b-6f7d-4983-8c78-673b6fca5878))
  (pad "89" smd roundrect (at 4 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 9646cafb-512c-4f40-b7f5-cfbb337ab2cc))
  (pad "89" smd roundrect (at 5.6 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp 9d7c2432-3c97-44e4-aaf8-c240283b3509))
  (pad "89" smd roundrect (at 4 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp ae28d0c8-40fc-40c9-9438-13b05d0a3052))
  (pad "89" smd roundrect (at 0.8 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp bbe4bf87-f392-4924-b692-c12ff9d9fd9f))
  (pad "89" smd roundrect (at 0.8 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp bc00f882-4d90-4f81-9cea-7c1df8093126))
  (pad "89" smd roundrect (at -5.6 -0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp c1481eca-5568-4e79-9cff-31d8b8168664))
  (pad "89" smd roundrect (at 4 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp c4f517f2-9090-4f74-b8e6-7369e468484d))
  (pad "89" smd roundrect (at 5.6 -2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp d0528fab-cbe0-4284-a167-26ef46651c33))
  (pad "89" smd roundrect (at -2.4 0.8 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp e1449a5e-d8d5-49b0-b9e9-4fc2b32525cd))
  (pad "89" smd roundrect (at -5.6 2.4 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.062) (tstamp e75410ca-4796-49b1-b706-7366937756de))
  (group "" (id 18bd096f-4cee-43f6-ba1d-29489f3c359b)
    (members
      10ff43fa-096d-4d2f-88f7-9c8249598313
      212a3e37-6042-47f4-8f67-2e60a3ab561e
 )
  )
  (group "" (id 5d813683-41e6-4934-96cb-6950f9f2b1fe)
    (members
      ab462511-48e5-4c55-a871-5c71f259a574
      f9986c4e-3f8c-4bb5-8ccc-579bea033260
 )
  )
  (group "" (id 6b8cef45-726c-4122-afa1-b45c054ec530)
    (members
      0d772260-4f32-4cc2-bd19-549f79991c39
      63dd7e29-a745-411b-bee2-380496314792
 )
  )
  (group "" (id 9a8275a3-c736-484d-9179-3e9cae2adf34)
    (members
      a605c515-e54f-4b5f-88c5-f649c1484d6f
      d8115940-f7e8-4333-bc32-2db4029e1657
 )
  )
  (model "${KICAD7_3DMODEL_DIR}/Module.3dshapes/Google_Coral_Accelerator_Module.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -180))
  )
)
