(module uPSU100 (layer F.Cu) (tedit 585412CC)
  (solder_mask_margin -0.01)
  (fp_text reference A3 (at -8.25 -4.5 180) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value uPSU100 (at -8.25 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start 13 -5) (end 11 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start 13 -3) (end 13 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start 11 -3) (end 13 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start 11 -5) (end 11 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start -13 5) (end -13 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -9 5) (end -13 5) (layer F.SilkS) (width 0.125))
  (fp_line (start -13 -5) (end -9 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -13 -5) (end 13 -5) (layer F.Fab) (width 0.05))
  (fp_line (start 13 -5) (end 13 5) (layer F.Fab) (width 0.05))
  (fp_line (start 13 5) (end -13 5) (layer F.Fab) (width 0.05))
  (fp_line (start -13 5) (end -13 -5) (layer F.Fab) (width 0.05))
  (fp_line (start -13 3) (end -9 3) (layer F.SilkS) (width 0.125))
  (fp_line (start -9 3) (end -9 5) (layer F.SilkS) (width 0.125))
  (fp_line (start -9 3) (end -9 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -9 1) (end -13 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -11 -5) (end -11 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -9 -5) (end -9 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -13 -1) (end -9 -1) (layer F.SilkS) (width 0.125))
  (fp_line (start -13 -3) (end -9 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start -11 3) (end -11 5) (layer F.SilkS) (width 0.125))
  (pad 11 thru_hole roundrect (at 12 -4) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 1 thru_hole roundrect (at -12 -4) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 2 thru_hole roundrect (at -10 -4) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 3 thru_hole roundrect (at -12 -2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 4 thru_hole roundrect (at -10 -2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 5 thru_hole roundrect (at -12 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 6 thru_hole roundrect (at -10 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 7 thru_hole roundrect (at -12 2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 8 thru_hole roundrect (at -10 2) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 9 thru_hole roundrect (at -12 4) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 10 thru_hole roundrect (at -10 4) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (model Module.3dshapes/uPSU_v1.0.0.stp
    (at (xyz -7.244094488188977 4.409448818897638 0.2322834645669292))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model Module.3dshapes/Pin_Header_2x05_2mm.step
    (at (xyz -0.4330708661417323 0.1574803149606299 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
