(footprint "WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "8-Lead Plastic WSON, 2x2mm Body, 0.5mm Pitch, WSON-8, http://www.ti.com/lit/ds/symlink/lm27761.pdf")
  (tags "WSON 8 1EP ThermalVias")
  (property "Sheetfile" "../../library/blocks/17 to 5V 0.25A Buck Converter.kicad_sch")
  (property "Sheetname" "10 to 5V Buck")
  (property "ki_description" "500mA Step-Down Converter with DCS-Control, adjustable output, 3-17V input voltage, WSON-8")
  (property "ki_keywords" "step-down dc-dc buck regulator")
  (attr smd)
  (fp_text reference "U6" (at 0.38 -1.9) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 60368dd3-90b6-4bf9-b5bc-9694a56aad66)
  )
  (fp_text value "TPS62170DSG" (at 0.01 2.14) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 252b20c4-14c5-4eb5-a8cb-d062417b634c)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.7 0.7) (thickness 0.1)))
    (tstamp 735183e7-c320-484c-9b17-ac61352da884)
  )
  (fp_line (start -1.15 -1.12) (end 0.5 -1.12)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fd7193d0-4b84-43e4-af57-f47c63d83224))
  (fp_line (start 0.5 1.12) (end -0.5 1.12)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 96e83b9e-842e-4a18-93ac-26b64b3078cf))
  (fp_line (start -1.350772 -0.825) (end -1.350772 0.826351)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 443ca9d1-0540-440d-b289-a0c8d09abcb1))
  (fp_line (start -1 1.25) (end 1 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8c6026b2-6b33-4663-96ca-9462dd83e489))
  (fp_line (start 0.999228 -1.248649) (end -1 -1.248649)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc88ebe9-3313-4a59-90d1-2e9d4bb3fff2))
  (fp_line (start 1.350772 0.826351) (end 1.35 -0.825)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d9b759a4-b3e1-4480-ad06-00e80c96abb3))
  (fp_arc (start -1.350772 -0.825) (mid -1.323754 -0.925385) (end -1.25 -0.998649)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d32b334-a89d-4d63-99d1-2616638a971d))
  (fp_arc (start -1.25 -0.998649) (mid -1.176777 -1.175426) (end -1 -1.248649)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c4806330-cbd3-4e73-9d31-723dc1961ac4))
  (fp_arc (start -1.25 1) (mid -1.323754 0.926737) (end -1.350772 0.826351)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6c9151fe-1022-49da-aabe-f70f6b486a10))
  (fp_arc (start -1 1.25) (mid -1.176777 1.176777) (end -1.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5abeb08a-cc9c-4354-bdda-46f6321d1da9))
  (fp_arc (start 0.999228 -1.248649) (mid 1.176005 -1.175426) (end 1.249228 -0.998649)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3c0d51e6-9a6b-4b04-a8e4-a4474cfb0ac9))
  (fp_arc (start 1.249228 -0.998649) (mid 1.322982 -0.925386) (end 1.35 -0.825)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c05bce31-5b77-413c-9770-5d6079091374))
  (fp_arc (start 1.25 1) (mid 1.176777 1.176777) (end 1 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp abe980d7-4452-44ee-9c75-7d34ff5c6291))
  (fp_arc (start 1.350772 0.826351) (mid 1.323754 0.926736) (end 1.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4e18d580-3e1c-453a-9daa-648f98f94146))
  (fp_line (start -1 -1) (end 1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec46a0c7-564a-46f0-853b-a0823744f396))
  (fp_line (start -1 1) (end -1 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2503f2c7-dd59-4b61-a030-1f3fbe846972))
  (fp_line (start -0.5 -1) (end -1 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cc42b62a-cad7-489b-9ff6-e988940008ca))
  (fp_line (start 1 -1) (end 1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a4c2e14e-f79a-48e5-9db7-0d2d485c02a4))
  (fp_line (start 1 1) (end -1 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4fbb0afa-7222-4a76-9368-e51e69c43f6d))
  (pad "" smd roundrect (at 0 -0.4) (size 0.75 0.65) (layers "F.Paste") (roundrect_rratio 0.3076923077) (tstamp 862a4b19-fbbf-4f1e-a631-794a1ff9007d))
  (pad "" smd roundrect (at 0 0.4) (size 0.75 0.65) (layers "F.Paste") (roundrect_rratio 0.3076923077) (tstamp f72bafc0-268c-4f95-a17a-98ea1b5027ad))
  (pad "1" smd roundrect (at -0.95 -0.75) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp f7e90090-c8ed-4d66-9a16-a22d815bbf0c))
  (pad "2" smd roundrect (at -0.95 -0.25) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp 3ce426b4-dc1e-4afb-83c2-8d9c96e950c7))
  (pad "3" smd roundrect (at -0.95 0.25) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp 2366d4da-7086-4c79-bf57-c76641a21206))
  (pad "4" smd roundrect (at -0.95 0.75) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp e1c8f4d9-db15-49cd-9abc-442bb5d80e8e))
  (pad "5" smd roundrect (at 0.95 0.75) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp 378feedf-bd25-4b07-9886-3a823b5808ba))
  (pad "6" smd roundrect (at 0.95 0.25) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp 8767e6b1-5cf6-4f58-aa5d-d64d21378b77))
  (pad "7" smd roundrect (at 0.95 -0.25) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp 4457e646-00a9-4167-a4e8-e2cacff054cb))
  (pad "8" smd roundrect (at 0.95 -0.75) (size 0.5 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp 6a2055ff-890e-43f4-8429-ba5f1f6bfaab))
  (pad "9" thru_hole circle (at 0 -0.5) (size 0.5 0.5) (drill 0.25) (layers "*.Cu") (tstamp 55c3ba80-93d8-4a43-aa12-a6526c9f5f60))
  (pad "9" smd roundrect (at 0 0) (size 0.9 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05555555556) (tstamp fe229382-1be5-4bae-8241-a67200536783))
  (pad "9" thru_hole circle (at 0 0.5) (size 0.5 0.5) (drill 0.25) (layers "*.Cu") (tstamp 910dfd02-9ba0-4c90-a46b-1285f35b355f))
  (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
