(footprint "CP_Radial_Laydown_8x20_P3.5" (version 20210424) (generator pcbnew) (layer "F.Cu")
  (tedit 60AFD496)
  (fp_text reference "REF**" (at 0 1.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a4fae145-4a49-4111-8c57-1781c18f239a)
  )
  (fp_text value "CP_Radial_Laydown_8x20_P3.5" (at -3.25 -10.5 90 unlocked) (layer "F.Fab")
    (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp 5cd74c22-e837-4d79-a99a-c08ba34e3b0a)
  )
  (fp_text user "${REF}" (at -0.25 -19.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fa7ca689-850f-41a5-9880-6bac2b05d5c6)
  )
  (fp_rect (start -4 -0.5) (end 4 -20.5) (layer "F.Fab") (width 0.12) (fill none) (tstamp 7e0ed462-d762-4ab9-bcb2-1b59a1c95b2f))
  (pad "1" thru_hole rect (at 1.75 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 5a6ec3df-b076-455b-8748-459187073a5c))
  (pad "2" thru_hole circle (at -1.75 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 084d6c25-58e2-4354-92f6-c95e61228ee6))
  (model "${KICAD7_3DMODEL_DIR}/Capacitor_THT.3dshapes/Capacitor_Polarised_Laydown_8x20.step"
    (offset (xyz 0 0 2))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
