(footprint "JST_SH_SM20B-SRSS-TB_1x20-1MP_P1.00mm_Horizontal" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 60005033)
  (descr "JST SH series connector, SM20B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH top entry")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.98) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d52bcd6e-c952-4336-bf1c-7350f6a73ca7)
  )
  (fp_text value "JST_SH_SM20B-SRSS-TB_1x20-1MP_P1.00mm_Horizontal" (at 0 3.98) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5e9f55dd-f48a-4663-aade-c4fe2aeec1a2)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7b60f8ad-8425-44fa-ba12-6e481de16e44)
  )
  (fp_line (start -11.11 -1.785) (end -10.06 -1.785) (layer "F.SilkS") (width 0.12) (tstamp 7655459e-ba84-458f-a54c-dfda73962407))
  (fp_line (start -9.94 2.685) (end 9.94 2.685) (layer "F.SilkS") (width 0.12) (tstamp bb21f69a-2c40-4ff4-ad3a-e49e8fb48f70))
  (fp_line (start -11.11 0.715) (end -11.11 -1.785) (layer "F.SilkS") (width 0.12) (tstamp c2a4d142-fec0-4cdc-bba3-aef3188b37af))
  (fp_line (start 11.11 -1.785) (end 10.06 -1.785) (layer "F.SilkS") (width 0.12) (tstamp c55f2797-b1ce-46d9-b392-68b85629a7dd))
  (fp_line (start 11.11 0.715) (end 11.11 -1.785) (layer "F.SilkS") (width 0.12) (tstamp e7f6f251-3289-4d98-bda2-97f22143f1f6))
  (fp_line (start -10.06 -1.785) (end -10.06 -2.775) (layer "F.SilkS") (width 0.12) (tstamp e9a05a34-febf-4444-8dea-c9839bec7324))
  (fp_line (start 11.9 3.28) (end 11.9 -3.28) (layer "F.CrtYd") (width 0.05) (tstamp 54302228-153e-4a3c-80e1-836c0bba1040))
  (fp_line (start 11.9 -3.28) (end -11.9 -3.28) (layer "F.CrtYd") (width 0.05) (tstamp 564edc7c-ec84-4c53-86fa-88683c3f0000))
  (fp_line (start -11.9 3.28) (end 11.9 3.28) (layer "F.CrtYd") (width 0.05) (tstamp 8bed8747-d5c8-4745-97de-b35a30ab3476))
  (fp_line (start -11.9 -3.28) (end -11.9 3.28) (layer "F.CrtYd") (width 0.05) (tstamp d4ea025b-22a0-40b6-983f-2c1a38deaa98))
  (fp_line (start -9.5 -0.967893) (end -9 -1.675) (layer "F.Fab") (width 0.1) (tstamp 09e979fc-daef-4f4f-b267-0106ab9e1dcd))
  (fp_line (start -10 -1.675) (end -9.5 -0.967893) (layer "F.Fab") (width 0.1) (tstamp 10ff080f-4e78-419d-9107-774d5090dadd))
  (fp_line (start -11 -1.675) (end -11 2.575) (layer "F.Fab") (width 0.1) (tstamp 4fb9aaaf-9702-4eff-b110-32c07a07b025))
  (fp_line (start 11 -1.675) (end 11 2.575) (layer "F.Fab") (width 0.1) (tstamp 9c9cb7db-959e-4e5a-b5a7-5ec14691b09e))
  (fp_line (start -11 2.575) (end 11 2.575) (layer "F.Fab") (width 0.1) (tstamp b62f42b4-b461-4bfa-adf5-2673dfd24b56))
  (fp_line (start -11 -1.675) (end 11 -1.675) (layer "F.Fab") (width 0.1) (tstamp cf005e8b-a04e-4799-a8c2-ea5e783ebdb8))
  (pad "1" smd roundrect (at -9.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a2dd5d53-9d75-4f8b-ad66-6ba8c3f0b193))
  (pad "2" smd roundrect (at -8.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dc03e30d-454f-4b34-a264-423288e9a42c))
  (pad "3" smd roundrect (at -7.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 677c33aa-3938-49b6-90e6-e2d5771889a4))
  (pad "4" smd roundrect (at -6.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fdb2c50a-932c-4864-ba1c-eeafe009045f))
  (pad "5" smd roundrect (at -5.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8dc40bb9-c0db-4e11-8721-af60d4f85ce5))
  (pad "6" smd roundrect (at -4.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8cbe98d6-e03e-422a-965d-1bcf1db99a86))
  (pad "7" smd roundrect (at -3.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dbfaa450-33ee-4747-846b-6e6dce6241ec))
  (pad "8" smd roundrect (at -2.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 45442a8f-69af-4f42-9abd-9f3f1f45ca85))
  (pad "9" smd roundrect (at -1.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 28a43219-060e-40b1-868b-4c8000f9403c))
  (pad "10" smd roundrect (at -0.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3879d915-c98f-43f6-b0e8-e70c9b226366))
  (pad "11" smd roundrect (at 0.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9c446588-d8cd-4148-8c5c-15b853c15a02))
  (pad "12" smd roundrect (at 1.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp cd6c7d9d-31c6-460a-afcd-d3ed7e5cde52))
  (pad "13" smd roundrect (at 2.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8b09b526-3699-4442-aaf0-b165166e16d1))
  (pad "14" smd roundrect (at 3.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1f7e2d37-44a3-45ea-a060-ea164fd555c0))
  (pad "15" smd roundrect (at 4.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3ac8a112-30c5-437e-9c70-c5ee2aa9b679))
  (pad "16" smd roundrect (at 5.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d004291f-fcd4-42df-b7ad-fba9207acf52))
  (pad "17" smd roundrect (at 6.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 59da82cb-4b34-4af1-9d21-cf523b90fd96))
  (pad "18" smd roundrect (at 7.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4cdf1fa9-188b-4eae-b92f-82e69883e955))
  (pad "19" smd roundrect (at 8.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c5bdb365-30d5-4bf8-9e2d-009a2f482fc0))
  (pad "20" smd roundrect (at 9.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 74427d5e-3432-4977-b5f4-5a1fb382a6e9))
  (pad "MP" smd roundrect (at -10.8 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 54d9d38d-1926-47d0-a051-83e3a08c3508))
  (pad "MP" smd roundrect (at 10.8 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp b5654b97-3da5-4a8d-8955-3cc903e7f0a2))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM20B-SRSS-TB_1x20-1MP_P1.00mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM20B-SRSS-TB.STEP"
    (offset (xyz 0 -0.45 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
