(module Atmel_AT30TS74-UFM1x-T (layer F.Cu) (tedit 5574B7E6)
  (solder_mask_margin 0.01)
  (solder_paste_margin -0.01)
  (attr smd)
  (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Atmel_AT30TS74-UFM1x-T (at 0 1.9) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 1.5) (end -1.5 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -1.5 -1.25) (end -1.45 -1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.75 1.25) (end -1.25 1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.25 1.25) (end -1.25 0.75) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.25 0.75) (end 1.25 1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.25 1.25) (end 0.75 1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.75 -1.25) (end 1.25 -1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.25 -1.25) (end 1.25 -0.75) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.25 -1.25) (end -0.75 -1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start -1.25 -1.25) (end -1.25 -0.75) (layer F.SilkS) (width 0.125))
  (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.05))
  (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.05))
  (fp_line (start -1 1) (end -1 -1) (layer F.Fab) (width 0.05))
  (fp_line (start -1 -1) (end 1 -1) (layer F.Fab) (width 0.05))
  (pad A1 smd circle (at -0.4 -0.4) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0.4 -0.4) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad B1 smd circle (at -0.4 0.4) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd circle (at 0.4 0.4) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask))
)
