(module Program_Pogo_6P_1.25mm (layer F.Cu) (tedit 59D21012)
  (solder_mask_margin 0.001)
  (attr virtual)
  (fp_text reference J2 (at -1.8 0 -270) (layer Cmts.User)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value SWD (at 1.7 0 -270) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user 1 (at 0 -4.325) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 connect rect (at 0 -3.125) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 2 connect oval (at 0 -1.875) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 3 connect oval (at 0 -0.625) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 4 connect oval (at 0 0.625) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 5 connect oval (at 0 1.875) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 6 connect oval (at 0 3.125) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 1 thru_hole circle (at 0 -3.125) (size 1 1) (drill 0.5) (layers *.Cu F.Mask))
  (pad 6 thru_hole circle (at 0 3.125) (size 1 1) (drill 0.5) (layers *.Cu F.Mask))
)
