(footprint "GU14095B-40TR_Ultrasonic_Transceiver" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "PIEZO TRANSCEIVER ULTRASONIC")
  (property "LCSC" "C242186")
  (property "MFG" "INGHAi")
  (property "MPN" "GU14095B-40TR")
  (property "Sheetfile" "../../library/blocks/Ultrasonic Distance Sensor.kicad_sch")
  (property "Sheetname" "Ultrasonic")
  (property "ki_description" "Ultrasonic transducer")
  (property "ki_keywords" "crystal speaker ultrasonic transducer")
  (attr through_hole)
  (fp_text reference "LS2" (at 0 0) (layer "B.SilkS")
      (effects (font (size 0.6 0.6) (thickness 0.127)) (justify mirror))
    (tstamp f8c9c01a-5b8c-4aa3-8e59-b5da2c12ae06)
  )
  (fp_text value "40kHz" (at 0 2.5) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.127)))
    (tstamp 3178358d-ac22-465e-bce9-97e61a819bf5)
  )
  (fp_text user "+" (at 3.5 -1) (layer "B.SilkS")
      (effects (font (size 0.6 0.6) (thickness 0.127)) (justify mirror))
    (tstamp d5b1a7df-2393-4ae1-92ea-7e44d5d3e115)
  )
  (fp_circle (center 0 0) (end 7 0)
    (stroke (width 0.125) (type solid)) (fill none) (layer "F.SilkS") (tstamp 0fa436ee-8c22-481b-86e9-e6e10a578fad))
  (fp_circle (center -2.5 0) (end -1.4 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 1687a0a6-e20f-47cc-a8cc-9ca4058cf1da))
  (fp_circle (center 2.5 0) (end 3.6 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 5654d00d-e538-4627-8fa6-64c91a2fbaba))
  (fp_circle (center 0 0) (end 7.25 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 1bff8bc3-8092-40c7-9110-7bff0437b8a9))
  (fp_circle (center 0 0) (end 7 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fe0d2860-d85a-44a1-8a84-5810758f0934))
  (pad "1" thru_hole circle (at -2.5 0) (size 1.1 1.1) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp eb7f71f3-2567-4bfc-a832-9a9d264b991f))
  (pad "1" connect circle (at -2.5 0) (size 1.8 1.8) (layers "B.Cu" "B.Mask") (tstamp 19d2e1bb-398f-4f88-bfed-4823f68f419c))
  (pad "2" thru_hole circle (at 2.5 0) (size 1.1 1.1) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 2c2a03b2-0471-4215-b430-56304eb889e9))
  (pad "2" connect circle (at 2.5 0) (size 1.8 1.8) (layers "B.Cu" "B.Mask") (tstamp 7b396e97-75ca-47b1-a8e8-6141b5fc42c9))
  (model ":KICAD7_3DMODEL_DIR:Speaker_Transducer.3dshapes/INGHAi GU14095B-40TR.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
