(footprint "Winsen_RDB223_and_lens_Side_Mount" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "LCSC" "C879408")
  (property "MFG" "Winsen")
  (property "MPN" "RDB223")
  (property "Sheetfile" "NightLight.kicad_sch")
  (property "Sheetname" "")
  (attr through_hole)
  (fp_text reference "U5" (at 0 -0.3 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp e71ae456-e3c9-4565-b1b3-04e1fabd9ff2)
  )
  (fp_text value "RDB223" (at 0 0.75 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3f7dc319-5a92-4f7c-b712-61599ab91e5b)
  )
  (fp_text user "BOARD EDGE" (at 4.6 -0.05 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold) (justify right bottom))
    (tstamp 223f3864-07a1-4ca6-bb99-aba1d84833f5)
  )
  (fp_text user "${REFERENCE}" (at 0 2.25 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5919aa9c-1eed-455e-86f4-8e1831195374)
  )
  (fp_line (start -4.55 0) (end 4.55 0)
    (stroke (width 0.05) (type default)) (layer "Dwgs.User") (tstamp 5a11aa01-86da-48f5-adc9-786d84359c48))
  (pad "1" thru_hole roundrect (at -1.8 -2 90) (size 1.3 1.6) (drill 0.7) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333) (tstamp 4ad1448e-108b-42fa-8fbb-da5963ed05aa))
  (pad "2" thru_hole circle (at 1.8 -2) (size 1.3 1.3) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp 5c5b15e6-dcda-4c1b-ae27-e7e4eb98c7f5))
  (pad "3" thru_hole circle (at 1.8 -5.592) (size 1.3 1.3) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp f0da1614-1b75-4a6c-ab5e-1434bee325a4))
  (model ":KICAD7_3DMODEL_DIR:Sensor_Optical.3dshapes/PIR Sensor and Lens.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
