(footprint "CP_Elec_6.3x7.7" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
  (solder_mask_margin -0.05)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference "REF**" (at -3.8 -2.3 90) (layer "F.SilkS")
      (effects (font (size 0.6 0.6) (thickness 0.125)))
    (tstamp 9891d5ae-9927-4fcc-aa8b-8825b4c55ec1)
  )
  (fp_text value "CP_Elec_6.3x7.7" (at -0.05 -3.7) (layer "F.Fab")
      (effects (font (size 0.3 0.3) (thickness 0.075)))
    (tstamp ab752cc1-903c-4484-9934-d03757b33621)
  )
  (fp_text user "+" (at -3.75 1.15) (layer "F.SilkS")
      (effects (font (size 0.6 0.6) (thickness 0.125)))
    (tstamp 574d8ebc-e1cf-4baa-a731-7b2b0a1001be)
  )
  (fp_text user "+" (at -1.73 -0.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d543020f-7038-4a53-86c7-b8466abc762d)
  )
  (fp_line (start -3.3 -2.54) (end -3.3 -1.12)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 0aea65af-332c-4457-8147-8208951f2650))
  (fp_line (start -3.3 -2.54) (end -2.54 -3.3)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp ea8e64bc-ce78-456d-9cae-54de2709330e))
  (fp_line (start -3.3 2.54) (end -3.3 1.12)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp eb6a4238-22fc-4734-9e3e-e415861383e1))
  (fp_line (start -2.54 -3.3) (end 3.3 -3.3)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 26ed526c-964d-4d00-93d0-582fd5ba6b39))
  (fp_line (start -2.54 3.3) (end -3.3 2.54)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 94e232b5-6d69-46ea-9731-93d35452e461))
  (fp_line (start 3.3 -3.3) (end 3.3 -1.12)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp deb9fa3b-17be-424c-b4d7-0ac2f9c7ac5e))
  (fp_line (start 3.3 3.3) (end -2.54 3.3)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 5caaa3ad-2578-490e-bb36-c78a8f8ca178))
  (fp_line (start 3.3 3.3) (end 3.3 1.12)
    (stroke (width 0.125) (type solid)) (layer "F.SilkS") (tstamp 1b439e30-2e33-479b-a5eb-d76286286664))
  (fp_line (start -4.7 -3.4) (end -4.7 3.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7a3c6232-2132-4a4c-bf03-b8ca5b78f77d))
  (fp_line (start -4.7 -3.4) (end 4.7 -3.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9c45853-7990-47a9-8968-4265bc23f5cf))
  (fp_line (start 4.7 3.4) (end -4.7 3.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 028c7991-4610-4476-b5c9-378693b25688))
  (fp_line (start 4.7 3.4) (end 4.7 -3.4)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c7bdaf9d-b44f-4b47-967d-a548823da33d))
  (fp_line (start -3.15 -2.48) (end -3.15 2.48)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp d79bed41-8b00-4717-a4ea-c9137217d763))
  (fp_line (start -3.15 2.48) (end -2.48 3.15)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp d4a6df65-eaf0-478b-96c4-5d7b387f7545))
  (fp_line (start -2.48 -3.15) (end -3.15 -2.48)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp b661982e-fcf4-4f3c-900c-a44fe31fca29))
  (fp_line (start -2.48 3.15) (end 3.15 3.15)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp ea2156bc-4a21-4ea9-9d7d-f8d89698d108))
  (fp_line (start 3.15 -3.15) (end -2.48 -3.15)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp b3aef20b-5a7a-4b37-b92c-b56d32a34b2e))
  (fp_line (start 3.15 3.15) (end 3.15 -3.15)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp f40e73db-cd22-4bf2-abe2-7e2e75d010e8))
  (fp_circle (center 0 0) (end 0 3.15)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.Fab") (tstamp ae45fe46-860d-4b45-96fa-426150e75424))
  (pad "1" smd roundrect (at -2.7 0 180) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 343719c8-fe7d-430a-89a1-f6aacb9e2527))
  (pad "2" smd roundrect (at 2.7 0 180) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bd5fdefb-b089-4de5-9bfe-cf75af930bcb))
  (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
