(footprint "JAE_SIM_Card_SF72S006" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SIM Card, Push-Push, https://www.jae.com/direct/topics/topics_file_download/topics_id=68892&ext_no=06&index=0&_lang=en&v=202003111511468456809")
  (tags "SIM Card with Detect Switch")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Nano-SIM Card (4FF) connector with Detect Switch")
  (property "ki_keywords" "SIM card UICC 4FF")
  (attr smd)
  (fp_text reference "J15" (at 2.667 10.541 180) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4341e791-6242-4f73-86a1-1be80961097a)
  )
  (fp_text value "JAE_SIM_Card_SF72S006" (at -0.98 -6.485 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a55b680a-f8a6-450c-8c81-97a3188a3aa4)
  )
  (fp_text user "PCB edge" (at 4.95 -5.1 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold) (justify left bottom))
    (tstamp 43897709-f088-4cd6-b233-c8dbcdb32797)
  )
  (fp_text user "${REFERENCE}" (at 0 2.54 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3799b48e-7bd0-4403-9547-bfa5c6e8cb41)
  )
  (fp_line (start -6.7945 -4.7625) (end -6.7945 -5.2705)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7ca616e-f0a2-4331-93f3-1cb542a4482a))
  (fp_line (start -6.7945 0.5715) (end -6.7945 -1.524)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 023747cb-ab45-400a-9779-ed80716f9e74))
  (fp_line (start -6.7945 5.461) (end -6.7945 2.815)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f31cd87b-9a63-427e-9520-a11dbd9481bd))
  (fp_line (start -6.7945 9.4615) (end -6.7945 8.1915)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4fd24ea7-f86b-4bfd-b6f0-0cafa7aa1824))
  (fp_line (start -4.0005 9.4615) (end -6.7945 9.4615)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 489fc5f8-e007-41f7-8e5e-a096e6d1fdda))
  (fp_line (start -4.0005 9.4615) (end -4.0005 9.017)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3dbb6fb9-ae48-4512-87e4-53f051ea8f72))
  (fp_line (start -3.048 9.015) (end -4.0005 9.015)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 03c73fd9-d9cc-4bc0-af73-0e8d423a2cc8))
  (fp_line (start 1.397 9.017) (end -1.397 9.015)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4b3f12c2-86dd-4574-8ca2-5f79f78f40a3))
  (fp_line (start 4.82 -5.2705) (end -6.7945 -5.2705)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee065102-d3ed-4810-8a64-d80b5d7faba0))
  (fp_line (start 4.82 -5.2705) (end 4.82 -4.7625)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52868df4-660c-49d9-a694-54a96fcf452c))
  (fp_line (start 4.826 -1.524) (end 4.826 0.5715)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51d277fc-a22d-46b5-9062-01a1486a90cf))
  (fp_line (start 4.826 2.815) (end 4.826 9.015)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2a60a4c0-6185-4c4e-a16a-ba2f052e41e6))
  (fp_line (start 4.826 9.015) (end 3.048 9.015)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a9993462-6c4b-4fc3-877d-6572b4b584e5))
  (fp_line (start -7.85 -5.05) (end 7.65 -5.05)
    (stroke (width 0.05) (type dash)) (layer "Dwgs.User") (tstamp e73d0a16-7c88-4963-b164-06e50d56aff5))
  (fp_line (start -6.98 -5.46) (end -6.98 9.69)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a9765da3-bd54-4e0a-bc18-5836a2701387))
  (fp_line (start -6.98 9.69) (end 5.02 9.69)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4c8edf2f-3f0c-4154-83e5-d32b7a182372))
  (fp_line (start 5.02 -5.46) (end -6.98 -5.46)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 605ad4ca-0fdc-4f6e-8155-3913fb8b6141))
  (fp_line (start 5.02 9.69) (end 5.02 -5.46)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ebcab5c7-ada7-442b-a173-d78d11f45782))
  (fp_line (start -6.58 9.29) (end -6.58 -5.06)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42df5494-8d2f-402c-8dc3-7516f9ea34c8))
  (fp_line (start -4.18 8.84) (end -4.18 9.29)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 282df36a-2245-4ebf-99ec-fb1a1a2ce7e8))
  (fp_line (start -4.18 9.29) (end -6.58 9.29)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81f07340-2d29-451e-a370-8762272be96c))
  (fp_line (start 4.62 -5.06) (end -6.58 -5.06)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 631dbedf-8472-434f-8366-1df16b9b4870))
  (fp_line (start 4.62 -5.06) (end 4.62 8.84)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12e07d69-c97b-4a21-8548-f5335556c4e2))
  (fp_line (start 4.62 8.84) (end -4.18 8.84)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fce5d3b1-caff-48c5-8ad9-d03bdbd86a11))
  (pad "C1" smd rect (at -2.54 -2.46 180) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 28633188-3bcc-40f4-a80b-1345e786b612))
  (pad "C2" smd rect (at 0 -2.46 180) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b3a0bc81-ca3c-4dcd-99c8-7131d3b4b706))
  (pad "C3" smd rect (at 2.54 -2.46 180) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a1c1abd9-72db-41a9-96a6-3fcad82c2ff6))
  (pad "C5" smd rect (at -2.54 0.71 180) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 28b03c3d-fea8-44ff-a8df-e9bc193d168c))
  (pad "C6" smd rect (at 0 0.71 180) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 2fc3f38e-0384-43f4-96e7-15ae2878ce43))
  (pad "C7" smd rect (at 2.54 0.71 180) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 97eaf43d-d6c8-4e13-b040-e9d6b0ee4292))
  (pad "CSW" smd rect (at 4.27 4.04 180) (size 0.7 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 90f3e575-5e7b-4c3c-b59f-e3d38df844d5))
  (pad "DSW" smd rect (at 0.55 7.715 180) (size 1.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c23fcb07-a42f-4f8c-a6e3-5008423380d3))
  (pad "SH" smd rect (at -6.555 -3.16 180) (size 0.45 2.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 18fde1c3-100f-4452-8bdf-66f2f0e3d641))
  (pad "SH" smd rect (at -6.555 1.69 180) (size 0.45 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 95e8ba0e-76a3-40d7-bac6-3ecbf8bc0e2f))
  (pad "SH" smd rect (at -6.555 6.84 180) (size 0.45 2.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 13f1fe18-079d-401e-8b54-0ae17853fbfb))
  (pad "SH" smd rect (at -2.2 8.79 180) (size 1.4 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7aaa1d19-da00-4ded-bddb-cc0e89166476))
  (pad "SH" smd rect (at -1.22 -4.31 180) (size 0.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ad906c94-d185-403c-be36-75dce9c6e2b9))
  (pad "SH" smd rect (at 1.22 -4.31 180) (size 0.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 296bc66a-cd07-4440-8a08-c736174a524f))
  (pad "SH" smd rect (at 2.22 8.79 180) (size 1.4 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 3ab9186a-ee23-4096-a00c-54b5fd0dcc6c))
  (pad "SH" smd rect (at 4.095 5.84 180) (size 0.75 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 561fca7b-5a54-4b70-a78e-3a3dc37a5adf))
  (pad "SH" smd rect (at 4.595 -3.16 180) (size 0.45 2.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 7f8edef7-1990-479a-86a1-09fa48ac61e5))
  (pad "SH" smd rect (at 4.595 1.69 180) (size 0.45 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp baa2d02d-f64e-439c-8e98-efdfca5b1feb))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JAE.3dshapes/JAE_SIM_Card_SF72S006.wrl" hide
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_Card.3dshapes/K3D-SF72S006VBD-V1_JAE_Proprietary.STEP"
    (offset (xyz 0 -6.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
