(footprint "Arducam PY064W" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "RK3588_Camcorder_Carrier.kicad_sch")
  (property "Sheetname" "")
  (fp_text reference "A2" (at 0 7.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f85160a1-d5e7-4aba-a7a9-b3b4229e2dd1)
  )
  (fp_text value "~" (at 0 -5.75 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 39891c76-c146-40d9-b7c6-bedd5280b1ef)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.25 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c49696e7-719f-4644-842b-8f8a3019ccf1)
  )
  (fp_line (start -6.25 8.25) (end -6.5 8)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 71a85f67-2397-4830-ab9d-08bf18665930))
  (fp_line (start -6 8) (end -6 8.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp cf2be580-95bb-4d60-89b0-acfa0efb0a44))
  (fp_line (start -6 8.25) (end -6.25 8.25)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7b822767-7bdd-432d-97dd-2573da280528))
  (fp_line (start -6 8.25) (end -5.75 8.25)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 644af51f-c0bf-4d70-bca1-56cdd29c840e))
  (fp_line (start -6 8.5) (end -6.25 9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e719d6d1-46a1-4104-8527-238c30da426e))
  (fp_line (start -6 8.5) (end -5.75 9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6a913b80-6eba-4297-b346-2daa17ee06b9))
  (fp_arc (start -6.775 -6.7) (mid -6.753033 -6.753033) (end -6.7 -6.775)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp b0496579-83ec-4761-845e-e1dd01317b96))
  (fp_arc (start -6.7 6.775) (mid -6.753033 6.753033) (end -6.775 6.7)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 6c76a09e-3c19-4fce-a8ac-a3f37e0a45ac))
  (fp_arc (start 6.7 -6.775) (mid 6.753033 -6.753033) (end 6.775 -6.7)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 1c2208e5-33ae-4f4f-b907-170429f54425))
  (fp_arc (start 6.775 6.7) (mid 6.753033 6.753033) (end 6.7 6.775)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 0e013900-ffb7-4901-b33c-ff2435bc7c36))
  (fp_circle (center -6 7.75) (end -6 7.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 0bbb8ae3-7c4f-440a-a085-7925f6ba5b31))
  (fp_poly
    (pts
      (xy -6.7 5.7)
      (xy -6.7 6.7)
      (xy -5.7 6.7)
      (xy -5.7 6.85)
      (xy -6.7 6.85)
      (xy -6.85 6.7)
      (xy -6.85 5.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp fffa203b-cf00-433a-909a-ae28b5cb9eb8))
  (fp_poly
    (pts
      (xy -5.7 -6.7)
      (xy -6.7 -6.7)
      (xy -6.7 -5.7)
      (xy -6.85 -5.7)
      (xy -6.85 -6.7)
      (xy -6.7 -6.85)
      (xy -5.7 -6.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 38c6b5fa-6d02-4f85-b574-80873ddd168a))
  (fp_poly
    (pts
      (xy 5.7 6.7)
      (xy 6.7 6.7)
      (xy 6.7 5.7)
      (xy 6.85 5.7)
      (xy 6.85 6.7)
      (xy 6.7 6.85)
      (xy 5.7 6.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 96188e70-d2a8-44b0-8802-666ee4f561a7))
  (fp_poly
    (pts
      (xy 6.7 -5.7)
      (xy 6.7 -6.7)
      (xy 5.7 -6.7)
      (xy 5.7 -6.85)
      (xy 6.7 -6.85)
      (xy 6.85 -6.7)
      (xy 6.85 -5.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp cd106ae1-91c3-482c-9f5c-055aa6a62407))
  (fp_line (start -9 2.25) (end -7.1 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d377e61b-ba4e-4b6d-802f-d70bec951a1f))
  (fp_line (start -7.1 -6.6) (end -7.1 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d3e9d8cf-44d9-4193-b1c7-192fbc92f321))
  (fp_line (start -7.1 -2.25) (end -9 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 13239ef1-14be-46fc-ba50-2c7e32983cb9))
  (fp_line (start -7.1 2.25) (end -7.1 6.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8b7ea2fd-966f-4683-ad49-c2da3ebc6edb))
  (fp_line (start -6.6 7.1) (end 6.6 7.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fd429bcc-9264-4171-b0f0-f6dc0d5b0d58))
  (fp_line (start 6.6 -7.1) (end -6.6 -7.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0d65fb40-3360-4ce0-9f7d-453a357c5c84))
  (fp_line (start 7.1 -2.25) (end 7.1 -6.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80616b44-5a5c-46c9-8b2f-3521bcb244c5))
  (fp_line (start 7.1 2.25) (end 9 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8bee93ad-0d09-4637-89fa-e0c52b8f27c4))
  (fp_line (start 7.1 6.6) (end 7.1 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3f5ada15-529d-4f1b-bd4a-b6e341d18359))
  (fp_line (start 9 -2.25) (end 7.1 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4a90a1cc-dcf3-4615-9db7-8791c83c5786))
  (fp_arc (start -9 2.25) (mid -11.25 0) (end -9 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3c443b52-f436-425c-b5ec-a3f976848adc))
  (fp_arc (start -7.1 -6.6) (mid -6.953553 -6.953553) (end -6.6 -7.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 094dd9e4-7811-473b-a295-a862d2e30faf))
  (fp_arc (start -6.6 7.1) (mid -6.953553 6.953553) (end -7.1 6.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1879c305-5aff-4123-80bb-c69ec89e8bad))
  (fp_arc (start 6.6 -7.1) (mid 6.953553 -6.953553) (end 7.1 -6.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 76a5eb37-50b8-485b-a95e-e85212d21759))
  (fp_arc (start 7.1 6.6) (mid 6.953553 6.953553) (end 6.6 7.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e457aa53-2b2a-4e38-95da-3f0f1734033a))
  (fp_arc (start 9 -2.25) (mid 11.25 0) (end 9 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0a04bf79-3617-4b34-b6c8-19d0b0042445))
  (fp_line (start -9 -2) (end -6.6 -2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0a0e83f1-3c9c-4aad-a5fb-101119559811))
  (fp_line (start -9 2) (end -6.6 2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 06114cee-9b84-48d2-9416-6de1843e0a50))
  (fp_line (start -5.1 6.6) (end -5.1 13)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 6e63ed68-3f43-475e-86b7-fc07cdd26299))
  (fp_line (start -5.1 10) (end 5.1 10)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 08113dce-8b59-4065-b94b-3128532ae6b8))
  (fp_line (start -5.1 13) (end 5.1 13)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3f8c138f-fdaa-4130-99d0-8a71ef17b6ac))
  (fp_line (start 5.1 13) (end 5.1 6.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 1c115a96-3089-4fe2-a908-2fe27703e96b))
  (fp_line (start 9 -2) (end 6.6 -2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp ae56e62a-42a5-4497-a039-52cbf49e54fa))
  (fp_line (start 9 2) (end 6.6 2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 5c31e3c6-64c5-4292-aa09-0bd276107b00))
  (fp_rect (start -6.6 -6.6) (end 6.6 6.6)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp cf4fc06f-64a8-40df-aa75-e878ee7a674a))
  (fp_arc (start -9 2) (mid -11 0) (end -9 -2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp eef6d8cc-b248-49dc-a9f3-be913347e7ae))
  (fp_arc (start 9 -2) (mid 11 0) (end 9 2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 9251cedb-7f25-46c7-8181-806876a25a64))
  (fp_circle (center -9 0) (end -8.25 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp b82d5892-5091-4e0d-9238-45aefa9b74b1))
  (fp_circle (center -9 0) (end -8 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 8e48dd94-147f-4b6a-a743-480aa6fe9a22))
  (fp_circle (center 0 0) (end 7 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp bbe9862d-18cb-4845-a70e-9cba358cbe1e))
  (fp_circle (center 9 0) (end 9.75 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 30b2604e-ccef-4347-a502-8727b50ea518))
  (fp_circle (center 9 0) (end 10 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp badbe7d4-0ed1-4291-9fc8-f130a809773c))
  (pad "MP" thru_hole circle (at -9 0) (size 4 4) (drill 2) (layers *.Cu *.Mask) (tstamp 5ac946bf-6169-4469-b20d-0b96bc22f090))
  (pad "MP" thru_hole circle (at 9 0) (size 4 4) (drill 2) (layers *.Cu *.Mask) (tstamp e86386c7-4540-4cfe-bb44-0e7c57f87af1))
  (model ":KICAD6_3DMODEL_DIR:Module.3dshapes/Camera Module [Arducam PY064W].STEP"
    (offset (xyz 0 0 0.66))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
