(module "2P_Castellated_16mm2" (layer F.Cu) (tedit 5D135DDB)
  (attr virtual)
  (fp_text reference "REF**" (at 7.25 0 270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "2P_Castellated_16mm2" (at -2.75 0 270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.05)))
  )
  (fp_line (start 0 -7.5) (end 0 7.5) (layer Dwgs.User) (width 0.12))
  (pad "1" thru_hole oval (at 2.3 -3.25) (size 8.3 6) (drill oval 6.9 4.6) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 2.3 3.25) (size 8.3 6) (drill oval 6.9 4.6) (layers *.Cu *.Mask))
)
