(module "D_5W_P5.08mm_Vertical_AnodeUp_AK" (layer F.Cu) (tedit 5D24928C)
  (descr "Diode, 5W series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
  (tags "Diode 5W series Axial Vertical pin pitch 5.08mm  length 8.9mm diameter 3.7mm")
  (fp_text reference "D2" (at 2.54 -3.174899) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "2A" (at 2.54 3.174899) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 1.85 0) (layer F.Fab) (width 0.1))
  (fp_circle (center 0 0) (end 2.174899 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 0) (end 5.08 0) (layer F.Fab) (width 0.1))
  (fp_line (start 2.174899 0) (end 3.38 0) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.1 -2.1) (end -2.1 2.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.1 2.1) (end 6.73 2.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.73 2.1) (end 6.73 -2.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.73 -2.1) (end -2.1 -2.1) (layer F.CrtYd) (width 0.05))
  (fp_text user "%R" (at 2.54 -3.174899) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "A" (at 2.98 1.4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "A" (at 2.98 1.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "K" thru_hole oval (at 5.08 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask))
  (pad "A" thru_hole rect (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask))
  (model "${KICAD7_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P5.08mm_Vertical_AnodeUp.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
