(footprint "JST_SHD_SM50B-SRDS-G-TF_2x25_P1.0_Right_Angle" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Field2" "")
  (property "Sheetfile" "Flight Controller.kicad_sch")
  (property "Sheetname" "Flight Controller")
  (property "ki_description" "Generic connectable mounting pin connector, double row, 02x25, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J29" (at -15.025 0 -90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp ebe9919f-1bc1-470a-9c6e-b9754e3116ef)
  )
  (fp_text value "GPIO_A" (at 0 4.3 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp a7309c94-352b-44db-821a-75425e3dbaa2)
  )
  (fp_text user "${REF}" (at 0 -1.325 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6e93ec64-f0a1-4d56-ab08-a2ddf73c8655)
  )
  (fp_poly
    (pts
      (xy 12 -3.7)
      (xy 11.85 -3.95)
      (xy 12.15 -3.95)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8d32b7e4-3fca-4ff6-9ff7-75acb801d697))
  (fp_poly
    (pts
      (xy -12.45 2.85)
      (xy -13.1 2.85)
      (xy -13.1 2.7)
      (xy -12.45 2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5977496c-5331-4292-bea4-95b8316d5b3e))
  (fp_poly
    (pts
      (xy 13.1 2.85)
      (xy 12.45 2.85)
      (xy 12.45 2.7)
      (xy 13.1 2.7)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 526fa9cb-06e1-4780-b155-a304e94b40d6))
  (fp_poly
    (pts
      (xy -14.35 2.85)
      (xy -14.2 2.85)
      (xy -14.2 -2.7)
      (xy -12.45 -2.7)
      (xy -12.45 -2.85)
      (xy -14.35 -2.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5b7a449f-b1df-4294-b7fe-f1152b4426f0))
  (fp_poly
    (pts
      (xy 14.35 2.85)
      (xy 14.2 2.85)
      (xy 14.2 -2.7)
      (xy 12.45 -2.7)
      (xy 12.45 -2.85)
      (xy 14.35 -2.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 792d48e3-ee5e-4bc7-b1f2-199a070b51c7))
  (fp_line (start -14.25 2.65) (end -14.25 -2.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d1bbe8e4-8100-4d97-9dd1-36390e1b7199))
  (fp_line (start -14 2.9) (end -12.45 2.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e60e611c-e689-4a25-aa66-120dca9a8e02))
  (fp_line (start -12.45 -3.45) (end -12.45 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 42fa0697-700e-4386-9f7f-60c70766e56d))
  (fp_line (start -12.45 -2.7) (end -14.1 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c0ff32fd-7ddf-4ce9-922e-c5ad39bbcbc7))
  (fp_line (start -12.45 2.9) (end -12.45 3.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 98d2c107-0f41-4a8c-aa43-043a4406ad14))
  (fp_line (start -12.1 -3.8) (end 12.1 -3.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 31a5b74c-25f8-41ee-b121-e2a02d21bb39))
  (fp_line (start -12.1 3.8) (end 12.1 3.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa611f5d-fae5-47d2-b709-0b6897ae3a5c))
  (fp_line (start 12.45 -2.7) (end 12.45 -3.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d66ad04b-f6f7-4390-b8e7-fe3ccef439b7))
  (fp_line (start 12.45 2.9) (end 14 2.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 030b8ece-f446-49ba-8a0a-978aa74357d2))
  (fp_line (start 12.45 3.45) (end 12.45 2.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 245a56b4-95ba-4358-a15c-7bb710ba7198))
  (fp_line (start 14.1 -2.7) (end 12.45 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 965d6339-350f-40d6-b88d-eb6fb2382cd2))
  (fp_line (start 14.25 2.65) (end 14.25 -2.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4a286a96-215a-41ff-a1c3-22d254434f4d))
  (fp_arc (start -14.25 -2.55) (mid -14.206066 -2.656066) (end -14.1 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5cc8efbb-2f7e-45d4-93ab-d156a820fa68))
  (fp_arc (start -14 2.9) (mid -14.176777 2.826777) (end -14.25 2.65)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 68c51eb1-8059-422c-9498-38c470d774eb))
  (fp_arc (start -12.45 -3.45) (mid -12.347487 -3.697487) (end -12.1 -3.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bff851e5-c303-4744-9af3-be7dc7357767))
  (fp_arc (start -12.1 3.8) (mid -12.347487 3.697487) (end -12.45 3.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cf12c0f1-67fb-41c3-b023-4ad231b70396))
  (fp_arc (start 12.1 -3.8) (mid 12.347487 -3.697487) (end 12.45 -3.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c21db0cb-9b8b-48fc-8756-b8461839d131))
  (fp_arc (start 12.45 3.45) (mid 12.347487 3.697487) (end 12.1 3.8)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a411b049-a498-4dea-83d1-9c358ec6ea78))
  (fp_arc (start 14.1 -2.7) (mid 14.206066 -2.656066) (end 14.25 -2.55)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 56439784-586a-46df-87a9-1585a481f2ec))
  (fp_arc (start 14.25 2.65) (mid 14.176777 2.826777) (end 14 2.9)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a64a46e3-d6cf-45ee-9c0c-fd369af45d79))
  (fp_line (start -14.05 2.8) (end -14.05 3.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba4cf137-1187-4f07-b3c6-29b1b1674f15))
  (fp_line (start -14.05 3.3) (end -14.05 3.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5924016b-d4ce-44f1-98fa-1381d10adf4a))
  (fp_line (start -14.05 3.8) (end -14.05 4.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 419ecc19-6969-41ea-bc3c-4cf4edba6992))
  (fp_line (start -14.05 4.3) (end -14.05 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c918bba0-4717-4cab-bae3-9ee380093606))
  (fp_line (start -14.05 4.55) (end -13.8 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1604dab3-4c85-4295-838c-bc84ccd65d00))
  (fp_line (start -13.5 4.55) (end -13.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d134629e-b502-4fff-9b34-570be7b414d3))
  (fp_line (start -13 4.55) (end -12.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15d6f9ab-6ed5-428c-8ec4-54b4bd103013))
  (fp_line (start -12.5 4.55) (end -12.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eb40da30-cbdc-4ece-a7e8-4d5abccc3e88))
  (fp_line (start -12 4.55) (end -11.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f452515b-2a9c-4d82-896c-28c3a2ddd6fa))
  (fp_line (start -11.5 4.55) (end -11.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9615b360-5787-41a7-9c5b-4cf872689658))
  (fp_line (start -11 4.55) (end -10.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d671cc89-a6d2-4aa1-91c3-a1b05f66700a))
  (fp_line (start -10.5 4.55) (end -10.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b45733f-7615-4fba-9a76-77f18ac85ba1))
  (fp_line (start -10 4.55) (end -9.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 147e35e1-5568-4fa7-8122-80f78e2fea87))
  (fp_line (start -9.5 4.55) (end -9.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2369d3d8-bc35-4f3d-96c8-b76ba1162af3))
  (fp_line (start -9 4.55) (end -8.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60ea8677-e7ea-4356-a447-7a821172cf93))
  (fp_line (start -8.5 4.55) (end -8.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 20d6a71b-e9ca-4ac0-a446-7c827e02d934))
  (fp_line (start -8 4.55) (end -7.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b32212c5-8dea-43c1-b8c7-21d40c27bc87))
  (fp_line (start -7.5 4.55) (end -7.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 47e4968d-dc46-4df6-b3b3-10602e84b322))
  (fp_line (start -7 4.55) (end -6.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cea509f9-4987-4a75-ae86-88587422903e))
  (fp_line (start -6.5 4.55) (end -6.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f202c4ff-9fed-45ee-9bc4-1ed4a282d2f4))
  (fp_line (start -6 4.55) (end -5.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcae4860-7bba-40e1-b6ba-5d599a59af98))
  (fp_line (start -5.5 4.55) (end -5.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec1f16cd-e78e-4258-bfa9-1564e9423c24))
  (fp_line (start -5 4.55) (end -4.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0aeb7ffc-0b54-46b4-a51f-be97f8301cbf))
  (fp_line (start -4.5 4.55) (end -4.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f85ca7f4-0a98-48ea-8053-7d596972ec00))
  (fp_line (start -4 4.55) (end -3.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db0f1ff3-5a52-42a2-834d-344d505827c9))
  (fp_line (start -3.5 4.55) (end -3.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 684415f1-8f37-435c-86c1-f13ce3ef1cf3))
  (fp_line (start -3 4.55) (end -2.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2f3b95c4-ba83-43ca-9566-8fa888f941db))
  (fp_line (start -2.5 4.55) (end -2.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76c8bf99-ef14-46b9-81a4-7897b00d22a4))
  (fp_line (start -2 4.55) (end -1.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48a3df52-e620-4418-b56a-cad69f4cb6f3))
  (fp_line (start -1.5 4.55) (end -1.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5fab4969-9e49-46da-a383-4ebdf7f04967))
  (fp_line (start -1 4.55) (end -0.75 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6a0501d6-a6d5-4b81-9c06-6848a388f658))
  (fp_line (start -0.5 4.55) (end -0.25 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed4528aa-ed9d-4bd9-91ef-2cc6228faacc))
  (fp_line (start 0.25 4.55) (end 0.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9b12667-e6a7-481d-b048-e1d4221ef773))
  (fp_line (start 0.75 4.55) (end 1 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8c1a73d-f442-49af-8280-7911f37671a5))
  (fp_line (start 1.25 4.55) (end 1.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12f4936a-9cf6-43c2-b7cd-3cbdec0776f0))
  (fp_line (start 1.75 4.55) (end 2 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1c4be09-5cf1-495f-9a78-d06d5cc917cb))
  (fp_line (start 2.25 4.55) (end 2.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7fb54301-ae0d-4dd8-bd37-4d55dd50830c))
  (fp_line (start 2.75 4.55) (end 3 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f0b9265b-b85e-4820-8d40-14f49608ff40))
  (fp_line (start 3.25 4.55) (end 3.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bee7cb4e-c3b3-4786-b7b1-04e36b565dc4))
  (fp_line (start 3.75 4.55) (end 4 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 851e6ef4-b54b-4190-9845-0bb9c451f9c6))
  (fp_line (start 4.25 4.55) (end 4.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43ca1a37-6faf-4823-8de3-8f49f3bb14cf))
  (fp_line (start 4.75 4.55) (end 5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eff16f5b-0307-42c6-b298-5e5f1d357027))
  (fp_line (start 5.25 4.55) (end 5.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9210c3e0-7533-45ee-b738-f47e0c779c51))
  (fp_line (start 5.75 4.55) (end 6 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aab6660b-a0c7-4138-a6dc-3288def224fe))
  (fp_line (start 6.25 4.55) (end 6.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2272e14d-38f4-46a2-9edd-394dd872a7e5))
  (fp_line (start 6.75 4.55) (end 7 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 904edcf5-462e-4a47-a7a0-cbf5921ff236))
  (fp_line (start 7.25 4.55) (end 7.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b190e283-bd61-4674-88b9-51af12b6bede))
  (fp_line (start 7.75 4.55) (end 8 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69118cde-1b5d-4cd0-a565-2e0e5e655bfa))
  (fp_line (start 8.25 4.55) (end 8.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7e9e636b-c2b8-4735-a6bd-dd1f1634f603))
  (fp_line (start 8.75 4.55) (end 9 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48bf1c27-0ffd-47c6-a4c4-81014deba63c))
  (fp_line (start 9.25 4.55) (end 9.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3054825e-6e6e-4bc9-9a3a-8b6c23c44abb))
  (fp_line (start 9.75 4.55) (end 10 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6cfb1005-38ab-4ec1-8ad3-8340f8755b22))
  (fp_line (start 10.25 4.55) (end 10.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2bae91f-21bb-4a69-85fc-1120b0fed0f3))
  (fp_line (start 10.75 4.55) (end 11 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9cf37c61-591a-4f6e-9f5d-b5cc406b21a6))
  (fp_line (start 11.25 4.55) (end 11.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5af770b1-a6ac-481c-b619-8fc3954b1d93))
  (fp_line (start 11.75 4.55) (end 12 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d99e7200-139b-44e1-aa7d-34addddaa1d8))
  (fp_line (start 12.25 4.55) (end 12.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9bd35bc4-ff9f-47ff-92b6-2fd0a4c516a4))
  (fp_line (start 12.75 4.55) (end 13 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c85214e3-98a3-4948-b6d8-3a6a44ebca66))
  (fp_line (start 13.25 4.55) (end 13.5 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e43c79df-5aa6-4171-b419-abc607161f6d))
  (fp_line (start 14.05 2.8) (end 14.05 3.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ce43c53-7cf6-4867-9c55-5369b19a3348))
  (fp_line (start 14.05 3.3) (end 14.05 3.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5588b9f4-3f94-44ec-86ba-7d968347d8e7))
  (fp_line (start 14.05 3.8) (end 14.05 4.05)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffc2f24e-13e4-4670-9c56-4ec99027cbb4))
  (fp_line (start 14.05 4.3) (end 14.05 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa82295e-9a81-42d8-9ba5-c6d31c1d3501))
  (fp_line (start 14.05 4.55) (end 13.8 4.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 862b12ba-c41e-4a59-b07e-91634a7a4622))
  (fp_rect (start -14.05 2.55) (end 14.05 -2.55)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp bc381907-951f-4fd8-a071-674d92976a20))
  (pad "1" smd roundrect (at 12 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d624226b-bd22-4a26-9bc8-0b2a99b4e76b))
  (pad "2" smd roundrect (at 12 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 28747b0b-a86d-43b6-9f90-2037c729231c))
  (pad "3" smd roundrect (at 11 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp bded7c2f-8070-4276-88ca-c50ced9e64fa))
  (pad "4" smd roundrect (at 11 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 5c0eca7c-3406-498f-a77b-4c9842418c45))
  (pad "5" smd roundrect (at 10 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 1e42e9b3-4279-4db2-89de-f9d6603cd3c2))
  (pad "6" smd roundrect (at 10 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 78bd0565-89b7-416f-8e65-63a0a96ad97c))
  (pad "7" smd roundrect (at 9 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp cf31b15e-5888-44cc-a56c-4b6a15e16c94))
  (pad "8" smd roundrect (at 9 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 3ff075ed-394b-463d-ac25-89887bb5c91d))
  (pad "9" smd roundrect (at 8 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 85526c75-e8b3-4934-a48b-c493e365e915))
  (pad "10" smd roundrect (at 8 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d2c67cba-8a8c-462d-94ba-bd74b1fd7409))
  (pad "11" smd roundrect (at 7 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 569c45d1-bf0f-4126-b984-87338674d3c2))
  (pad "12" smd roundrect (at 7 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp da2f1c8f-1743-472c-9a44-49df5088f7e3))
  (pad "13" smd roundrect (at 6 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 0c4583f2-cddf-4a1e-80db-66fe8edccaa4))
  (pad "14" smd roundrect (at 6 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 3d0e1c77-6692-4862-ba73-60318e190f2f))
  (pad "15" smd roundrect (at 5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 82d79232-a631-4b8a-893c-f453d65397c0))
  (pad "16" smd roundrect (at 5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 8c21c8fe-a9d5-4525-81d5-63a088cf681c))
  (pad "17" smd roundrect (at 4 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 33a027ad-9f93-4ee2-b20c-1dc7236a3390))
  (pad "18" smd roundrect (at 4 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 425ffd56-bb60-44aa-9b1d-22e7fba21161))
  (pad "19" smd roundrect (at 3 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 78ddf4e4-de16-486e-aca7-7b2d03218210))
  (pad "20" smd roundrect (at 3 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp cf8005b4-7fef-4060-9b5d-b6a43eb794ab))
  (pad "21" smd roundrect (at 2 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp c543e9e6-e79a-44ba-adae-1be32758c27b))
  (pad "22" smd roundrect (at 2 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d6ce2f1a-efb8-4e0d-b7f0-ef4b2b0e547c))
  (pad "23" smd roundrect (at 1 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 66d885df-d56b-444c-8ced-d09278503e25))
  (pad "24" smd roundrect (at 1 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp da19b190-9e4d-4619-825c-301956b518f3))
  (pad "25" smd roundrect (at 0 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f4485a62-5c04-4abb-919b-13333105bed5))
  (pad "26" smd roundrect (at 0 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp b4175368-4472-4ba9-9a2c-23e97b0af74e))
  (pad "27" smd roundrect (at -1 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 03ab8f6d-ac46-479f-982f-551107ddf6b3))
  (pad "28" smd roundrect (at -1 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 10923155-b1a1-4914-9f98-bf3ee3fd8e00))
  (pad "29" smd roundrect (at -2 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp bf4abe38-6583-4f94-85e2-f23744f1f051))
  (pad "30" smd roundrect (at -2 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 831b26f8-3f6e-4c07-974b-3775a5273898))
  (pad "31" smd roundrect (at -3 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp ff31a4a2-256b-4199-81b6-6a0b8d5e34bf))
  (pad "32" smd roundrect (at -3 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 31504e5c-8a57-4c6d-bd14-3782b79a11cb))
  (pad "33" smd roundrect (at -4 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp d52996f7-b6e2-410a-8b58-e441a2aa19b7))
  (pad "34" smd roundrect (at -4 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp c6c78879-ed29-48ea-866a-1ea79ee6e4cc))
  (pad "35" smd roundrect (at -5 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 613d1d19-1f4e-4c47-9839-6124110e7162))
  (pad "36" smd roundrect (at -5 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 54a3e87a-aeda-4052-adb5-d9a9692bed77))
  (pad "37" smd roundrect (at -6 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp ffa23018-ecec-4fa9-a261-7fc259abd634))
  (pad "38" smd roundrect (at -6 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp ed85f054-589c-4d68-878f-c8af887fef08))
  (pad "39" smd roundrect (at -7 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp ee58b982-5bd0-4993-a687-251840217c37))
  (pad "40" smd roundrect (at -7 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f9169513-bda1-4f64-abcb-902ab6980420))
  (pad "41" smd roundrect (at -8 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp f4ce7431-5c7c-4615-bcbc-f954e17661eb))
  (pad "42" smd roundrect (at -8 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 0c368f0c-9309-43a3-b112-b4e204254787))
  (pad "43" smd roundrect (at -9 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 1aa8b8cc-cba1-4b4c-951d-3eddeaa5b069))
  (pad "44" smd roundrect (at -9 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 81d502b8-0675-4c14-b1cb-025939082b13))
  (pad "45" smd roundrect (at -10 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 6bc0ccc3-0d42-4b4a-8434-fd83bd6e9c57))
  (pad "46" smd roundrect (at -10 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 6db649a1-3e24-4894-81b7-3280aea38018))
  (pad "47" smd roundrect (at -11 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 9eeb6574-1cae-46db-b84c-11e87e5d9968))
  (pad "48" smd roundrect (at -11 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 7a2afe2c-f7fc-4d47-b7fe-6b292425a9d4))
  (pad "49" smd roundrect (at -12 -2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 2fc5f3f4-38ed-4260-81e1-42ad30cf5834))
  (pad "50" smd roundrect (at -12 2.85) (size 0.6 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.333) (tstamp 9e97cd1c-56cd-4859-bfe6-c0cc5a29a0c1))
  (pad "MP" smd roundrect (at -13.675 1.85) (size 0.85 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.118) (tstamp 9dbf542a-c6dd-4331-b334-755371661b8c))
  (pad "MP" smd roundrect (at 13.675 1.85) (size 0.85 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.118) (tstamp 51893cb6-d996-4bad-8b93-bf258c28bb0e))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/SM50B-SRDS-G-TF.STEP"
    (offset (xyz 0 -2.55 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
