(module JP3_2mm (layer F.Cu) (tedit 54896AF3)
  (fp_text reference JP3_2mm (at 0 -1.75) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 1.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start 3 1) (end -1 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -1 -1) (end 3 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 3 -1) (end 3 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -3 -1) (end -1 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start -1 -1) (end -1 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -1 1) (end -3 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -3 1) (end -3 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 3.5 -1.5) (end -3.5 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.5 -1.5) (end 3.5 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.5 2) (end -3.5 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.5 2) (end -3.5 -1.5) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at -2 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 connect oval (at 0 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
  (pad 1 connect rect (at -2 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
  (pad 3 connect oval (at 2 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
)
