(footprint "Texas_X2SON-4_1x1mm_P0.65mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "X2SON 5 pin 1x1mm package (Reference Datasheet: http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf Reference part: TPS383x) [StepUp generated footprint]")
  (tags "X2SON")
  (property "LCSC" "C485137")
  (property "MFG" "TI")
  (property "MPN" "TLV74211PDQNR")
  (property "Sheetfile" "Samsung_S5KGN2_Module.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "U5" (at 0 -1.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 25a82975-fc2c-4a63-9197-e7e310ef4494)
  )
  (fp_text value "TLV74211PDQNR" (at 0 1.5) (layer "F.Fab")
      (effects (font (size 0.6 0.6) (thickness 0.1)))
    (tstamp bd7c6519-ca4d-45fb-a811-bf7bec2db502)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.04)))
    (tstamp 0ade6619-9673-4b16-81f5-726fbade7fc6)
  )
  (fp_line (start -0.66 -0.63) (end 0.5 -0.63)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9110e5a0-1265-4134-85c1-908e4395111c))
  (fp_line (start -0.5 0.63) (end 0.5 0.63)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 39f7192a-ba41-4463-965b-d4c253210dfb))
  (fp_line (start -0.91 -0.75) (end 0.91 -0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e0fe713d-9f2d-4ea2-b41f-e0787bd7c7b7))
  (fp_line (start -0.91 0.75) (end -0.91 -0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9add77e1-3e96-4331-b17e-24b47daa6bfe))
  (fp_line (start 0.91 -0.75) (end 0.91 0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 344b5574-8135-46fa-a808-1d37a52a8914))
  (fp_line (start 0.91 0.75) (end -0.91 0.75)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8a912281-cdd2-4566-a60c-64d89f1d1888))
  (fp_line (start -0.5 -0.25) (end -0.25 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dd59fab4-2508-4472-b1b0-aa4510f71717))
  (fp_line (start -0.5 0.5) (end -0.5 -0.25)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb80e144-bc1a-492b-a20c-32cbab1a38a7))
  (fp_line (start -0.25 -0.5) (end 0.5 -0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ad11a39d-7bfa-4b1d-b286-08625c193ec1))
  (fp_line (start 0.5 -0.5) (end 0.5 0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f6f7815-7212-49be-bfc4-00ce5372426c))
  (fp_line (start 0.5 0.5) (end -0.5 0.5)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ecb12163-b306-4566-aa97-23fd8bb2d017))
  (pad "" smd custom (at -0.43 -0.325) (size 0.148492 0.148492) (layers "F.Paste")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.18 -0.075)
          (xy 0 0.105)
          (xy -0.22 0.105)
          (xy -0.22 -0.105)
          (xy 0.18 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp a1d0a6c2-ccd6-4368-9f56-e295d391ba0b))
  (pad "" smd custom (at -0.43 -0.325) (size 0.148492 0.148492) (layers "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.18 -0.075)
          (xy 0 0.105)
          (xy -0.18 0.105)
          (xy -0.18 -0.105)
          (xy 0.18 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp 80ffc9fa-d3aa-4433-bf14-11585d373790))
  (pad "" smd custom (at -0.43 0.325) (size 0.148492 0.148492) (layers "F.Paste")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.18 0.075)
          (xy 0.18 0.105)
          (xy -0.22 0.105)
          (xy -0.22 -0.105)
          (xy 0 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp 33b8e448-9283-427a-809d-0a4bdb5a11c5))
  (pad "" smd custom (at -0.43 0.325) (size 0.148492 0.148492) (layers "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.18 0.075)
          (xy 0.18 0.105)
          (xy -0.18 0.105)
          (xy -0.18 -0.105)
          (xy 0 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp ffc804e0-cfdf-44b6-b5f1-4e56c570cff2))
  (pad "" smd custom (at 0.43 -0.325) (size 0.148492 0.148492) (layers "F.Paste")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.22 0.105)
          (xy 0 0.105)
          (xy -0.18 -0.075)
          (xy -0.18 -0.105)
          (xy 0.22 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp 415d3e25-a980-4ed5-86ca-2ef67c0f7e51))
  (pad "" smd custom (at 0.43 -0.325) (size 0.148492 0.148492) (layers "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.18 0.105)
          (xy 0 0.105)
          (xy -0.18 -0.075)
          (xy -0.18 -0.105)
          (xy 0.18 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp 092ef061-745d-43e0-b8fc-f534634e42e8))
  (pad "" smd custom (at 0.43 0.325) (size 0.148492 0.148492) (layers "F.Paste")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.22 0.105)
          (xy -0.18 0.105)
          (xy -0.18 0.075)
          (xy 0 -0.105)
          (xy 0.22 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp eb0100d5-027d-448f-a02c-f27dff4659b0))
  (pad "" smd custom (at 0.43 0.325) (size 0.148492 0.148492) (layers "F.Mask")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.18 0.105)
          (xy -0.18 0.105)
          (xy -0.18 0.075)
          (xy 0 -0.105)
          (xy 0.18 -0.105)
        )
        (width 0) (fill yes))
    ) (tstamp 5f402610-ec15-45e9-9555-5409e2139296))
  (pad "1" smd custom (at -0.43 -0.325) (size 0.148492 0.148492) (layers "F.Cu")
    (zone_connect 2) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.23 -0.054289)
          (xy 0.020711 0.155)
          (xy -0.23 0.155)
          (xy -0.23 -0.155)
          (xy 0.23 -0.155)
        )
        (width 0) (fill yes))
    ) (tstamp 2d86f041-1aa8-45ee-bcd6-96b4d7570b98))
  (pad "2" smd custom (at -0.43 0.325) (size 0.148492 0.148492) (layers "F.Cu")
    (zone_connect 2) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.23 0.054289)
          (xy 0.23 0.155)
          (xy -0.23 0.155)
          (xy -0.23 -0.155)
          (xy 0.020711 -0.155)
        )
        (width 0) (fill yes))
    ) (tstamp 459b2d37-271d-419f-b3dd-e9ec764d0bf8))
  (pad "3" smd custom (at 0.43 0.325) (size 0.148492 0.148492) (layers "F.Cu")
    (zone_connect 2) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.23 0.155)
          (xy -0.23 0.155)
          (xy -0.23 0.054289)
          (xy -0.020711 -0.155)
          (xy 0.23 -0.155)
        )
        (width 0) (fill yes))
    ) (tstamp 745f7ec1-8b86-4aa0-b138-3b4914c6ab17))
  (pad "4" smd custom (at 0.43 -0.325) (size 0.148492 0.148492) (layers "F.Cu")
    (zone_connect 2) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly
        (pts
          (xy 0.23 0.155)
          (xy -0.020711 0.155)
          (xy -0.23 -0.054289)
          (xy -0.23 -0.155)
          (xy 0.23 -0.155)
        )
        (width 0) (fill yes))
    ) (tstamp cd932e6f-baa7-4504-a06f-707e2fdf2cfb))
  (pad "5" smd roundrect (at 0 0 45) (size 0.48 0.48) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1041666667)
    (solder_mask_margin -0.05) (solder_paste_margin -0.065) (solder_paste_margin_ratio -0.00000001) (tstamp a4733489-b868-44e3-8a64-754dcc50699d))
  (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/Texas_X2SON-4_1x1mm_P0.65mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
