(footprint "JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH top entry")
  (property "LCSC" "C160404")
  (property "MFG" "JST")
  (property "MPN" "SM04B-SRSS-TB(LF)(SN)")
  (property "Sheetfile" "CAN_Node.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J1" (at 0 -3.35 180) (layer "F.SilkS") hide
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 00122d8c-2727-4c44-9bce-7e62da2c01ab)
  )
  (fp_text value "SWD" (at 0 3.5 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d8e9b535-3259-4c9a-a03f-14ae56d3dd31)
  )
  (fp_text user "${REFERENCE}" (at 0 2.2 180) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp af3ce60a-3cf6-4a01-969c-d6d384f2f714)
  )
  (fp_line (start -3.11 -1.785) (end -2.06 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6ef236b0-5785-4bf2-a4e4-0115d8e851d1))
  (fp_line (start -3.11 0.715) (end -3.11 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b07c23a0-5c00-48bf-bac8-7112dcd245b0))
  (fp_line (start -2.06 -1.785) (end -2.06 -2.775)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d8de07a5-d068-4732-8342-d2f2222c6609))
  (fp_line (start -1.94 2.685) (end 1.94 2.685)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c4c65532-47f0-41ad-9ba0-e6639f8f044a))
  (fp_line (start 3.11 -1.785) (end 2.06 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be12adcc-b827-4a31-a44a-0918545bb7a5))
  (fp_line (start 3.11 0.715) (end 3.11 -1.785)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0114f026-7d2f-4127-9fd1-20e3784a0385))
  (fp_line (start -3.55 2.525) (end -3.55 1.225)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7d7998d4-9127-440c-818f-a9c9933adcb3))
  (fp_line (start -3.25 -1.675) (end -3.247014 0.836943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0818a603-d20f-472e-8efb-71ff9c6828a4))
  (fp_line (start -3 -1.925) (end -1.95 -1.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 45011bc0-2611-4ebb-934f-ff4291b1a4db))
  (fp_line (start -1.95 -1.925) (end -1.95 -2.625)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f6b4f7ec-c681-49e9-b64e-753118c67c44))
  (fp_line (start -1.65 -2.925) (end 1.65 -2.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c281c848-3040-4640-9923-1990e461bb97))
  (fp_line (start 1.95 -1.925) (end 1.95 -2.625)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6aa9a9a2-4fcf-4a85-b989-967654c7d485))
  (fp_line (start 3 -1.925) (end 1.95 -1.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a1db9030-efb4-4a38-adf3-5f56d6f0fdbe))
  (fp_line (start 3.15 2.925) (end -3.15 2.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4dd63cff-b1e6-4103-ba05-a34b8070097d))
  (fp_line (start 3.25 -1.675) (end 3.247014 0.836943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b799cb11-2e6f-4465-abe6-e585fc7124c0))
  (fp_line (start 3.55 2.525) (end 3.55 1.225)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc3efc3f-e0f1-4a30-a65d-ccd4ed46f882))
  (fp_arc (start -3.55 1.225) (mid -3.465282 0.978835) (end -3.247014 0.836943)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 785176d7-60b5-4fb8-ad8d-35e8eaf09061))
  (fp_arc (start -3.25 -1.675) (mid -3.176777 -1.851777) (end -3 -1.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6e50c791-9e9f-4200-bea4-46fa639fedc9))
  (fp_arc (start -3.15 2.925) (mid -3.432843 2.807843) (end -3.55 2.525)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bf5c34a8-362e-4271-8e1c-6d4af096794d))
  (fp_arc (start -1.95 -2.625) (mid -1.862132 -2.837132) (end -1.65 -2.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e8c93e3c-3eb0-4377-a811-51caf26dda49))
  (fp_arc (start 1.65 -2.925) (mid 1.862132 -2.837132) (end 1.95 -2.625)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1fcb62f3-1dd3-451a-8960-7252e692372d))
  (fp_arc (start 3 -1.925) (mid 3.176777 -1.851777) (end 3.25 -1.675)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 70286e2a-46ec-417b-96f4-5a53cd6c556c))
  (fp_arc (start 3.247014 0.836943) (mid 3.465282 0.978835) (end 3.55 1.225)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 523064ff-7c46-45a9-b246-19f7b4408114))
  (fp_arc (start 3.55 2.525) (mid 3.432843 2.807843) (end 3.15 2.925)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cdd7ec9a-bb67-4d36-b8d0-3431dce3ca03))
  (fp_line (start -3 -1.675) (end -3 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1369d0c-4454-49d7-900b-456dc3f5ac07))
  (fp_line (start -3 -1.675) (end 3 -1.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 867d3787-e89b-45af-b149-282fc4783b9f))
  (fp_line (start -3 2.575) (end -3 4.575)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp 88d8a933-c671-4273-aea3-a01f0877f760))
  (fp_line (start -3 2.575) (end 3 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4178b6e7-ea3d-47c3-9039-9a4f9cfca767))
  (fp_line (start -3 4.575) (end 3 4.575)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp 38c2e161-a59e-4202-8b4d-66cd6f319120))
  (fp_line (start -2 -1.675) (end -1.5 -0.967893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2650108-01a9-4b0d-bb0d-b57f6e49583d))
  (fp_line (start -1.5 -0.967893) (end -1 -1.675)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bd7a4ce5-e442-4a9c-b446-ee1c24167561))
  (fp_line (start 3 -1.675) (end 3 2.575)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09195d5b-0e88-4fe1-8a97-923559ab4817))
  (fp_line (start 3 4.575) (end 3 2.575)
    (stroke (width 0.1) (type dash)) (layer "F.Fab") (tstamp 420abb2d-a59e-4be9-8214-543d419d8220))
  (pad "1" smd roundrect (at -1.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3b613439-ec7f-4f1e-ac7a-71dacbd7f31e))
  (pad "2" smd roundrect (at -0.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d3264131-476f-416a-8e4f-2277c089231a))
  (pad "3" smd roundrect (at 0.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 5110ca27-4cdc-4f35-95df-00b5921e6ce8))
  (pad "4" smd roundrect (at 1.5 -2) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 46c3b9e0-1186-46c2-9cc6-ea63dc7e42af))
  (pad "MP" smd roundrect (at -2.8 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333) (tstamp 8ca17580-bb55-43e7-901e-6a1d7eafc920))
  (pad "MP" smd roundrect (at 2.8 1.875) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333) (tstamp 65002192-e354-44e5-a479-7a4367bde5b4))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
    (offset (xyz 0 1.325 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
