(module "USB_C_Receptacle_Jing_C168700" (layer "F.Cu") (tedit 5FA416DD)
  (property "MPN" "DX07B024JJ1R1500")
  (property "Sheet file" "/home/stefan/Projects/Current/Thunderbolt3_PCB/Thunderbolt3_PCB.kicad_sch")
  (property "Sheet name" "")
  (attr through_hole)
  (fp_text reference "J2" (at -5.75 -2.5 90 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 7a1bde42-dbf0-4db6-a13a-67adce822c75)
  )
  (fp_text value "Jing C168700" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 896ef3e0-2719-4594-8767-c58d6793344b)
  )
  (fp_text user "PCB CUTOUT" (at 0 -4.25 unlocked) (layer "Dwgs.User")
    (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp 11a5aa99-4d10-4781-b6c9-dc137e82a3cb)
  )
  (fp_text user "${REF}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 348c5fb4-d58f-48ab-9fc4-0e09b99030b5)
  )
  (fp_line (start -4.75 0) (end -4.75 -4.7) (layer "Dwgs.User") (width 0.1) (tstamp 1d3b3d48-97f5-4402-acfb-8eb2d1948d89))
  (fp_line (start 4.75 -4.7) (end 4.75 0) (layer "Dwgs.User") (width 0.1) (tstamp ab986c8d-f74e-4bdc-a88f-3a1254d10a41))
  (fp_line (start -4.75 -4.7) (end 4.75 -4.7) (layer "Dwgs.User") (width 0.1) (tstamp b43232bc-43ac-4f67-bb2b-d49f89def02f))
  (pad "" np_thru_hole circle (at -3.725 -5.25) (size 0.75 0.75) (drill 0.65) (layers "F.Mask") (tstamp 26104d89-c663-4d91-93c3-f2bb3bf7bdd0))
  (pad "" np_thru_hole oval (at 3.725 -5.25) (size 1.05 0.75) (drill oval 0.95 0.65) (layers "F.Mask") (tstamp 5cbb5cee-3b74-44bb-886c-75fc200fac2f))
  (pad "A1" smd roundrect (at -2.75 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp afbf9fa2-21a3-4d98-a5f1-3fa02f66157e))
  (pad "A2" smd roundrect (at -2.25 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 81a96cd1-038a-4248-897e-555e380a9cc7))
  (pad "A3" smd roundrect (at -1.75 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp bd994f92-1b8f-42b8-b759-d17fd77bbb80))
  (pad "A4" smd roundrect (at -1.25 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 25284279-3d6d-4f6b-a5f2-503f5d95ca57))
  (pad "A5" smd roundrect (at -0.75 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 5b81ce03-8a7d-45fc-adea-b9e88c50d5bb))
  (pad "A6" smd roundrect (at -0.25 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp ab1d0685-d542-4233-9b62-3fc542c16572))
  (pad "A7" smd roundrect (at 0.25 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp bb7bcb1b-7fc5-40ba-b6de-30e24b72197e))
  (pad "A8" smd roundrect (at 0.75 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 6af87349-6b79-4e97-a3ee-c8b0f5bdedfb))
  (pad "A9" smd roundrect (at 1.25 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 504f5d48-306e-47ae-a8f9-4bb49082436c))
  (pad "A10" smd roundrect (at 1.75 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp d1cbbef0-e8a4-4650-b850-71e97fca0304))
  (pad "A11" smd roundrect (at 2.25 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 06679f1c-9af8-4aad-88ba-d1e5653e4f8b))
  (pad "A12" smd roundrect (at 2.75 -7.06) (size 0.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp e01ffaae-5045-4539-8dd1-c446c82d7fbc))
  (pad "B1" thru_hole oval (at 3.05 -5.95) (size 1.15 0.65) (drill oval 0.9 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 5e2ad4c5-893c-456d-a9b7-c55a71ac1229))
  (pad "B2" thru_hole circle (at 2.4 -5.25) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 0895e56c-74f8-4101-8082-87694bb4d789))
  (pad "B3" thru_hole circle (at 1.6 -5.25) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 13732d66-9d27-4263-a871-d5a90637bf0d))
  (pad "B4" thru_hole circle (at 1.2 -5.95) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 05cb7ecd-4fb5-4824-89b4-aafd7bc45c4b))
  (pad "B5" thru_hole circle (at 0.8 -5.25) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 71c5a92b-58b0-4563-b77f-7fa78f08629a))
  (pad "B6" thru_hole circle (at 0.4 -5.95) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp c4c3797e-943e-454e-a9b2-acf933900633))
  (pad "B7" thru_hole circle (at -0.4 -5.95) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 66e4d780-28d9-4d3a-8506-1e2ee8d15a9e))
  (pad "B8" thru_hole circle (at -0.8 -5.25) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp f1bf6fe4-6ca7-4399-b91b-8d7d38bf3762))
  (pad "B9" thru_hole circle (at -1.2 -5.95) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 2a644f88-5e0b-4143-b74f-81fa8e87b626))
  (pad "B10" thru_hole circle (at -1.6 -5.25) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp a4ea7d75-947a-4a86-aba2-3c1f14d7c7db))
  (pad "B11" thru_hole circle (at -2.4 -5.25) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp fe687708-d461-45d0-b7ac-4339e0474240))
  (pad "B12" thru_hole oval (at -3.05 -5.95) (size 1.15 0.65) (drill oval 0.9 0.4) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 8fb667fa-1cec-4e91-8b3e-cb4766b0cf4a))
  (pad "S1" thru_hole oval (at -4.5 -6.76) (size 1 1.6) (drill oval 0.5 1.1) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 0f17a45b-0017-4cce-aa85-98adc96fe542))
  (pad "S1" thru_hole oval (at 4.5 -6.76) (size 1 1.6) (drill oval 0.5 1.1) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 47ed8805-0f63-4cf4-b7ac-d9d4010c74e8))
  (pad "S1" thru_hole oval (at 6.075 -1.25) (size 1 2) (drill oval 0.5 1.5) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 77954250-dd74-42f6-a63d-bc63c203d310))
  (pad "S1" thru_hole oval (at -6.075 -1.25) (size 1 2) (drill oval 0.5 1.5) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 90591387-0b33-406e-b9eb-6baf78f09100))
)
