(footprint "1P_3.5x2.5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "Sim.Enable" "0")
  (property "exclude_from_bom" "")
  (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "J28" (at 2 0 90 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 0d9baa9f-cc7a-4dfe-9d94-b50df6f05ebd)
  )
  (fp_text value "|" (at -2.625 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 50a2dfee-5353-4f0f-bcf4-2c7bd2876d69)
  )
  (fp_text user "${REFERENCE}" (at 2 0 90 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.05) bold))
    (tstamp 5f9e993b-3fa0-43a6-9c57-96d2b9b62954)
  )
  (fp_line (start -1.9 -0.5) (end -1.9 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e374dd70-39cc-4ea8-9a3b-9fd42692d96d))
  (fp_line (start -1 -1.4) (end 1.9 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3825671f-0e24-4bf2-a5e0-56254e477706))
  (fp_line (start 1.9 -1.4) (end 1.9 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c9514ef7-0941-4c91-b10f-e858f8bfb60c))
  (fp_line (start 1.9 1.4) (end -1 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c2f41ce6-a04d-46cd-9c3f-863513ac1de3))
  (fp_arc (start -1.9 -0.5) (mid -1.636396 -1.136396) (end -1 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 97a276e0-662b-483c-8328-d1649006fbe3))
  (fp_arc (start -1 1.4) (mid -1.636396 1.136396) (end -1.9 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 817f81a3-67c1-419f-8ee1-ff6ac447fcaf))
  (pad "1" smd roundrect (at 0 0) (size 3.5 2.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.3)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 2a9b588e-d7c2-491a-b196-65232b528452))
)
