(module USB_Compact_Cable (layer F.Cu) (tedit 586136EA)
  (solder_mask_margin 0.025)
  (attr virtual)
  (fp_text reference J3 (at -2.65 0 90) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value USB (at -0.05 -1.35) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user N (at 0.35 -0.5 180) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user P (at -0.35 0.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user + (at -1.5 -0.6) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text user - (at 1.5 -0.6) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -1.5 -1.1) (end -2.3 -1.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.3 -1.1) (end -2.3 1.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -2.3 1.1) (end 2.3 1.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 2.3 1.1) (end 2.3 -1.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 2.3 -1.1) (end 1.5 -1.1) (layer F.SilkS) (width 0.125))
  (pad 1 connect roundrect (at -1.5 0) (size 1.1 1.8) (layers B.Cu B.Mask)(roundrect_rratio 0.25)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 4 connect oval (at 1.5 0) (size 1.1 1.8) (layers B.Cu B.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 2 connect roundrect (at -0.4 -0.5 90) (size 0.8 1.1) (drill (offset 0 0.2)) (layers B.Cu B.Mask)(roundrect_rratio 0.25)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 3 connect roundrect (at 0.4 0.5 270) (size 0.8 1.1) (drill (offset 0 0.2)) (layers B.Cu B.Mask)(roundrect_rratio 0.25)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 1 thru_hole circle (at -1.5 0.35) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 4 thru_hole circle (at 1.5 0.35) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 2 thru_hole circle (at -0.35 -0.5 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
  (pad 3 thru_hole circle (at 0.35 0.5 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
    (zone_connect 1) (thermal_width 0.2) (thermal_gap 0.2))
)
