(footprint "2P_TH_2x3.5_P2.5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.7 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 00d6e831-3729-4c35-a504-df7c0368c32c)
  )
  (fp_text value "2P_TH_2x3.5_P2.5" (at 0 3.45 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 38f8e0dd-6e47-42a6-b591-f0d36fd918bf)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.7 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8625d9b7-44ce-4619-af98-ec77972663a0)
  )
  (fp_line (start -2.5 -0.8) (end -2.5 2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 871fc49e-c596-4fe1-a0a9-be9d800dbe0e))
  (fp_line (start -2.05 2.75) (end 1.95 2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4a8aa056-00a6-410f-9490-950e06cef7f4))
  (fp_line (start 1.95 -1.25) (end -2.05 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb1170c3-e3d8-4a42-bdfc-cd1871555c9c))
  (fp_line (start 2.5 2.2) (end 2.5 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fe54ef2c-831a-4399-a54f-feaad01941c8))
  (fp_arc (start -2.5 -0.8) (mid -2.368198 -1.118198) (end -2.05 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a292966c-9bc7-4537-a2ab-e03ee3667c6a))
  (fp_arc (start -2.05 2.75) (mid -2.368198 2.618198) (end -2.5 2.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4c72b5ff-bfaf-47b9-867b-41b26a2fd475))
  (fp_arc (start 1.95 -1.25) (mid 2.338909 -1.088909) (end 2.5 -0.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6105e1f9-e43d-41a8-b859-b296906f3389))
  (fp_arc (start 2.5 2.2) (mid 2.338909 2.588909) (end 1.95 2.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b293f72f-667a-47f6-9550-55448ed51951))
  (pad "1" thru_hole circle (at -1.25 0) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp a5fc1198-00f9-4520-9024-b0779f871d3c))
  (pad "1" smd roundrect (at -1.25 0.75) (size 2 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1) (tstamp 796533eb-2e62-4c31-8a04-e6dda60f9a1f))
  (pad "2" thru_hole circle (at 1.25 0) (size 1.5 1.5) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp 6bb5ae67-3dee-4edd-a97a-d7c3655d8cc7))
  (pad "2" smd roundrect (at 1.25 0.75) (size 2 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2) (tstamp c61ccb5d-dc51-4bd5-a086-d7603a6b9420))
)
