(footprint "JST_SH_BM06B-SRSS-TB_1x06-1MP_P1.00mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST SH series connector, BM06B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH side entry")
  (property "Sheetfile" "G4ESC.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J1" (at 0 -3.3 -180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 83ad969e-a2f3-4fd8-8b7d-c3691ced20fc)
  )
  (fp_text value "HALL/TEMP" (at 0 3.3 -180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 04d7784f-46c5-4f73-af1e-1d66bcf29fe3)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.25 -180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 766dea55-7b0b-440b-bf04-0a554b760bd1)
  )
  (fp_line (start -4.11 -0.04) (end -4.11 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6bee04e9-4e82-4995-987d-2fb3855c07cf))
  (fp_line (start -4.11 1.11) (end -3.06 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 243f4ba4-ad4b-4899-861f-899ba6adedab))
  (fp_line (start -3.06 1.11) (end -3.06 2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 380ed112-7132-4431-bcc8-6f08ff461588))
  (fp_line (start -2.94 -2.01) (end 2.94 -2.01)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1e27eaa-3b09-4099-bf31-90ace5708f3b))
  (fp_line (start 4.11 -0.04) (end 4.11 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49894b5a-6b56-43de-9d6c-0e19c64e077b))
  (fp_line (start 4.11 1.11) (end 3.06 1.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d2d9c761-633e-4b69-a312-14a8aa79d6f5))
  (fp_line (start -4.55 -1.85) (end -4.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7e60eb96-78d1-4e3e-bc6f-415fc8db7ae0))
  (fp_line (start -4.25 1) (end -4.259888 -0.16539)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 69a674f7-2cb9-42ac-b2c0-e4545b7e5afa))
  (fp_line (start -4.15 -2.25) (end 4.15 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp acaa05f7-c905-41fd-aa28-97c31d7aa22f))
  (fp_line (start -4 1.25) (end -2.95 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 75442229-ead3-4924-8395-b9bb53f2b247))
  (fp_line (start -2.95 1.25) (end -2.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 53275c2f-969a-4905-a977-fbd5fc815221))
  (fp_line (start 2.65 2.25) (end -2.65 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6f385bed-c6ed-47d5-afcb-bccd5ae0479d))
  (fp_line (start 2.95 1.25) (end 2.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 067bcac4-15fc-4f26-bf7c-f68012dbc968))
  (fp_line (start 4 1.25) (end 2.95 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 28bc5af5-d9af-45a1-90b6-1d8ae6a6bdd1))
  (fp_line (start 4.25 1) (end 4.259888 -0.16539)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 37cb5e37-5926-4502-b4eb-92337bd5ccd6))
  (fp_line (start 4.55 -1.85) (end 4.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7f245a24-a6b3-48a7-a34f-95d8930c2e15))
  (fp_arc (start -4.55 -1.85) (mid -4.432843 -2.132843) (end -4.15 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 41791a2e-a7dc-44c0-9a36-941138278358))
  (fp_arc (start -4.259888 -0.16539) (mid -4.46934 -0.309121) (end -4.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9326a8e1-2845-40b7-9863-b81474720def))
  (fp_arc (start -4 1.25) (mid -4.176777 1.176777) (end -4.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ee2dc648-3bd1-4030-9c2f-fcc85774666f))
  (fp_arc (start -2.65 2.25) (mid -2.862132 2.162132) (end -2.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 05f42fe7-47b6-4c44-9b8a-549978bb28a0))
  (fp_arc (start 2.95 1.95) (mid 2.862132 2.162132) (end 2.65 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bf44914e-0c29-4b87-b328-029ac3776be1))
  (fp_arc (start 4.15 -2.25) (mid 4.432843 -2.132843) (end 4.55 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 13f2d618-4c81-44d5-ba98-8952dd41714b))
  (fp_arc (start 4.25 1) (mid 4.176777 1.176777) (end 4 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b376dae4-d274-4fed-ae48-899006eacdd8))
  (fp_arc (start 4.55 -0.55) (mid 4.469339 -0.309122) (end 4.259888 -0.16539)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5915ed1b-5e35-478c-b73d-ae2ba7f01282))
  (fp_line (start -4 -1.9) (end 4 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8bdb168e-2dac-4ef7-8adc-a4a4f0d3ff0b))
  (fp_line (start -4 1) (end -4 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 999855e2-511e-4757-9136-8cdfeb0e0ee9))
  (fp_line (start -4 1) (end 4 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 22187d49-0e21-46b9-b808-6e49ec1734c1))
  (fp_line (start -3 1) (end -2.5 0.292893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea271187-6af5-4be2-a53f-0fa6e999c271))
  (fp_line (start -2.65 -1.55) (end -2.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5cc86a01-ec28-49db-aeb5-8241389e179c))
  (fp_line (start -2.65 -0.95) (end -2.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5b91baf7-782f-4df9-a93f-abe6691bd34a))
  (fp_line (start -2.5 0.292893) (end -2 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d60e3da-7282-4fa8-a0a6-eadb6168d4dd))
  (fp_line (start -2.35 -1.55) (end -2.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3de3b91-0f19-4d46-81c4-8758bc2c48a2))
  (fp_line (start -2.35 -0.95) (end -2.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c6b9ec42-68f1-4c8d-bf24-a1e6ff5b04ed))
  (fp_line (start -1.65 -1.55) (end -1.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fca6859d-0851-4d97-b7a6-a866ea100a84))
  (fp_line (start -1.65 -0.95) (end -1.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91be6011-437c-4fb9-9b13-1e19248d1f77))
  (fp_line (start -1.35 -1.55) (end -1.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 928ba337-7d34-4b87-84cd-643a758a1c8b))
  (fp_line (start -1.35 -0.95) (end -1.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 63e33434-2c6c-4af7-bb0b-250743d2b563))
  (fp_line (start -0.65 -1.55) (end -0.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6a3bc0d3-c8d6-4849-9f55-c262a32a2d18))
  (fp_line (start -0.65 -0.95) (end -0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c530d6f4-f6f7-4fe0-8111-96539a931596))
  (fp_line (start -0.35 -1.55) (end -0.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a5da7ff-2a0a-49c1-8f0d-082decde991c))
  (fp_line (start -0.35 -0.95) (end -0.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4ef8bebd-36a4-494f-80bc-8d5df123cc4d))
  (fp_line (start 0.35 -1.55) (end 0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d359fab-3060-460d-a3ef-128cb64c812f))
  (fp_line (start 0.35 -0.95) (end 0.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d279781e-e471-43b5-aaf9-7bad4f398d1d))
  (fp_line (start 0.65 -1.55) (end 0.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2bcaa77f-3697-4f5f-98d6-04d31dedc5b5))
  (fp_line (start 0.65 -0.95) (end 0.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86c86c44-cb7c-4a83-b3cc-0e45beafdb3d))
  (fp_line (start 1.35 -1.55) (end 1.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8c45ad2-88d3-4546-864a-5ce63d5acdc9))
  (fp_line (start 1.35 -0.95) (end 1.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c70a6fb6-6f7e-4143-b359-b5a99c76a916))
  (fp_line (start 1.65 -1.55) (end 1.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a92f4453-ed52-46e1-a117-fe1b8d93f059))
  (fp_line (start 1.65 -0.95) (end 1.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6bcde98f-85db-47bc-b82d-d6428514e2d7))
  (fp_line (start 2.35 -1.55) (end 2.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7f8ed3a8-671a-4289-8520-bc34aa978e3a))
  (fp_line (start 2.35 -0.95) (end 2.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 75554e63-5656-43b0-a58f-12a9e1a7f55b))
  (fp_line (start 2.65 -1.55) (end 2.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25b538ba-08ff-4f7a-9914-13dbc10f12c4))
  (fp_line (start 2.65 -0.95) (end 2.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a0d4db2c-8e76-46c9-b6f9-b4b5cb487826))
  (fp_line (start 4 1) (end 4 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7f68b128-fdb1-4bb2-a402-ba0dcc3fe6a6))
  (pad "1" smd roundrect (at -2.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b6b8283a-609f-4ffd-8e03-cfe56708d31e))
  (pad "2" smd roundrect (at -1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0a4e62e2-7e1c-4c69-bf84-f107f24f8cb6))
  (pad "3" smd roundrect (at -0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 07a0c589-354a-4e01-bf3c-53b2a2ff8f3d))
  (pad "4" smd roundrect (at 0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4d78d27d-0e6b-4f6b-8e87-a5339f0ea6ad))
  (pad "5" smd roundrect (at 1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 08b5caab-6001-4c57-bfae-4baf9a574413))
  (pad "6" smd roundrect (at 2.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 983dc9a5-f84e-4b2d-b982-10da7ed425c8))
  (pad "MP" smd roundrect (at -3.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 705f365b-4ec4-41e2-80b4-b4029933a93e))
  (pad "MP" smd roundrect (at 3.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 8c23711e-1d00-4de2-9a4b-eb203622540d))
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM06B-SRSS-TB_1x06-1MP_P1.00mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM06B-SRSS-TB.STEP"
    (offset (xyz 0 0.45 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
