(module "Kingbright_ATDS3534" (layer F.Cu) (tedit 5D6EB13C)
  (solder_paste_margin -0.001)
  (solder_paste_ratio -0.00000001)
  (attr smd)
  (fp_text reference "D2" (at -2.7 1.7) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text value "405nm" (at 0 2) (layer F.Fab)
    (effects (font (size 0.25 0.25) (thickness 0.05)))
  )
  (fp_circle (center 0 0) (end 1.3 0) (layer F.Fab) (width 0.12))
  (fp_circle (center 0.9 -1.4) (end 1 -1.4) (layer F.Fab) (width 0.12))
  (fp_line (start -1.1 -1.4) (end -0.7 -1.4) (layer F.Fab) (width 0.12))
  (fp_line (start -0.9 -1.6) (end -0.9 -1.2) (layer F.Fab) (width 0.12))
  (fp_line (start -2 2) (end -2 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 2) (end -2 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 2) (end 1 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 1) (end 2 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -2) (end 2 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 -2) (end 2 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -2) (end -1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -2) (end -2 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.725 1.725) (end -1.725 -1.725) (layer F.Fab) (width 0.12))
  (fp_line (start 1.725 1.725) (end -1.725 1.725) (layer F.Fab) (width 0.12))
  (fp_line (start 1.725 -1.725) (end 1.725 1.725) (layer F.Fab) (width 0.12))
  (fp_line (start -1.725 -1.725) (end 1.725 -1.725) (layer F.Fab) (width 0.12))
  (fp_circle (center -2.3 -1.9) (end -2.3 -2) (layer F.SilkS) (width 0.15))
  (pad "MP" smd roundrect (at 0 0) (size 1.3 3.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.077))
  (pad "K" smd roundrect (at 1.4 0) (size 0.5 3.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1))
  (pad "A" smd roundrect (at -1.4 0) (size 0.5 3.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1))
  (model "${KICAD7_3DMODEL_DIR}/LED_SMD.3dshapes/Kingbright_ATDS3534.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
