(footprint "WQFN-30-1EP_4x6mm_P0.5mm_EP1.8x4.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "B1F_U2"
		(at 0 -3.85 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "7b6cf963-25c4-42fc-8640-fc85eaacfece")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LM76002"
		(at -2.25 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0443f0e5-2621-4ebd-a1a4-58c710ee9c41")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:WQFN-30-1EP_4x6mm_P0.5mm_EP1.8x4.5mm"
		(at -0.2 3.45 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4fe533fe-1e5c-420b-99a6-443fd13210b0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -0.2 3.45 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3fd6ef56-6878-4126-bba7-bc6d60532d8d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -0.2 3.45 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "05ec2f95-9c52-4652-9bc9-3da271443a1f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f57703df-8ad4-47f8-96a1-2d434909e6a3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "LM76002RNPR"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "054b1914-756f-4b26-a2a3-4503a79e8838")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C544769"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ce75d326-1954-483d-a81c-cb6646777ec4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB Rotation Offset" "-90"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d9358ca0-539d-458d-b45e-4b65c5d975cc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -2.175 -3.1)
		(mid -2.153033 -3.153033)
		(end -2.1 -3.175)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2e8ead7d-c40f-43e2-8f13-ba7ad820649b")
	)
	(fp_arc
		(start -2.1 3.175)
		(mid -2.153033 3.153033)
		(end -2.175 3.1)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2ec7875c-a22a-4d58-ad25-44e9226d4f5c")
	)
	(fp_arc
		(start 2.1 -3.175)
		(mid 2.153033 -3.153033)
		(end 2.175 -3.1)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d6cbe7c1-1e2e-4c7a-b2c8-7aee458ee9ce")
	)
	(fp_arc
		(start 2.175 3.1)
		(mid 2.153033 3.153033)
		(end 2.1 3.175)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "101af37b-8739-4b4d-8fd1-98935c333d41")
	)
	(fp_poly
		(pts
			(xy -2.300001 -2.5) (xy -2.55 -2.7) (xy -2.55 -2.3)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "530c9b46-7c0c-471e-bb68-b0d7a3d7e67c")
	)
	(fp_poly
		(pts
			(xy -2.1 -3.1) (xy -2.1 -2.75) (xy -2.25 -2.75) (xy -2.25 -3.1) (xy -2.1 -3.25) (xy -1 -3.25) (xy -1 -3.1)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "ddfcef49-3157-454e-917b-073a0c54de44")
	)
	(fp_poly
		(pts
			(xy -2.1 3.1) (xy -2.1 2.75) (xy -2.25 2.75) (xy -2.25 3.1) (xy -2.1 3.25) (xy -1.35 3.25) (xy -1.35 3.1)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "c6863275-46ec-403c-ad43-031cf867f762")
	)
	(fp_poly
		(pts
			(xy 2.1 -3.1) (xy 2.1 -2.75) (xy 2.25 -2.75) (xy 2.25 -3.1) (xy 2.1 -3.25) (xy 1.35 -3.25) (xy 1.35 -3.1)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bde99519-1623-4b64-b3cf-fa5051e7b732")
	)
	(fp_poly
		(pts
			(xy 2.1 3.1) (xy 2.1 2.75) (xy 2.25 2.75) (xy 2.25 3.1) (xy 2.1 3.25) (xy 1.35 3.25) (xy 1.35 3.1)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "86e57de8-f658-4eb3-916e-9b4ae733617f")
	)
	(fp_line
		(start -2.35 -2.575)
		(end -2.35 2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3f68d4af-c291-4e18-a902-8802d7baef61")
	)
	(fp_line
		(start -2.25 -3)
		(end -2.249228 -2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7d5c5471-a03b-4b67-a8ce-2a3e21c5633e")
	)
	(fp_line
		(start -2.25 3)
		(end -2.249228 2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "52c8d39b-fa74-40c4-8b69-0f7c8167d9d2")
	)
	(fp_line
		(start -2.000001 -3.25)
		(end -1 -3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "22ef850f-95e1-4633-b110-ed3df066cfc6")
	)
	(fp_line
		(start -2.000001 3.25)
		(end -1 3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "67a8f9db-3f2d-4b33-ae32-5183adab53cf")
	)
	(fp_line
		(start -0.85 3.35)
		(end 0.85 3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "21db4616-6145-475c-afa2-f20ac1b81cf9")
	)
	(fp_line
		(start 0.85 -3.35)
		(end -0.85 -3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0e32f347-0fa8-449e-a098-c887725f949f")
	)
	(fp_line
		(start 2.000001 -3.25)
		(end 1 -3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c98d6d2f-f7a4-406b-b148-56b9da2baf23")
	)
	(fp_line
		(start 2.000001 3.25)
		(end 1 3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4c90f723-e592-4576-8b1b-74a1766f570b")
	)
	(fp_line
		(start 2.25 -3)
		(end 2.249228 -2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "afa11837-0ec8-4cd2-b2da-a987a099fd09")
	)
	(fp_line
		(start 2.25 3)
		(end 2.249228 2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "769c2438-6634-4ee0-a57c-0a9fd748bdc5")
	)
	(fp_line
		(start 2.35 2.575)
		(end 2.35 -2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e9e72137-f3a4-4eb5-ab70-ed06168abea9")
	)
	(fp_arc
		(start -2.35 -2.575)
		(mid -2.322982 -2.675385)
		(end -2.249228 -2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cfeb391b-1c6c-4e49-b543-79620684059f")
	)
	(fp_arc
		(start -2.25 -3)
		(mid -2.176777 -3.176777)
		(end -2.000001 -3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2348f266-dcf4-4aa1-874c-efed4a4f80e1")
	)
	(fp_arc
		(start -2.249228 2.748649)
		(mid -2.322982 2.675385)
		(end -2.35 2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8dd92e1c-e0ad-4f10-b57c-7d8f7adbcd8c")
	)
	(fp_arc
		(start -2.000001 3.25)
		(mid -2.176777 3.176777)
		(end -2.25 3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "13d3be12-74b2-4d6b-a1b2-e91748aeda17")
	)
	(fp_arc
		(start -1 -3.25)
		(mid -0.936803 -3.317705)
		(end -0.85 -3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "aa94fcbb-3de4-4035-96ab-1d6306c30c02")
	)
	(fp_arc
		(start -0.85 3.35)
		(mid -0.936803 3.317705)
		(end -1 3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "385f3d4f-a97a-457e-aec5-ae8dc8c14eac")
	)
	(fp_arc
		(start 0.85 -3.35)
		(mid 0.936803 -3.317705)
		(end 1 -3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4dfe4168-de8f-4d53-a635-0af3eb13a136")
	)
	(fp_arc
		(start 1 3.25)
		(mid 0.936803 3.317705)
		(end 0.85 3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "da05889c-0af5-429a-9aad-9b26a5539797")
	)
	(fp_arc
		(start 2.000001 -3.25)
		(mid 2.176777 -3.176776)
		(end 2.25 -3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b9f5c365-92d9-4db4-9b55-96332d04a10a")
	)
	(fp_arc
		(start 2.249228 -2.748649)
		(mid 2.322982 -2.675386)
		(end 2.35 -2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1d907d3a-3e1d-4fab-8bb4-ed7453f34cbc")
	)
	(fp_arc
		(start 2.25 3)
		(mid 2.176777 3.176776)
		(end 2.000001 3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d1ef3319-269a-4238-aa50-fbc5a146de50")
	)
	(fp_arc
		(start 2.35 2.575)
		(mid 2.322982 2.675385)
		(end 2.249228 2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "40375513-7581-4aa5-9c33-3e32a38fe896")
	)
	(fp_poly
		(pts
			(xy 2 3) (xy -2 3) (xy -2 -3) (xy 2 -3)
		)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "f6a5aab0-76f4-407a-854d-bc1ce69b0d65")
	)
	(fp_text user "${REFERENCE}"
		(at 2.300001 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7a8b5a05-d25a-4be9-8e01-782ffa5f81b7")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(pad "" smd oval
		(at -1.825 -2.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1dd0b789-89c5-4d6d-a6c6-1ad2e7180cd8")
	)
	(pad "" smd oval
		(at -1.825 -1.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "02509601-d230-4d99-9d2e-770a97fe0bf0")
	)
	(pad "" smd oval
		(at -1.825 -1)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fe3c68a4-b08a-462f-8ad1-9fac0fe3d84a")
	)
	(pad "" smd oval
		(at -1.825 0)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e707b090-6b1b-4148-b114-bec04e50294f")
	)
	(pad "" smd oval
		(at -1.825 1)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "128f2367-7544-4840-93e8-941aac630681")
	)
	(pad "" smd oval
		(at -1.825 1.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "60215ba5-7481-4012-934b-51fe5c6f0042")
	)
	(pad "" smd oval
		(at -1.825 2.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a2e48c8c-2fa2-45f8-b514-181fcda1c7d6")
	)
	(pad "" smd oval
		(at -1.824999 -2)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1f054dbb-ab05-4e0b-b753-cd8e20c028db")
	)
	(pad "" smd oval
		(at -1.824999 -0.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e1f8b9d2-8449-498e-b0fa-15da7b8ed62c")
	)
	(pad "" smd oval
		(at -1.824999 0.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "41a93e06-51d9-4b79-b2ee-9a77cb15bc95")
	)
	(pad "" smd oval
		(at -1.824999 2)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fdf5baa0-49ec-4168-a0d7-f8e79eae9eb4")
	)
	(pad "" smd oval
		(at -0.75 -2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "02796a2b-9345-4c26-9116-3df1457b8d01")
	)
	(pad "" smd oval
		(at -0.75 2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6c793eaa-5c3c-4d31-8d67-952ade920454")
	)
	(pad "" smd roundrect
		(at -0.5 -1.725 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "db24727d-b249-4d14-a6bb-9e80c31ec77d")
	)
	(pad "" smd roundrect
		(at -0.5 -0.575 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "86d8c955-5f7d-4552-81f6-b2b69d62b0ce")
	)
	(pad "" smd roundrect
		(at -0.5 0.575 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6a106baa-7d64-4c13-ae8e-b097f02d05e9")
	)
	(pad "" smd roundrect
		(at -0.5 1.725 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5e66cfcd-42f9-40c0-bca5-d1c1cbb8ea27")
	)
	(pad "" smd oval
		(at -0.25 -2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1aa25ddc-eb07-42b9-aae8-e0ee9b9ed066")
	)
	(pad "" smd oval
		(at -0.25 2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2670984e-14db-4495-9b98-a382aec95fad")
	)
	(pad "" smd oval
		(at 0.25 -2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d020e2f3-e470-4e5b-8914-94481078e0e2")
	)
	(pad "" smd oval
		(at 0.25 2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0aaf74d5-8085-40b2-afb5-2f251d42a4a6")
	)
	(pad "" smd roundrect
		(at 0.5 -1.725 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "00eda885-d604-4855-a6a8-5039d09840d9")
	)
	(pad "" smd roundrect
		(at 0.5 -0.575 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "81e8b885-185c-49b3-b67f-97f33be194e7")
	)
	(pad "" smd roundrect
		(at 0.5 0.575 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "41df826b-1e40-491f-aeda-19b120827563")
	)
	(pad "" smd roundrect
		(at 0.5 1.725 180)
		(size 0.8 0.95)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "13c45752-26bc-4aa3-b2cc-448424434242")
	)
	(pad "" smd oval
		(at 0.75 -2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f59e628b-3d31-4886-a6be-e667da039563")
	)
	(pad "" smd oval
		(at 0.75 2.9 90)
		(size 0.55 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "57da127d-686c-4bda-968d-a8c8c9b9eb1c")
	)
	(pad "" smd oval
		(at 1.824999 -2)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "57215b9b-1fc6-48e3-b12e-5ab82e537b33")
	)
	(pad "" smd oval
		(at 1.824999 -0.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0871282d-1577-4ccf-b14b-49ef9fa799ff")
	)
	(pad "" smd oval
		(at 1.824999 0.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "73f39750-c6c0-4558-b54d-a0a420ff128e")
	)
	(pad "" smd oval
		(at 1.824999 2)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "937c4db4-2453-427c-a602-44b5f1faf163")
	)
	(pad "" smd oval
		(at 1.825 -2.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e1f76b9b-71d1-4cfe-b3bb-7665a401450d")
	)
	(pad "" smd oval
		(at 1.825 -1.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d6f86a8f-c20c-45a6-8207-4d418ef7d5ae")
	)
	(pad "" smd oval
		(at 1.825 -1)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0c58eb53-65f6-4ca1-9eff-1cb6b9aeac17")
	)
	(pad "" smd oval
		(at 1.825 0)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bc33b10f-da37-4df8-a7e8-5c8935dd7c19")
	)
	(pad "" smd oval
		(at 1.825 1)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d864dc86-9aee-409c-a54b-e05a933e5a5b")
	)
	(pad "" smd oval
		(at 1.825 1.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e88b76c4-28ec-4e62-b334-e59a48b76665")
	)
	(pad "" smd oval
		(at 1.825 2.5)
		(size 0.6 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b945d5bf-4c01-424b-9e8e-13709755f732")
	)
	(pad "1" smd roundrect
		(at -1.825 -2.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2f11bd3b-d112-4d08-874b-cf0e6b81e986")
	)
	(pad "2" smd roundrect
		(at -1.824999 -2)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e22c5230-1ddf-4874-bccd-3278ffada035")
	)
	(pad "3" smd roundrect
		(at -1.825 -1.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6077c9e2-8c31-4076-8a51-514b8dff7665")
	)
	(pad "4" smd roundrect
		(at -1.825 -1)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ba9d41c0-9b30-470b-8536-61883c6fd8ed")
	)
	(pad "5" smd roundrect
		(at -1.824999 -0.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5fba9029-3bd3-431c-929d-a490f3879751")
	)
	(pad "6" smd roundrect
		(at -1.825 0)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1760e981-a0d9-47b7-b733-58fb9bfd0324")
	)
	(pad "7" smd roundrect
		(at -1.824999 0.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4c5229a9-ab42-4114-aa58-aaa92e9589a2")
	)
	(pad "8" smd roundrect
		(at -1.825 1)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e58d9967-4d54-49a5-b1bb-b7e2a456707a")
	)
	(pad "9" smd roundrect
		(at -1.825 1.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c096aa5b-2a54-495b-8006-481349ee4f8e")
	)
	(pad "10" smd roundrect
		(at -1.824999 2)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5735d6ba-414a-4c25-942f-149e65c6cae1")
	)
	(pad "11" smd roundrect
		(at -1.825 2.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f3e3bc6c-3584-4345-ac94-b381fbf0b419")
	)
	(pad "12" smd roundrect
		(at -0.75 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d4c18ac9-e1f7-4a00-9116-78dd54fbf8c5")
	)
	(pad "13" smd roundrect
		(at -0.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bb90ad89-0b6f-4abe-9783-53f9fb2d6f4a")
	)
	(pad "14" smd roundrect
		(at 0.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1cfbb48c-a28c-48c9-9f58-36637bbc286f")
	)
	(pad "15" smd roundrect
		(at 0.75 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a182399a-e9b1-47db-a839-a8cc10ea6dac")
	)
	(pad "16" smd roundrect
		(at 1.825 2.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8f4751e1-4661-460c-aa60-89d7679bfe87")
	)
	(pad "17" smd roundrect
		(at 1.824999 2)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7ecd6568-84c4-41f3-87d8-15190f8e00e7")
	)
	(pad "18" smd roundrect
		(at 1.825 1.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a617f0a3-2fdf-428f-b6da-df3178feb327")
	)
	(pad "19" smd roundrect
		(at 1.825 1)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b06f647c-2fb9-4a27-b1c8-efe375e43938")
	)
	(pad "20" smd roundrect
		(at 1.824999 0.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "58ab94ff-3037-4de2-a96a-0d6b9fea4275")
	)
	(pad "21" smd roundrect
		(at 1.825 0)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "99912598-15f6-4e83-b337-2f8ac5933c2a")
	)
	(pad "22" smd roundrect
		(at 1.824999 -0.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "72370d44-cf19-42a8-88e8-340738bd98a0")
	)
	(pad "23" smd roundrect
		(at 1.825 -1)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "10c9932f-ea7c-486a-80c3-713053a7d0af")
	)
	(pad "24" smd roundrect
		(at 1.825 -1.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f94c61a7-2785-4a37-9df0-5c3d668ac55a")
	)
	(pad "25" smd roundrect
		(at 1.824999 -2)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "47fe5aca-a1c5-450e-a3c7-1acc0eb812f1")
	)
	(pad "26" smd roundrect
		(at 1.825 -2.5)
		(size 0.75 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b63bcd71-ab75-47dc-97b8-512c6e4010b4")
	)
	(pad "27" smd roundrect
		(at 0.75 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "71d3b8fc-1946-4a03-8183-2526d8539e08")
	)
	(pad "28" smd roundrect
		(at 0.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a2822d2d-9187-4500-9579-117d7ca11595")
	)
	(pad "29" smd roundrect
		(at -0.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1a5e9ce3-18f0-4bdd-9cdc-03e93d642469")
	)
	(pad "30" smd roundrect
		(at -0.75 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e946a85e-7cc7-4f59-93aa-699efb56b189")
	)
	(pad "31" smd roundrect
		(at 0 0)
		(size 1.8 4.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.05555555556)
		(thermal_bridge_angle 45)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8a3c7dbb-9c7e-4ce8-b1d6-8d4e4c65a05d")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WQFN-30_4x6mm_P0.5mm_EP1.85x4.5mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
