(module USB3_A_Molex_48393-001 (layer F.Cu) (tedit 5B3E1B8E)
  (descr "USB 3.0, type A, right angle (http://www.molex.com/pdm_docs/sd/483930003_sd.pdf)")
  (tags "USB 3.0 type A right angle")
  (fp_text reference J6 (at 3.5 -3.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "USB Host 1" (at 3.5 13) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.46 -2.56) (end -3.46 -1.85) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.46 -2.56) (end 10.46 -1.85) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.4 11.75) (end -3.4 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 10.4 -2.5) (end 10.4 11.75) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 3.5 5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 12.3) (end -4 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11 12.3) (end -4 12.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11 -3) (end 11 12.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 -3) (end 11 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.46 -2.56) (end 10.46 -2.56) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.46 6.8) (end 10.46 0.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.46 6.8) (end -3.46 0.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.46 11.81) (end -3.46 8.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.46 11.81) (end 10.46 8.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.46 11.81) (end 10.46 11.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.4 11.75) (end -3.4 11.75) (layer F.Fab) (width 0.1))
  (fp_line (start -3.4 -2.5) (end 10.4 -2.5) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 4.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 7 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 7.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 5.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 3.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 1.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -0.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 9.9 -0.75) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at -2.9 -0.75) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 9.9 7.75) (size 1.2 2.1) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at -2.9 7.75) (size 1.2 2.1) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
  (model ${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB3_A_Molex_48393-0003.step
    (offset (xyz 3.5 -11.75 1.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
