(module 6-UFBGA (layer F.Cu) (tedit 573A389C)
  (solder_mask_margin 0.01)
  (solder_paste_margin -0.01)
  (attr smd)
  (fp_text reference REF** (at 0 -1.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value 6-UFBGA (at 0 1.5) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -0.75 -1) (end 0.75 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.75 -1) (end 0.75 1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.75 1) (end -0.75 1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.75 1) (end -0.75 -1) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -0.85 -0.8) (end -0.85 -0.85) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.25 -0.9) (end -0.65 -0.9) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.65 -0.9) (end -0.65 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.25 0.9) (end -0.65 0.9) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.65 0.9) (end -0.65 0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.65 0.5) (end 0.65 0.85) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.65 0.85) (end 0.65 0.9) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.65 0.9) (end 0.25 0.9) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.25 -0.9) (end 0.65 -0.9) (layer F.SilkS) (width 0.125))
  (fp_line (start 0.65 -0.9) (end 0.65 -0.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -0.5 0.75) (end -0.5 -0.75) (layer F.Fab) (width 0.05))
  (fp_line (start -0.5 -0.75) (end 0.5 -0.75) (layer F.Fab) (width 0.05))
  (fp_line (start 0.5 -0.75) (end 0.5 0.75) (layer F.Fab) (width 0.05))
  (fp_line (start 0.5 0.75) (end -0.5 0.75) (layer F.Fab) (width 0.05))
  (pad A1 smd circle (at -0.25 -0.5) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at -0.25 0) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask))
  (pad C1 smd circle (at -0.25 0.5) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0.25 -0.5) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd circle (at 0.25 0) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask))
  (pad C2 smd circle (at 0.25 0.5) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask))
)
