(module TCT40-18_Ultrasonic_Transceiver_Edge_Mounted (layer F.Cu) (tedit 585E524C)
  (tags "PIEZO TRANSCEIVER ULTRASONIC")
  (solder_mask_margin -0.05)
  (fp_text reference SP1 (at 0 0.7) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value 40kHz (at 0 -0.5 180) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user + (at 6 -1.5) (layer B.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)) (justify mirror))
  )
  (fp_line (start 9 0) (end -9 0) (layer F.Fab) (width 0.05))
  (fp_line (start -5 -12) (end -9 -7.5) (layer F.Fab) (width 0.05))
  (fp_line (start -9 -7.5) (end -9 0) (layer F.Fab) (width 0.05))
  (fp_line (start -5 -12) (end 5 -12) (layer F.Fab) (width 0.05))
  (fp_line (start 5 -12) (end 9 -7.5) (layer F.Fab) (width 0.05))
  (fp_line (start 9 -7.5) (end 9 0) (layer F.Fab) (width 0.05))
  (pad 2 connect roundrect (at 5.1 3.75) (size 2.3 6.5) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (pad 1 connect roundrect (at -5.1 4.75) (size 2.3 8.5) (layers F.Cu F.Mask)(roundrect_rratio 0.25))
  (model "${KICAD7_3DMODEL_DIR}/Speaker_Transducer.3dshapes/Ultrasonic Tranceiver [Closed] [Waterproof] [Dual Use].step"
    (at (xyz 0 0.4763779527559055 0.02165354330708662))
    (scale (xyz 1 1 1))
    (rotate (xyz -180 0 0))
  )
)
