(footprint "USB3_A_Molex_484060-003" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "C6490_Carrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "USB Type A connector, stacked")
  (property "ki_keywords" "connector USB")
  (attr through_hole)
  (fp_text reference "J9" (at 0 -17.95 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9b5e10b4-dec3-4fca-9949-23f3581c90bb)
  )
  (fp_text value "USB_A_Stacked" (at 0 -2.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 263e938d-65a3-4f03-82ea-a303845bea0a)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.65 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8bee37fd-031e-42b8-8205-0d667678cea3)
  )
  (fp_line (start -6.9 -17.45) (end -6.9 -16.85)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6c877572-b31d-4b0b-a286-e50f5bb7d416))
  (fp_line (start -6.9 -17.45) (end -6.3 -17.45)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp cfa6a500-653f-4e4c-beac-47b309fe2e2f))
  (fp_line (start 6.9 -17.45) (end 6.3 -17.45)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp ac664d6c-4392-43f8-a54b-cdd10ab719f3))
  (fp_line (start 6.9 -17.45) (end 6.9 -16.85)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp bb2a33e5-1545-4b0e-8a64-d394bfba8650))
  (fp_line (start -7.4 -17.45) (end -7.4 -16.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 028cc3fb-295d-4d66-93cf-4fe6bc42c2dc))
  (fp_line (start -7.4 -13.7) (end -7.4 -10.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 546cec52-5e93-4710-999a-d3ca45e00242))
  (fp_line (start -7.4 -8.05) (end -7.4 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 573e2511-6b50-4b5c-941f-25fd8b43f285))
  (fp_line (start 6.9 -17.95) (end -6.9 -17.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 148eab7e-697a-4494-b9cc-e97c74c34cd7))
  (fp_line (start 6.9 0.5) (end -6.9 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a94b89e3-f663-4ba8-9ed4-a383d0245986))
  (fp_line (start 7.4 -17.45) (end 7.4 -16.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e259a3b7-0557-408b-997c-cc691dbc5775))
  (fp_line (start 7.4 -10.85) (end 7.4 -13.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 58375746-8268-49ce-a373-efbdd86f22a9))
  (fp_line (start 7.4 0) (end 7.4 -8.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 02ff1066-6032-4cf0-b383-7e151c2a8ac5))
  (fp_arc (start -7.4 -17.45) (mid -7.253553 -17.803553) (end -6.9 -17.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 82cfa620-3e03-4c0c-8fa9-341c7629ea0f))
  (fp_arc (start -7.4 -13.7) (mid -8.212452 -15.1) (end -7.4 -16.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3ed89e2e-585f-475c-a64e-af49448a70a1))
  (fp_arc (start -7.4 -8.05) (mid -8.212452 -9.45) (end -7.4 -10.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9d0ddfb2-ce6b-4052-a297-be7a5f4ad2b2))
  (fp_arc (start -6.9 0.5) (mid -7.253553 0.353553) (end -7.4 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4f7dc6d1-9e7c-47ff-837e-548ec1b9edd5))
  (fp_arc (start 6.9 -17.95) (mid 7.253553 -17.803553) (end 7.4 -17.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 47ccffc4-9b1a-48a0-aa93-20745ea29413))
  (fp_arc (start 7.4 -16.5) (mid 8.212452 -15.1) (end 7.4 -13.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bf2aa283-05f6-479d-83ac-2a4e811e22f1))
  (fp_arc (start 7.4 -10.85) (mid 8.212452 -9.45) (end 7.4 -8.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp da50ecb5-e1f2-49a0-b80b-966734937548))
  (fp_arc (start 7.4 0) (mid 7.253553 0.353553) (end 6.9 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp aa9a7031-61e0-4531-bb21-556f523ee06b))
  (fp_rect (start -6.9 -17.46) (end 6.9 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp 6d6a0498-929b-4a05-8e1b-2ac8718bb3c2))
  (pad "1" thru_hole circle (at -3.5 -11.44) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp b735aebe-4b22-41c6-bf82-666a2e8329b4))
  (pad "2" thru_hole circle (at -1 -11.44) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 9b4e1a72-ada1-4ab0-8508-b1b5cd1e65c1))
  (pad "3" thru_hole circle (at 1 -11.44) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 41a4b00a-a84f-4ab4-b9b6-221247752cbd))
  (pad "4" thru_hole circle (at 3.500001 -11.44) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 735817d5-2b36-45d4-a6a6-efba50d97dc7))
  (pad "5" thru_hole circle (at 4 -12.94) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 6e7ea310-a392-4f4c-88bd-3e854784d1b3))
  (pad "6" thru_hole circle (at 2 -12.94) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 937f93a4-3d3e-4216-9846-130a91a08002))
  (pad "7" thru_hole circle (at 0 -12.94) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 659d84aa-c928-46d7-b921-31a2d41bb83f))
  (pad "8" thru_hole circle (at -2 -12.94) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp db1a8300-5892-440d-9360-97ad1dc1af45))
  (pad "9" thru_hole circle (at -4 -12.94) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 96779a4e-9c73-4507-9ddd-1d30135e53e8))
  (pad "10" thru_hole circle (at -3.500001 -14.64) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp aba21f86-3bcc-4d24-81ae-e082b2e1a76b))
  (pad "11" thru_hole circle (at -1 -14.64) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 941520f1-6e17-464f-bae7-e8768da8b450))
  (pad "12" thru_hole circle (at 1 -14.64) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 560c46df-85e9-42dc-b630-3d61b34ce872))
  (pad "13" thru_hole circle (at 3.500001 -14.64) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp b4f56066-32e8-43a2-babc-f34d8352a460))
  (pad "14" thru_hole circle (at 4 -16.14) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 1f2db4ae-4478-4669-8f1d-8ba4b0aec15b))
  (pad "15" thru_hole circle (at 2 -16.14) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 0c6cc061-7fc0-4e73-a741-197d5c1919bb))
  (pad "16" thru_hole circle (at 0 -16.14) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 0d5f2901-e597-4da1-bfa7-103505560136))
  (pad "17" thru_hole circle (at -2 -16.14) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp ed1ee472-70e1-4a9e-8e03-c7f7aef112ef))
  (pad "18" thru_hole circle (at -4 -16.14) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask) (tstamp 32213b2c-8368-4ade-a90a-c6169b1cfa9e))
  (pad "MP" thru_hole circle (at -6.57 -15.12) (size 2.9 2.9) (drill 2.3) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 03a80450-a620-490f-8dd5-7ab6c4945b4d))
  (pad "MP" thru_hole circle (at -6.57 -9.44) (size 2.9 2.9) (drill 2.3) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 49583fd2-9fb1-41c8-ada0-269bb37bd8e9))
  (pad "MP" thru_hole circle (at 6.57 -15.12) (size 2.9 2.9) (drill 2.3) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 7f939a17-9e8c-41f3-85f8-588b0c63f652))
  (pad "MP" thru_hole circle (at 6.57 -9.44) (size 2.9 2.9) (drill 2.3) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp e84c853a-45b8-48f8-bf45-32e73bc365ab))
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/Molex_484060003.stp"
    (offset (xyz -6.55 0.23 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 90 0))
  )
)
