(footprint "1220_4P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.8 0 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5e511783-aa0c-4147-b7fc-a5161139ded3")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1220_4P"
		(at 0 -1.375 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "57def0b2-fb37-4b63-a527-990d06d3bb29")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(property "Footprint" ""
		(at 0 -3.925 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2e135eaa-c523-4cfd-8dfa-187e9c41cdaa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -3.925 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "29d4d963-a615-486e-8f71-3336d3c2391a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 -3.925 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "582c7367-50bc-4335-95dc-1e3654bf0936")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.2 -0.65)
		(end -1.05 0.65)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bf46cb98-a1e3-4d5c-9c6d-a5038e0fb632")
	)
	(fp_rect
		(start 1.05 -0.65)
		(end 1.2 0.65)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "b2794a49-147d-4207-80a6-8ab3913b726c")
	)
	(fp_line
		(start -1.2 0.65)
		(end -1.2 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fb7e6a69-26e3-4aa3-a13b-0503964d3b0a")
	)
	(fp_line
		(start -1.05 -0.8)
		(end -1.028453 -0.801535)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "77ee220e-1d6b-4fef-8325-6a2a093ac380")
	)
	(fp_line
		(start -1.05 0.8)
		(end -1.028453 0.801535)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "52ce41bd-da54-43a6-97ce-7b4d1d9774e6")
	)
	(fp_line
		(start -0.8 -0.95)
		(end 0.8 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a2e7e753-a326-4b5f-88b3-0b5bf92d3743")
	)
	(fp_line
		(start 0.8 0.95)
		(end -0.8 0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ef653f39-89ce-425f-bdc9-1052cb678544")
	)
	(fp_line
		(start 1.05 -0.8)
		(end 1.028453 -0.801535)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "106dd7ef-296c-45d1-8b61-18a63e8449bc")
	)
	(fp_line
		(start 1.05 0.8)
		(end 1.028453 0.801535)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "490eaf88-deba-43d6-8703-ba88869fceea")
	)
	(fp_line
		(start 1.2 -0.65)
		(end 1.2 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "37844ffd-7973-47d2-8e88-e4795af53afb")
	)
	(fp_arc
		(start -1.2 -0.65)
		(mid -1.156066 -0.756066)
		(end -1.05 -0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2aa0019d-ba65-4f4d-ac9b-6da37dc2dd18")
	)
	(fp_arc
		(start -1.05 0.8)
		(mid -1.156066 0.756066)
		(end -1.2 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f0b914db-8d33-4e57-8bc6-d503a1292eda")
	)
	(fp_arc
		(start -1.028453 -0.801535)
		(mid -0.936228 -0.909623)
		(end -0.8 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "570af6b7-99ac-4bf0-af04-d57ea6819afb")
	)
	(fp_arc
		(start -0.8 0.95)
		(mid -0.936228 0.909623)
		(end -1.028453 0.801535)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0c97280b-dc43-4fae-9825-37622f0c431e")
	)
	(fp_arc
		(start 0.8 -0.95)
		(mid 0.936228 -0.909623)
		(end 1.028453 -0.801535)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "15595cd9-e075-488b-bcda-58f6c102beaa")
	)
	(fp_arc
		(start 1.028453 0.801535)
		(mid 0.936228 0.909623)
		(end 0.8 0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "aa79df2f-426d-4530-9b8c-79747c5c6cb9")
	)
	(fp_arc
		(start 1.05 -0.8)
		(mid 1.156066 -0.756066)
		(end 1.2 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "94e80c00-a894-47bf-be5b-d0325b415352")
	)
	(fp_arc
		(start 1.2 0.65)
		(mid 1.156066 0.756066)
		(end 1.05 0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "949c3a23-18c8-42fa-a94d-e59f70a625f0")
	)
	(fp_rect
		(start -1.05 -0.65)
		(end 1.05 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "0cec837e-bada-4bda-a4a9-a6ccf120c097")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0443af7f-e5ce-4a3a-bb28-df7053bb767c")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(pad "" smd oval
		(at -0.75 -0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "2a9e07ce-5b81-47ff-bf1f-b7d900a5209d")
	)
	(pad "" smd oval
		(at -0.75 0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d0269333-1438-43ff-b515-7ece7cfa80f5")
	)
	(pad "" smd oval
		(at -0.25 -0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "1d921d9c-31df-4479-a935-9093c6f30adf")
	)
	(pad "" smd oval
		(at -0.25 0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "145f431a-a78f-490c-9870-cdc3c7024774")
	)
	(pad "" smd oval
		(at 0.25 -0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b433bafa-7d96-4c27-b503-859fdb45db5c")
	)
	(pad "" smd oval
		(at 0.25 0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7bcd4ef4-fd79-4584-962a-e1465e92b7f0")
	)
	(pad "" smd oval
		(at 0.75 -0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "76a2489e-2746-47b7-b47f-4a242fd5158a")
	)
	(pad "" smd oval
		(at 0.75 0.575)
		(size 0.25 0.3)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "5fba912d-6634-4891-954b-bc23782fe43c")
	)
	(pad "1" smd roundrect
		(at -0.75 0.575)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "34be54d9-ab83-41c1-940c-c431120c9ce6")
	)
	(pad "2" smd roundrect
		(at -0.25 0.575)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "132666df-bf9b-40e5-863f-faf3516c741f")
	)
	(pad "3" smd roundrect
		(at 0.25 0.575)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "9d1450fc-5d1e-415c-8697-813bdc1a5af5")
	)
	(pad "4" smd roundrect
		(at 0.75 0.575)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "d80c7c57-9f39-4c32-9692-6aa4ff5ce4f5")
	)
	(pad "5" smd roundrect
		(at 0.75 -0.575 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "84d9e244-f270-4bbe-aac9-2b4265193ea3")
	)
	(pad "6" smd roundrect
		(at 0.25 -0.575 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "1068c850-f421-4d5e-ae51-1d822fa0e2bf")
	)
	(pad "7" smd roundrect
		(at -0.25 -0.575 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "ca07b728-c233-480b-b250-2b902402c7d1")
	)
	(pad "8" smd roundrect
		(at -0.75 -0.575 180)
		(size 0.3 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "167dae1f-c52c-47d1-a357-615c80937760")
	)
)
