(footprint "Arc_Ri0.9_0.1-0.1_0.2_5DP_45deg" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (zone_connect 0)
  (attr board_only exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -8.075 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c79dc91-7d87-4312-a8b9-19715fd00ffa)
  )
  (fp_text value "Arc_Ri0.9_0.1-0.1_0.2_5DP_45deg" (at 0 -6.575 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5beec144-4cc1-474b-a704-c5bb50798690)
  )
  (fp_text user "${REFERENCE}" (at 0 -5.075 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 329fd6c7-7418-4566-b934-69bde1aafa29)
  )
  (pad "2" smd custom (at -0.95 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.072314 -0.363549) (end 0.278249 -0.671751) (width 0.1))
    ) (tstamp aa408ecd-bba1-4102-9d21-bf669b763fdc))
  (pad "2" smd custom (at -0.671751 -0.671751) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.278249 0.671751) (mid -0.205934 0.308202) (end 0 0) (width 0.1))
    ) (tstamp 88ba24f6-f951-49ea-a3b8-95d3b82d44b5))
  (pad "3" smd custom (at -1.15 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.087539 -0.440086) (end 0.336827 -0.813173) (width 0.1))
    ) (tstamp f53fbdce-af9d-43fd-b9c3-648bfc302f41))
  (pad "3" smd custom (at -0.813173 -0.813173) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.336827 0.813173) (mid -0.249289 0.373087) (end -0.000001 -0.000001) (width 0.1))
    ) (tstamp 2502ec05-edb1-4def-842f-42f749dab410))
  (pad "4" smd custom (at -1.45 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.110375 -0.554891) (end 0.424695 -1.025305) (width 0.1))
    ) (tstamp 609b5c07-0466-43b9-ad5f-131d75a5e7d9))
  (pad "4" smd custom (at -1.025305 -1.025305) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.424695 1.025305) (mid -0.31432 0.470414) (end 0 0) (width 0.1))
    ) (tstamp 6a4f0046-3eff-4d0c-9139-94b87b1c59a8))
  (pad "5" smd custom (at -1.65 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.125599 -0.631428) (end 0.483274 -1.166726) (width 0.1))
    ) (tstamp 32e8f1c6-9502-4582-a5cb-53db52d71d05))
  (pad "5" smd custom (at -1.166726 -1.166726) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.483274 1.166726) (mid -0.357674 0.535299) (end 0.000001 0.000001) (width 0.1))
    ) (tstamp 6a9abc1b-5413-47c6-b253-795dbf164a85))
  (pad "6" smd custom (at -1.95 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.148435 -0.746233) (end 0.571142 -1.378858) (width 0.1))
    ) (tstamp 853f39e3-d44d-4aef-ab9b-aa2175c5aa29))
  (pad "6" smd custom (at -1.378858 -1.378858) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.571142 1.378858) (mid -0.422707 0.632626) (end 0 0) (width 0.1))
    ) (tstamp a9f844da-120b-4784-beb3-b004f17fee72))
  (pad "7" smd custom (at -2.15 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.163659 -0.822769) (end 0.62972 -1.52028) (width 0.1))
    ) (tstamp 97c7c4ef-261d-403d-bc30-90f6388751d1))
  (pad "7" smd custom (at -1.52028 -1.52028) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.62972 1.52028) (mid -0.466061 0.697511) (end 0 0) (width 0.1))
    ) (tstamp e989b206-3973-4685-804a-7d8d5b471e80))
  (pad "8" smd custom (at -2.45 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.186495 -0.937574) (end 0.717588 -1.732412) (width 0.1))
    ) (tstamp 7a2c0b2c-8fca-4167-ba18-951f7c3b6034))
  (pad "8" smd custom (at -1.732412 -1.732412) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.717588 1.732412) (mid -0.531093 0.794837) (end 0 0) (width 0.1))
    ) (tstamp d163d3eb-8a25-4e9d-bc26-978daa56055c))
  (pad "9" smd custom (at -2.65 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.201719 -1.014111) (end 0.776167 -1.873833) (width 0.1))
    ) (tstamp a7c319b6-e4b9-473d-ae01-f2052433c6da))
  (pad "9" smd custom (at -1.873833 -1.873833) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.776167 1.873833) (mid -0.574449 0.859721) (end -0.000001 -0.000001) (width 0.1))
    ) (tstamp 68c682e8-b2ae-463f-bd18-302ad5bca4da))
  (pad "10" smd custom (at -2.95 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.224555 -1.128916) (end 0.864035 -2.085965) (width 0.1))
    ) (tstamp 0adc12f7-34b9-4c0a-9f45-8e5baf90c99f))
  (pad "10" smd custom (at -2.085965 -2.085965) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.864035 2.085965) (mid -0.63948 0.957049) (end 0 0) (width 0.1))
    ) (tstamp dd6fa34f-4e52-41fa-8d09-0be3d531be8b))
  (pad "11" smd custom (at -3.15 0) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.239779 -1.205453) (end 0.922614 -2.227386) (width 0.1))
    ) (tstamp 537100b4-4ab2-4ad1-9c89-144b15f78809))
  (pad "11" smd custom (at -2.227386 -2.227386) (size 0.1 0.1) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -0.922614 2.227386) (mid -0.682833 1.021934) (end 0.000001 0.000001) (width 0.1))
    ) (tstamp 01732a19-3aeb-49f8-be68-519c9b87a57f))
)
