(footprint "3225_C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "1206 3216")
	(property "Reference" "C54"
		(at 1.75 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "de06779f-2b7d-4211-b70d-6bc976ac6795")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "10uF"
		(at 1.825 0.675 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "630be4a8-1796-444f-a880-40fed08f71fb")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
			(justify left)
		)
	)
	(property "Footprint" "3225_C"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3abf70fb-0626-488c-8d08-b64cd3fde798")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "808a570c-5280-4f0b-8938-48b4bb943047")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "64d9a79f-1c96-4d5f-8c9d-c83c44a6f00a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C5156756"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "061f5538-783d-4db7-a9c8-ec8a4a7db015")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "PSA"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2cbfcceb-5ae9-40fa-b8ed-f3203339cc19")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "FS32X106K101EGG"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b07fbab8-dbcf-4a7d-8a0e-2381e6454159")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Device" "SPICE"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cb959c66-003b-477a-ad3f-98016f3f0c90")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Params" "type=\"C\" model=\"100n\" lib=\"\""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "87e7ea42-446c-44b8-ab35-aa2354aa7235")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Pins" "1=1 2=2"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "59e2186c-c933-4d62-929e-8282481f805a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.05)
	(solder_paste_margin -0.03)
	(attr smd)
	(fp_poly
		(pts
			(xy 0.95 -1.275) (xy -0.95 -1.275) (xy -0.95 -1.425) (xy 0.95 -1.425)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "93d27896-14f2-491f-9d2b-78f6d0324bac")
	)
	(fp_poly
		(pts
			(xy 0.95 1.425) (xy -0.95 1.425) (xy -0.95 1.275) (xy 0.95 1.275)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "adf41f2c-ebd5-4e4c-93b5-97e214a07519")
	)
	(fp_line
		(start -1.9 -1.1)
		(end -1.9 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3d3a8fdf-3eb5-49ef-ba99-0087cc5af1a3")
	)
	(fp_line
		(start -1.6 -1.4)
		(end 1.6 -1.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "45a7563e-6c07-4194-a37d-bb5c511382b7")
	)
	(fp_line
		(start 1.6 1.4)
		(end -1.6 1.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f3551d9a-b0b0-4830-90ba-2613c312566c")
	)
	(fp_line
		(start 1.9 1.1)
		(end 1.9 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ac6d8162-ad9c-455e-b9c6-5218643f738d")
	)
	(fp_arc
		(start -1.9 -1.1)
		(mid -1.812132 -1.312132)
		(end -1.6 -1.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "21debccd-cc7d-4a44-8b53-96cbbeeb4835")
	)
	(fp_arc
		(start -1.6 1.4)
		(mid -1.812132 1.312132)
		(end -1.9 1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1d3f308d-5a46-479a-ab84-2a3a14cbf277")
	)
	(fp_arc
		(start 1.6 -1.4)
		(mid 1.812132 -1.312132)
		(end 1.9 -1.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "14def761-2afb-4418-94cb-e82ddafa8967")
	)
	(fp_arc
		(start 1.9 1.1)
		(mid 1.812132 1.312132)
		(end 1.6 1.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "689bce39-ed84-4486-826c-976364b5c7b2")
	)
	(fp_rect
		(start -1.6 -1.25)
		(end 1.6 1.25)
		(stroke
			(width 0.025)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "80a295c0-1522-419c-a179-09988c0e1568")
	)
	(pad "" smd oval
		(at -1.425 -0.65)
		(size 0.6 1.1)
		(layers "F.Paste")
		(uuid "571b059b-8df8-4f08-bab5-7ed64da5dca9")
	)
	(pad "" smd oval
		(at -1.425 0.65)
		(size 0.6 1.1)
		(layers "F.Paste")
		(uuid "6aa98fb1-9918-48c1-a89b-36bee8677e5b")
	)
	(pad "" smd oval
		(at 1.425 -0.65)
		(size 0.6 1.1)
		(layers "F.Paste")
		(uuid "cf2b3beb-f90d-48ef-830e-120d4ed084e6")
	)
	(pad "" smd oval
		(at 1.425 0.65)
		(size 0.6 1.1)
		(layers "F.Paste")
		(uuid "d5fae7ea-09c7-475d-b327-0f8564b720e5")
	)
	(pad "1" smd roundrect
		(at -1.425 0)
		(size 0.65 2.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "7a18fcdd-680f-4f73-b987-bbbb6ab69d04")
	)
	(pad "2" smd roundrect
		(at 1.425 0)
		(size 0.65 2.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.05)
		(chamfer top_left bottom_left)
		(uuid "123139d3-3f42-456a-94e9-22f965e2906e")
	)
	(model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/Capacitor_SMD_3225.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
