(footprint "Crystal_4-SMD_2x1.6mm" (version 20220417) (generator pcbnew)
  (layer "F.Cu")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "C255898")
  (property "MFG" "Seiko Epson")
  (property "MPN" "Q22FA12800101")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "ESC_Dual_10A.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference "Y1" (at 0 -1.4) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp c6f1aaa9-ead5-445b-a6fa-58b212e086a9)
  )
  (fp_text value "40MHz <=10ppm" (at 0 1.3) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp c91f0009-0aca-4d55-927c-5f4cfb2bf485)
  )
  (fp_rect (start -1.375 -0.5) (end -1.225 -0.85)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6f5c8a8b-faf1-4dbc-acd6-702496bf73f4))
  (fp_rect (start -1.05 -1.175) (end -0.7 -1.025)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f8f48918-e1a5-416a-a511-27e12ebf7b5f))
  (fp_rect (start 0.7 -1.175) (end 1.05 -1.025)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 50e72c16-61ab-4cb9-81b2-8318bac84073))
  (fp_rect (start 1.05 1.175) (end 0.7 1.025)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 71a4a869-16fa-4626-8791-7479c3e22ac8))
  (fp_rect (start 1.375 -0.85) (end 1.225 -0.5)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e539330a-614e-485d-a120-030abcc0eb90))
  (fp_rect (start 1.375 0.5) (end 1.225 0.85)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f29be0bd-1508-413b-baae-914ed4993b19))
  (fp_arc (start -1.3 -0.85) (mid -1.226777 -1.026776) (end -1.05 -1.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 5df6fe51-1d3d-46f0-a89b-3f51dff5558d))
  (fp_arc (start 1.05 -1.1) (mid 1.226776 -1.026777) (end 1.3 -0.85)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 85844aab-d8f2-493a-828a-99fb3996a519))
  (fp_arc (start 1.3 0.85) (mid 1.226777 1.026776) (end 1.05 1.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp fe090093-6e1e-4bae-b407-57afc160d341))
  (fp_poly
    (pts
      (xy -1.225 1.025)
      (xy -0.7 1.025)
      (xy -0.7 1.175)
      (xy -1.375 1.175)
      (xy -1.375 0.5)
      (xy -1.225 0.5)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 94a98841-33b6-40e4-b188-ad26328cf85d))
  (fp_line (start -1.3 0.85) (end -1.3 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6c9ff10b-a26d-47ad-bf8a-e7cd915ed7db))
  (fp_line (start -1.05 -1.1) (end 1.05 -1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0579039a-e435-44ce-91ac-20408854c052))
  (fp_line (start 1.05 1.1) (end -1.05 1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d7780a77-3e53-4d5e-b5d9-b4ffc19fc159))
  (fp_line (start 1.3 -0.85) (end 1.3 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6c14481b-f345-48e8-abb7-1953e4c13c16))
  (fp_arc (start -1.3 -0.85) (mid -1.226777 -1.026777) (end -1.05 -1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d82c62d7-5116-47d4-9599-9241ec968896))
  (fp_arc (start -1.05 1.1) (mid -1.226777 1.026777) (end -1.3 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ccaefffa-f090-43cb-8964-6472a908cb35))
  (fp_arc (start 1.05 -1.1) (mid 1.226777 -1.026777) (end 1.3 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d2b20c59-0dbd-4d75-b0ee-9717b9427c32))
  (fp_arc (start 1.3 0.85) (mid 1.226777 1.026777) (end 1.05 1.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3c0d08bd-db7c-4070-b3ad-76a6ece2def1))
  (fp_line (start -1 -0.8) (end 1 -0.8)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 840229e8-e789-408c-aa4a-7d4bc7e24cdf))
  (fp_line (start -1 0.8) (end -1 -0.8)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 101e65b7-e410-4a9d-9d38-c6fd96f99861))
  (fp_line (start 1 -0.8) (end 1 0.8)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp d6c1fa8b-d945-483c-9812-a105578c518c))
  (fp_line (start 1 0.8) (end -1 0.8)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp b4bafbd7-c983-4e99-a666-c80e23336e68))
  (pad "1" smd roundrect (at -0.7 0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6690f061-1669-403f-92f2-4b0116f03ea1))
  (pad "2" smd roundrect (at 0.7 0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3899c755-72bf-4848-a665-fdfbec4cbec4))
  (pad "3" smd roundrect (at 0.7 -0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ad00bae2-66c7-415f-a660-f19b17cdddb6))
  (pad "4" smd roundrect (at -0.7 -0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp edabd404-098a-4202-b388-474f8512b539))
  (model "${KICAD7_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_4P_2016.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
