(module "Hirose_FH12-10S-0.5SH_1x10-1MP_P0.50mm_Horizontal" (layer F.Cu) (tedit 5CC30090)
  (descr "Molex FH12, FFC/FPC connector, FH12-10S-0.5SH, 10 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
  (tags "connector Hirose  top entry")
  (attr smd)
  (fp_text reference "J1" (at 0 -3.7 180) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "FPC" (at 0 5.6 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "%R" (at 0 3.7 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.55 -3) (end -5.55 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.55 4.9) (end 5.55 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.55 4.9) (end 5.55 4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.55 -3) (end -5.55 4.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.25 -0.492893) (end -1.75 -1.2) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 -1.2) (end -2.25 -0.492893) (layer F.Fab) (width 0.1))
  (fp_line (start -2.66 -1.3) (end -2.66 -2.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.15 4.5) (end 4.15 2.76) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.15 4.5) (end 4.15 4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.15 2.76) (end -4.15 4.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.15 -1.3) (end 4.15 0.04) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.66 -1.3) (end 4.15 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -4.15 -1.3) (end -4.15 0.04) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.66 -1.3) (end -4.15 -1.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.95 4.4) (end 0 4.4) (layer F.Fab) (width 0.1))
  (fp_line (start 3.95 3.7) (end 3.95 4.4) (layer F.Fab) (width 0.1))
  (fp_line (start 3.45 3.7) (end 3.95 3.7) (layer F.Fab) (width 0.1))
  (fp_line (start 3.45 3.4) (end 3.45 3.7) (layer F.Fab) (width 0.1))
  (fp_line (start 4.05 3.4) (end 3.45 3.4) (layer F.Fab) (width 0.1))
  (fp_line (start 4.05 -1.2) (end 4.05 3.4) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.2) (end 4.05 -1.2) (layer F.Fab) (width 0.1))
  (fp_line (start -3.95 4.4) (end 0 4.4) (layer F.Fab) (width 0.1))
  (fp_line (start -3.95 3.7) (end -3.95 4.4) (layer F.Fab) (width 0.1))
  (fp_line (start -3.45 3.7) (end -3.95 3.7) (layer F.Fab) (width 0.1))
  (fp_line (start -3.45 3.4) (end -3.45 3.7) (layer F.Fab) (width 0.1))
  (fp_line (start -4.05 3.4) (end -3.45 3.4) (layer F.Fab) (width 0.1))
  (fp_line (start -4.05 -1.2) (end -4.05 3.4) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.2) (end -4.05 -1.2) (layer F.Fab) (width 0.1))
  (pad "10" smd rect (at 2.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 1.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.75 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -2.25 -1.85) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "MP" smd rect (at -4.15 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "MP" smd rect (at 4.15 1.4) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KICAD7_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-10S-0.5SH_1x10-1MP_P0.50mm_Horizontal.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
